VERSION 6							// V1 expects map checkpoint rectangles
// V2 and above expect map checkpoint points
// V3 and above expect splash file stuff at the end
// V4 and above expect two sets of PIX and MAT and ped substitution entry
-256.540,-2.555,-102.5						// Position of centre of start of grid
160									// Direction that grid faces in
// Direction that grid faces in
// Laps, checkpoints etc
120,60,20							// Initial timer count for each skill level
4									// # laps
10000,5000,3000						// Race completed bonus (all laps raced) for each skill level
75000,50000,30000					// Race completed bonus (all peds killed) for each skill level
20000,10000,5000					// Race completed bonus (all oppos wasted) for each skill level
// Width and height of map checkpoint rectangles
9,18
11,26
4									// # checkpoints
// Checkpoint #1
20,10,5								// Timer increment for each skill level (ped mode)
60,30,10							// Timer increment for each skill level (pedless mode)
1									// # quads for this checkpoint
-288.923,-100,-66.164						// Point #0
-288.923,100,-66.164						// Point #1
-289.032,100,-69.796						// Point #2
-289.032,-100,-69.796					// Point #3
58,116
59,142
// Checkpoint #2
20,10,5								// Timer increment for each skill level (ped mode)
60,30,10							// Timer increment for each skill level (pedless mode)
1									// # quads for this checkpoint
-284.960,-100,28.585						// Point #0
-284.960,100,28.585						// Point #1
-284.317,100,31.694						// Point #2
-284.317,-100,31.694					// Point #3
65,130
132,317
// Checkpoint #3
20,10,5								// Timer increment for each skill level (ped mode)
60,30,10							// Timer increment for each skill level (pedless mode)
1									// # quads for this checkpoint
-267.698,-100,-15.744						// Point #0
-267.698,100,-15.744						// Point #1
-264.604,100,-16.553						// Point #2
-264.604,-100,-16.553					// Point #3
81,162
96,230
// Checkpoint #4
20,10,5								// Timer increment for each skill level (ped mode)
60,30,10							// Timer increment for each skill level (pedless mode)
1									// # quads for this checkpoint
-148.876,-100,-137.803						// Point #0
-148.876,100,-137.803						// Point #1
-148.825,100,-141.435						// Point #2
-148.825,-100,-141.435					// Point #3
165,330
6,14
6									// # pixelmap files to load
NYSKY1.PIX
C3SKY2.PIX
COASTA1.pix
NCHORIZN.PIX
DRKSCRN.PIX
FOGSCRN.PIX
6									// # pixelmap files to load (low memory)
NYSKY1.PIX
C3SKY2.PIX
COA8TA3.pix
NCHORIZN.PIX
DRKSCRN.PIX
FOGSCRN.PIX
2									// # shade table files to load
COASTA1.TAB
identity.tab
9									// # material files to load
YWW.MAT
WATTY.MAT
NYSKY1.MAT
C3SKY2.MAT
COASTA1.MAT
DARKSKY.MAT
DRKSCRN.MAT
FOGSCRN.MAT
SKIDMARK.MAT
9
YWW.MAT									// # material files to load (low memory)
WATTY.MAT
NYSKY1.MAT
C3SKY2.MAT
COA8TA3.MAT
DARKSKY.MAT
DRKSCRN.MAT
FOGSCRN.MAT
SKIDMARK.MAT
1									// # model files to load
COASTA1.dat
1									// # model files to load
COSTA81.dat
COASTA1.ACT							// Track actor
COSTA81.ACT
COASTAX.ACT							// Additional actor
// HORIZON STUFF
NCHORIZN.PIX						// Name of sky texture pixelmap (or "none")
4									// Horizontal repetitions of sky texture
66									// Vertical size of sky texture (degrees)
128									// Position of horizon (pixels below top)
dark								// Depth cue mode ("none", "dark" or "fog")
8,0									// Degree of fog/darkness
// DEFAULT ENGINE NOISE
0
// SPECIAL EFFECTS VOLUMES
11				// # special effects volumes
DEFAULT WATER
0.2									// gravity multiplier
50									// viscosity multiplier
0									// Car damage per millisecond
0.002								// Pedestrian damage per millisecond
0									// camera effect index
1									// Sky colour
WATTY.MAT								// Windscreen material to use
5100								// Sound ID of entry noise
5100								// Sound ID of exit noise
2									// Engine noise index
0									// material index
NEW IMPROVED!
8.702, -0.080, -1.941
0.031, 3.583, -0.007
12.018, 0.007, 53.882
-267.444, -15.562, -32.364
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index
NEW IMPROVED!
5.124, 0.000, 5.680
0.000, 1.000, 0.000
-40.065, 0.000, 22.294
-254.058, -16.907, -75.250
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index
NEW IMPROVED!
0.022, 0.000, 1.728
0.000, 2.074, 0.000
-3.583, 0.000, 0.046
-212.111, -17.667, -89.661
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index
NEW IMPROVED!
-0.416, 0.000, -1.677
0.003, 1.728, -0.001
1.398, -0.002, -0.347
-193.901, -17.667, -91.913
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index
NEW IMPROVED!
-0.940, 0.000, -1.848
0.000, 1.000, 0.000
1.283, 0.000, -0.653
-181.791, -16.747, -97.209
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index
NEW IMPROVED!
1.262, 0.000, 1.645
0.000, 1.728, 0.000
-1.143, 0.000, 0.876
-171.178, -16.427, -105.123
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index
NEW IMPROVED!
1.210, 0.000, 1.684
0.014, 1.440, -0.010
-0.975, 0.014, 0.700
-165.651, -14.506, -108.596
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index
NEW IMPROVED!
-0.462, 0.000, -2.022
0.000, 1.000, 0.000
1.170, 0.000, -0.267
-133.374, -12.981, -118.326
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index
NEW IMPROVED!
-0.472, 0.000, -2.019
0.013, 1.000, -0.003
1.402, -0.020, -0.328
-93.955, -12.942, -127.460
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index
NEW IMPROVED!
-0.444, 0.000, -1.831
0.000, 1.000, 0.000
9.804, 0.000, -2.379
-72.472, -13.061, -132.528
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index
// REFLECTIVE WINDSCREEN SPECIFICATIONS
NYSKY1.MAT							// Material to use for default screens
DRKSCRN.MAT							// Material to use for default screens during darkness
FOGSCRN.MAT							// Material to use for default screens during fog
0									// # areas with different screens
// MAP DETAILS
CSTAMAP1.PIX						// Map pixelmap name
0.744,		0,			0			// World->map transformation matrix
0,			0,			0
0,			0.744, 		0
282.4,		114.9,		0
// ****** START OF FUNK AND GROOVE STUFF ******
START OF FUNK
!!WATER.MAT
constant
slither
harmonic
0.20,0
5,5
no fucking lighting
no animation you cunt
NEXT FUNK
CHECK.MAT
constant
roll
continuous
0.2,0
no fucking lighting
no animation you cunt
END OF FUNK
START OF GROOVE
&YAC0001.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.07,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
2							// max angle of rock
NEXT GROOVE
&YAC0002.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.07,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
2							// max angle of rock
NEXT GROOVE
&YAC0003.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.23							// Cycles per second
0,.08,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
8							// max angle of rock
NEXT GROOVE
&YAC0004.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.23							// Cycles per second
0,.08,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.14							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
7							// max angle of rock
NEXT GROOVE
&YAC0005.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.07,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
8							// max angle of rock
NEXT GROOVE
&YAC0006.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.23							// Cycles per second
0,.05,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
7							// max angle of rock
NEXT GROOVE
&YAC0007.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.16							// Cycles per second
0,.08,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
8							// max angle of rock
NEXT GROOVE
&YAC0008.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.15							// Cycles per second
0,.05,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
8							// max angle of rock
NEXT GROOVE
&YAC0009.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.08,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
7							// max angle of rock
NEXT GROOVE
&YAC0010.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.15							// Cycles per second
0,.08,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.17							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
8							// max angle of rock
NEXT GROOVE
&YAC0011.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0012.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0013.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.15							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0014.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.16							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.16							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0015.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.17							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0016.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.15							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.17							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0017.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.15							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0018.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.14							// Cycles per second
0,.9,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.14							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0018.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.14							// Cycles per second
0,.1,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.14							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0019.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.14							// Cycles per second
0,.12,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.14							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
11							// max angle of rock
NEXT GROOVE
&YAC0020.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.18							// Cycles per second
0,.12,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0020.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0021.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.17							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0022.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0023.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.17							// Cycles per second
0,.06,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0024.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.18							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0025.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.16							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0026.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.15,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
11							// max angle of rock
NEXT GROOVE
&YAC0027.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0028.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.16							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0029.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.16							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0030.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.18							// Cycles per second
0,.06,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0031.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.18							// Cycles per second
0,.05,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock
END OF GROOVE
// ****** START OF PEDESTRIAN STUFF ******
29				// Ped subs table index
512				// Number of pedestrians
// M*^n{b"XlSWw<joo
1				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-270.099,-2.552,-90.191
point
-270.283,-2.552,-90.262
point
-270.642,-2.552,-90.240
point
-270.750,-2.552,-90.830
point
-270.106,-2.552,-94.390
reverse
// M*^n{b"XlSWw<joo
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-269.542,-2.552,-93.851
point
-269.226,-2.552,-94.602
point
-268.805,-2.552,-97.226
point
-269.183,-2.552,-97.602
reverse
// M*^n{b"XlSWw<joo
3				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-269.651,-2.552,-96.212
point
-270.692,-2.552,-96.146
point
-271.176,-2.552,-93.826
point
-270.885,-2.550,-90.653
point
-269.978,-2.552,-89.883
reverse
// M*^n{b"XlSWw<joo
3				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-283.484,-2.539,-69.888
point
-283.344,-2.539,-70.484
point
-282.090,-2.547,-71.521
point
-281.665,-2.552,-75.949
reverse
// M*^n{b"XlSWw<joo
1				// Ref num
7				// Number of instructions
2				// Initial instruction
point
-273.553,-2.552,-71.184
point
-274.416,-2.552,-70.664
point
-276.012,-2.552,-69.593
point
-282.558,-2.541,-69.943
point
-283.671,-2.538,-70.196
point
-285.278,-2.538,-71.625
reverse
// M*^n{b"XlSWw<joo
5				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-267.804,-2.552,-75.968
point
-269.345,-2.552,-74.693
point
-270.275,-2.552,-73.536
point
-272.513,-2.552,-72.074
point
-272.953,-2.552,-71.371
reverse
// M*^n{b"XlSWw<joo
8				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-283.972,-2.540,-69.747
point
-285.354,-2.540,-66.865
point
-287.150,-2.531,-66.831
point
-287.955,-2.543,-68.800
point
-288.656,-2.544,-69.908
reverse
// M*^n{b"XlSWw<joo
1				// Ref num
7				// Number of instructions
2				// Initial instruction
point
-313.628,-11.971,-26.568
point
-313.384,-11.971,-24.033
point
-312.579,-11.971,-22.773
point
-312.587,-11.971,-21.316
point
-312.863,-11.971,-19.602
point
-312.938,-11.971,-18.287
reverse
// M*^n{b"XlSWw<joo
1				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-273.343,-15.627,25.364
point
-272.440,-15.626,22.412
point
-271.392,-15.627,22.991
point
-270.066,-15.627,23.992
point
-266.453,-15.627,23.741
reverse
// Pedestrian number 10
8				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-256.908,-15.622,24.732
point
-258.387,-15.620,25.909
point
-261.283,-15.627,26.499
point
-261.930,-15.627,25.909
point
-262.724,-15.627,24.242
reverse
// Pedestrian number 11
1				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-259.411,-15.657,19.155
point
-259.250,-15.651,21.396
point
-258.661,-15.627,22.942
point
-257.584,-15.627,22.954
point
-254.533,-15.627,25.546
reverse
// Pedestrian number 12
5				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-261.806,-15.627,23.787
point
-260.932,-15.627,24.492
point
-260.637,-15.631,25.771
point
-261.612,-15.627,26.439
point
-263.339,-15.627,27.132
reverse
// Pedestrian number 13
8				// Ref num
7				// Number of instructions
3				// Initial instruction
point
-259.648,-15.627,26.691
point
-260.517,-15.634,24.927
point
-260.682,-15.634,24.331
point
-259.094,-15.652,22.352
point
-259.229,-15.655,20.294
point
-263.211,-15.657,16.713
reverse
// Pedestrian number 14
3				// Ref num
5				// Number of instructions
4				// Initial instruction
point
-258.070,-15.645,23.910
point
-258.197,-15.634,25.400
point
-258.889,-15.628,26.320
point
-260.490,-15.627,27.624
reverse
// Pedestrian number 15
8				// Ref num
7				// Number of instructions
3				// Initial instruction
point
-260.701,-15.599,47.238
point
-259.289,-15.606,46.406
point
-257.955,-15.616,46.773
point
-256.369,-15.627,46.363
point
-254.084,-15.627,46.205
point
-253.703,-15.666,46.495
reverse
// Pedestrian number 16
8				// Ref num
5				// Number of instructions
5				// Initial instruction
point
-253.063,-15.627,45.480
point
-254.008,-15.627,44.645
point
-254.846,-15.627,44.699
point
-257.222,-15.627,43.235
reverse
// Pedestrian number 17
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-255.654,-15.627,46.287
point
-253.574,-15.627,43.281
point
-246.306,-15.632,43.864
reverse
// Pedestrian number 18
3				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-254.375,-15.627,42.839
point
-252.268,-15.627,44.870
point
-251.614,-15.627,45.550
reverse
// Pedestrian number 19
1				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-277.839,-15.626,46.964
point
-278.242,-15.626,48.289
point
-278.639,-15.626,48.814
point
-279.885,-15.622,51.172
point
-280.454,-15.622,51.603
reverse
// Pedestrian number 20
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-279.755,-15.627,47.717
point
-280.472,-15.627,48.585
point
-282.667,-15.627,49.018
reverse
// Pedestrian number 21
1				// Ref num
4				// Number of instructions
3				// Initial instruction
point
-273.077,-15.595,49.765
point
-277.955,-15.626,48.609
point
-278.568,-15.627,47.785
reverse
// Pedestrian number 22
1				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-261.550,-15.627,24.535
point
-259.447,-15.657,20.859
point
-259.724,-15.657,19.231
point
-260.028,-15.657,17.513
point
-261.038,-15.657,13.342
point
-264.753,-15.657,11.104
// Pedestrian number 23
8				// Ref num
9				// Number of instructions
5				// Initial instruction
point
-266.082,-2.553,-107.261
point
-264.257,-2.552,-109.714
point
-261.583,-2.552,-110.630
point
-254.872,-2.555,-114.747
point
-251.657,-2.553,-118.503
point
-250.448,-2.553,-118.685
point
-248.889,-2.553,-119.259
point
-247.098,-2.551,-119.696
reverse
// Pedestrian number 24
1				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-246.091,-2.560,-122.113
point
-245.615,-2.566,-123.061
point
-245.679,-2.573,-124.489
point
-246.242,-2.578,-125.649
point
-247.503,-2.581,-126.887
reverse
// Pedestrian number 25
1				// Ref num
8				// Number of instructions
5				// Initial instruction
point
-266.410,998.041,-108.087
point
-265.176,997.648,-109.687
point
-264.586,-2.552,-109.784
point
-263.782,-2.552,-111.050
point
-262.242,-2.552,-111.443
point
-261.234,-2.552,-111.416
point
-256.954,-2.552,-113.230
reverse
// Pedestrian number 26
5				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-263.329,-2.552,-106.691
point
-264.653,-2.552,-106.833
point
-265.447,-2.552,-106.684
point
-265.923,-2.552,-106.075
point
-266.551,-2.552,-106.131
reverse
// Pedestrian number 27
3				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-267.692,-2.552,-101.129
point
-265.751,-2.552,-104.003
point
-265.192,-2.552,-104.223
point
-264.814,-2.552,-104.245
point
-264.475,-2.552,-103.716
reverse
// Pedestrian number 28
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-288.495,-2.544,-69.925
point
-287.502,-2.542,-70.409
point
-285.983,-2.538,-71.673
point
-282.791,-2.544,-71.385
reverse
// Pedestrian number 29
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-294.143,-2.791,-66.783
point
-295.765,-2.911,-66.707
point
-298.187,996.963,-66.782
point
-301.141,997.563,-65.627
reverse
// Pedestrian number 30
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-309.792,-4.048,-66.420
point
-310.831,-4.048,-65.068
point
-308.452,-4.048,-62.614
point
-307.596,996.743,-61.857
reverse
// Pedestrian number 31
3				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-287.373,-8.005,-48.814
point
-286.748,-8.005,-48.424
point
-285.763,-8.005,-47.190
point
-284.516,-8.005,-44.545
reverse
// Pedestrian number 32
3				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-288.702,-8.004,-37.911
point
-289.819,-8.005,-36.912
point
-291.675,-8.005,-35.896
point
-293.116,-8.132,-35.655
reverse
// Pedestrian number 33
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-316.138,-11.971,-26.853
point
-315.844,-11.971,-24.747
point
-315.337,-11.971,-23.907
point
-314.748,-11.971,-20.162
reverse
// Pedestrian number 34
8				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-280.964,-13.137,0.325
point
-279.881,-14.067,6.853
point
-279.061,-14.283,8.372
point
-278.439,-14.469,9.711
reverse
// Pedestrian number 35
1				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-281.143,-13.637,4.305
point
-279.878,-13.759,4.398
point
-277.683,-14.024,5.166
point
-277.137,-14.175,6.063
point
-276.633,-14.232,6.556
reverse
// Pedestrian number 36
1				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-279.125,-13.614,2.765
point
-278.599,-13.753,3.557
point
-278.165,-13.871,4.247
point
-278.714,-14.200,7.385
point
-279.385,-14.220,7.974
reverse
// Pedestrian number 37
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-276.482,-14.300,7.130
point
-276.218,-14.378,7.742
point
-276.264,-14.536,9.064
point
-276.652,-15.143,13.609
reverse
// Pedestrian number 38
3				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-275.002,-15.619,19.806
point
-274.496,-15.618,19.663
point
-268.392,-15.627,22.206
reverse
// Pedestrian number 39
3				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-272.264,-15.588,17.210
point
-275.058,-15.622,20.682
point
-274.902,-15.625,21.666
point
-278.184,-15.627,30.167
reverse
// Pedestrian number 40
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-277.417,-15.627,29.835
point
-279.133,-15.627,30.441
point
-280.492,-15.627,30.747
reverse
// Pedestrian number 41
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-282.975,-15.627,28.137
point
-283.564,-15.627,28.642
point
-284.591,-15.627,31.486
reverse
// Pedestrian number 42
5				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-280.448,-15.627,34.628
point
-282.453,-15.627,32.370
point
-284.006,-15.627,31.417
point
-284.666,-15.627,28.681
reverse
// Pedestrian number 43
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-281.126,-15.627,31.345
point
-281.238,-15.627,31.978
point
-283.168,-15.627,35.341
reverse
// Pedestrian number 44
8				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-285.095,-15.627,28.814
point
-286.271,-15.627,29.022
point
-287.036,-15.627,29.290
point
-287.996,-15.627,29.336
reverse
// Pedestrian number 45
3				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-289.209,-15.627,30.392
point
-288.316,-15.627,34.406
point
-288.427,-15.627,35.933
point
-284.900,-15.627,51.411
reverse
// Pedestrian number 46
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-288.387,-15.627,48.459
point
-287.352,-15.627,49.820
point
-276.078,-15.617,50.597
reverse
// Pedestrian number 47
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-59.975,-14.067,-138.803
point
-60.505,-14.035,-138.556
point
-61.242,-13.918,-136.903
point
-62.150,-13.901,-136.874
reverse
// Pedestrian number 48
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-62.775,-13.901,-136.216
point
-60.787,-13.911,-134.451
point
-57.955,-14.207,-135.354
reverse
// Pedestrian number 49
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-56.289,-14.327,-137.813
point
-58.024,-14.202,-137.874
point
-60.730,-13.909,-134.134
point
-61.790,-13.901,-132.943
reverse
// Pedestrian number 50
1				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-65.611,-13.901,-132.644
point
-64.250,-13.901,-133.070
point
-62.385,-13.901,-136.494
point
-62.564,-13.916,-137.158
point
-66.376,-13.713,-136.860
reverse
// Pedestrian number 51
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-69.041,-13.532,-139.787
point
-67.521,-13.635,-139.776
point
-62.387,-13.925,-137.424
point
-62.022,-13.949,-137.335
reverse
// Pedestrian number 52
13				// Ref num
7				// Number of instructions
2				// Initial instruction
point
-75.245,-13.901,-133.507
point
-73.024,-13.906,-133.906
point
-71.821,-13.901,-133.901
point
-70.394,-13.901,-134.566
point
-61.138,-13.915,-136.228
point
-58.166,-14.192,-136.758
reverse
// Pedestrian number 53
13				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-97.076,-13.901,-125.689
point
-99.376,-13.901,-124.838
point
-106.368,-13.901,-123.246
point
-109.898,-13.901,-125.363
point
-111.093,-13.901,-125.195
reverse
// Pedestrian number 54
13				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-112.755,-13.901,-121.814
point
-111.085,-13.901,-122.181
point
-109.744,-13.901,-122.466
point
-106.911,-13.901,-125.959
reverse
// Pedestrian number 55
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-175.042,-17.667,-100.004
point
-179.117,-17.667,-100.649
point
-181.253,-17.667,-99.148
point
-181.745,-17.667,-95.709
reverse
// Pedestrian number 56
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-179.293,-17.667,-97.039
point
-176.732,-17.667,-98.838
point
-175.654,-17.667,-99.802
point
-174.310,-17.667,-100.624
reverse
// Pedestrian number 57
13				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-170.557,-16.453,-106.909
point
-174.975,-17.426,-103.830
point
-176.094,-17.667,-102.846
point
-177.133,-17.667,-101.969
point
-178.138,-17.667,-101.345
reverse
// Pedestrian number 58
13				// Ref num
7				// Number of instructions
4				// Initial instruction
point
-203.787,-17.667,-91.459
point
-207.159,-17.667,-88.463
point
-209.744,-17.667,-88.486
point
-211.957,-17.667,-88.351
point
-213.212,-17.667,-88.337
point
-214.288,-17.667,-91.441
reverse
// Pedestrian number 59
3				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-214.358,-17.667,-88.482
point
-212.875,-17.667,-88.949
point
-210.600,-17.667,-88.317
point
-208.806,-17.667,-89.242
point
-207.125,-17.667,-91.163
reverse
// Pedestrian number 60
5				// Ref num
5				// Number of instructions
4				// Initial instruction
point
-244.356,-17.667,-77.863
point
-245.862,-17.667,-77.901
point
-248.054,-17.667,-78.765
point
-252.012,-17.667,-78.072
reverse
// Pedestrian number 61
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-250.827,-17.667,-75.431
point
-250.251,-17.667,-75.935
point
-247.056,-17.667,-80.030
reverse
// Pedestrian number 62
13				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-261.819,-17.667,-73.050
point
-260.784,-17.667,-73.119
point
-259.624,-17.667,-71.430
point
-257.921,-17.667,-71.828
point
-254.443,-17.667,-72.824
reverse
// Pedestrian number 63
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-261.064,-17.667,-70.032
point
-260.448,-17.667,-70.677
point
-259.825,-17.667,-74.013
reverse
// Pedestrian number 64
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-265.666,-15.657,7.363
point
-265.003,-15.657,8.315
point
-262.073,-15.657,10.449
reverse
// Pedestrian number 65
13				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-264.227,-15.657,12.830
point
-264.807,-15.657,10.788
point
-262.833,-15.657,7.393
point
-263.603,-15.657,2.374
reverse
// Pedestrian number 66
14				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-266.605,-15.657,0.758
point
-266.129,-15.657,3.554
point
-264.564,-15.657,9.533
point
-263.000,-15.657,11.069
point
-261.491,-15.657,11.978
reverse
// Pedestrian number 67
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-262.447,-15.657,8.891
point
-262.242,-15.657,9.640
point
-262.573,-15.657,10.781
point
-263.959,-15.657,13.668
reverse
// Pedestrian number 68
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-259.638,-15.657,18.489
point
-261.348,-15.657,12.474
point
-264.456,-15.657,10.126
point
-264.992,-15.657,9.778
reverse
// Pedestrian number 69
13				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-263.145,-15.657,5.505
point
-263.338,-15.657,6.703
point
-262.725,-15.657,8.248
point
-261.501,-15.657,11.636
reverse
// Pedestrian number 70
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-257.690,-15.632,24.742
point
-257.953,-15.627,26.535
point
-257.212,-15.627,28.230
point
-259.492,-15.627,31.657
reverse
// Pedestrian number 71
13				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-256.166,-15.627,33.743
point
-256.624,-15.627,33.108
point
-257.324,-15.627,29.408
point
-257.476,-15.627,25.473
point
-255.290,-15.627,22.277
reverse
// Pedestrian number 72
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-257.372,-15.627,22.881
point
-256.107,-15.627,22.939
point
-250.981,-15.627,24.575
reverse
// Pedestrian number 73
14				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-252.187,-15.627,28.373
point
-252.575,-15.627,27.283
point
-251.458,-15.627,23.884
reverse
// Pedestrian number 74
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-261.113,-15.628,25.080
point
-261.443,-15.630,22.852
point
-262.229,-15.657,20.201
point
-259.412,-15.657,19.456
reverse
// Pedestrian number 75
17				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-245.970,-15.627,39.348
point
-249.793,-15.627,39.942
point
-250.178,-15.626,41.146
reverse
// Pedestrian number 76
8				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-251.313,-15.627,42.251
point
-250.581,-15.627,41.983
point
-249.967,-15.627,41.610
point
-246.073,-15.632,42.138
point
-245.368,-15.627,39.850
reverse
// Pedestrian number 77
12				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-244.877,-15.635,43.594
point
-247.082,-15.631,43.610
point
-248.305,-15.628,42.389
point
-251.868,-15.627,23.453
reverse
// Pedestrian number 78
8				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-254.490,-15.627,41.847
point
-257.747,-15.627,39.460
point
-258.167,-15.627,37.313
point
-258.321,-15.654,23.099
reverse
// Pedestrian number 79
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-261.943,-15.627,25.544
point
-263.120,-15.627,26.106
point
-267.710,-15.627,26.051
reverse
// Pedestrian number 80
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-268.220,-15.627,25.990
point
-268.947,-15.627,25.494
point
-269.505,-15.627,20.972
reverse
// Pedestrian number 81
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-280.302,-15.627,27.697
point
-281.003,-15.627,27.992
point
-282.525,-15.627,38.145
reverse
// Pedestrian number 82
3				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-279.237,-15.627,47.436
point
-279.147,-15.627,46.697
point
-280.958,-15.627,32.440
reverse
// Pedestrian number 83
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-283.974,-15.627,31.730
point
-283.756,-15.627,32.563
point
-283.491,-15.627,33.863
point
-278.829,-15.627,47.333
reverse
// Pedestrian number 84
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-278.011,-15.627,46.284
point
-278.348,-15.627,45.160
point
-281.207,-15.627,44.482
reverse
// Pedestrian number 85
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-278.334,-15.708,52.126
point
-276.456,-15.917,53.527
point
-276.025,-16.174,56.155
point
-277.909,-16.318,58.276
reverse
// Pedestrian number 86
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-272.600,-18.908,82.287
point
-269.042,-18.912,86.156
point
-269.557,-18.914,89.312
point
-270.740,-18.916,92.449
reverse
// Pedestrian number 87
13				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-267.411,-18.915,94.181
point
-269.126,-18.915,92.989
point
-270.514,-18.916,93.653
point
-274.046,-18.916,92.297
point
-290.575,-18.915,96.467
reverse
// Pedestrian number 88
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-290.535,-18.915,97.563
point
-274.153,-18.915,94.451
point
-268.527,-18.915,89.919
reverse
// Pedestrian number 89
13				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-267.077,-18.915,92.468
point
-267.702,-18.915,91.826
point
-268.247,-18.915,90.436
point
-270.731,-18.914,89.718
reverse
// Pedestrian number 90
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-266.066,-18.913,106.289
point
-269.661,-18.914,94.163
point
-267.923,-18.915,90.522
reverse
// Pedestrian number 91
17				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-246.888,-18.915,85.598
point
-246.557,-18.915,88.305
point
-246.116,-18.915,89.756
reverse
// Pedestrian number 92
5				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-242.658,-18.915,100.699
point
-242.385,-18.915,96.290
point
-244.021,-18.915,89.483
point
-244.344,-18.914,85.812
reverse
// Pedestrian number 93
17				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-224.432,-18.915,81.168
point
-225.555,-18.916,82.652
point
-228.229,-18.916,84.140
reverse
// Pedestrian number 94
12				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-224.098,-18.916,82.961
point
-224.899,-18.916,82.519
point
-225.427,-18.916,82.805
point
-232.529,-18.916,82.657
reverse
// Pedestrian number 95
13				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-224.172,-18.916,82.005
point
-243.623,-18.915,87.028
point
-244.561,-18.915,86.304
point
-245.521,-18.913,82.788
point
-248.219,-18.911,80.794
reverse
// Pedestrian number 96
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-246.298,-18.910,78.252
point
-246.004,-18.911,79.590
point
-247.313,-18.916,88.406
reverse
// Pedestrian number 97
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-245.505,-18.915,92.686
point
-245.012,-18.915,94.175
point
-244.047,-18.915,100.455
reverse
// Pedestrian number 98
8				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-221.401,-18.916,95.766
point
-222.908,-18.916,95.051
point
-227.663,-18.916,95.340
point
-230.000,-18.916,96.978
point
-244.157,-18.915,98.220
reverse
// Pedestrian number 99
3				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-238.820,-18.915,99.952
point
-241.360,-18.915,98.651
point
-244.445,-18.915,96.720
point
-244.997,-18.915,95.096
reverse
// Pedestrian number 100
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-242.120,-18.915,97.469
point
-244.093,-18.915,98.859
point
-245.851,-18.916,101.360
point
-287.253,-18.914,110.686
reverse
// Pedestrian number 101
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-245.032,-18.916,101.345
point
-244.585,-18.915,98.971
point
-242.312,-18.914,96.801
reverse
// Pedestrian number 102
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-251.461,-18.916,100.610
reverse
// Pedestrian number 103
129				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-253.398,-15.627,45.697
reverse
// Pedestrian number 104
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-257.272,-15.627,42.491
reverse
// Pedestrian number 105
129				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-256.284,-15.627,33.307
reverse
// Pedestrian number 106
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-254.620,-15.627,22.531
reverse
// Pedestrian number 107
130				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-250.575,-15.627,41.531
reverse
// Pedestrian number 108
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-254.042,-17.667,-73.114
reverse
// Pedestrian number 109
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-252.533,-17.667,-77.667
reverse
// Pedestrian number 110
129				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-226.823,-17.667,-91.019
reverse
// Pedestrian number 111
129				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-27.743,-15.561,-44.497
reverse
// Pedestrian number 112
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-26.788,-15.561,-45.238
reverse
// Pedestrian number 113
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-25.847,-15.561,-45.968
reverse
// Pedestrian number 114
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-82.993,-13.028,-48.234
reverse
// Pedestrian number 115
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-129.713,-18.645,-45.533
reverse
// Pedestrian number 116
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-127.573,-18.655,-46.141
reverse
// Pedestrian number 117
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-125.686,-18.634,-45.420
reverse
// Pedestrian number 118
129				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-138.923,-18.725,-58.154
reverse
// Pedestrian number 119
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-141.695,-18.737,-59.375
reverse
// Pedestrian number 120
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-145.946,-18.665,-48.496
reverse
// Pedestrian number 121
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-145.198,-18.670,-46.779
reverse
// Pedestrian number 122
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-139.581,-16.166,-39.660
reverse
// Pedestrian number 123
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-137.255,-14.010,-30.646
reverse
// Pedestrian number 124
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-136.103,-13.938,-30.522
reverse
// Pedestrian number 125
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-132.813,-9.082,-50.595
reverse
// Pedestrian number 126
130				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-133.365,-9.082,-50.436
reverse
// Pedestrian number 127
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-264.404,-2.552,-104.048
reverse
// Pedestrian number 128
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-264.253,-2.552,-104.536
reverse
// Pedestrian number 129
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-268.549,-2.552,-98.537
reverse
// Pedestrian number 130
1				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-154.797,-8.795,-37.416
point
-155.758,-9.008,-39.093
point
-155.682,-9.077,-40.053
point
-146.436,-9.077,-42.540
reverse
// Pedestrian number 131
3				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-146.536,-9.077,-45.589
point
-148.877,-9.077,-44.903
point
-149.937,-9.077,-44.138
point
-150.793,-9.077,-41.614
reverse
// Pedestrian number 132
13				// Ref num
4				// Number of instructions
1				// Initial instruction
point
-144.951,-8.822,-45.084
point
-146.179,-9.077,-44.767
point
-147.609,-9.077,-45.393
reverse
// Pedestrian number 133
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-135.266,-8.919,-46.250
point
-134.767,-9.089,-46.979
point
-132.236,-9.084,-46.497
point
-121.404,-9.078,-49.433
reverse
// Pedestrian number 134
13				// Ref num
7				// Number of instructions
4				// Initial instruction
point
-132.587,-9.081,-50.555
point
-132.074,-8.967,-50.100
point
-131.552,-9.077,-49.757
point
-128.024,-9.077,-49.940
point
-124.245,-9.078,-48.738
point
-122.163,-9.338,-46.182
reverse
// Pedestrian number 135
14				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-125.546,-9.934,-40.050
point
-123.504,-9.673,-41.952
point
-124.452,-9.143,-47.802
point
-121.549,-9.096,-49.138
reverse
// Pedestrian number 136
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-127.186,-9.077,-48.003
point
-128.893,-9.077,-48.697
point
-134.625,-9.081,-48.200
point
-136.083,-8.818,-47.566
reverse
// Pedestrian number 137
8				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-134.164,-9.096,-46.011
point
-133.139,-9.080,-47.536
point
-131.164,-9.077,-48.998
point
-125.868,-9.078,-51.521
reverse
// Pedestrian number 138
14				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-23.454,-15.561,-49.659
point
-25.541,-15.561,-45.735
point
-28.159,-15.561,-43.634
point
-37.209,-15.561,-46.669
reverse
// Pedestrian number 139
3				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-31.746,-15.561,-44.197
point
-29.092,-15.561,-44.828
point
-23.428,-15.561,-47.823
reverse
// Pedestrian number 140
1				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-23.237,-15.561,-51.567
point
-24.452,-15.560,-51.263
point
-27.403,-15.561,-49.276
point
-29.418,-15.561,-46.721
point
-28.054,-15.561,-43.551
reverse
// Pedestrian number 141
5				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-24.211,-15.561,-46.619
point
-25.772,-15.561,-47.198
point
-26.246,-15.561,-49.840
point
-24.516,-15.561,-50.401
reverse
// Pedestrian number 142
1				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-274.111,-15.600,47.219
point
-273.015,-15.599,47.834
point
-271.303,-15.599,49.503
point
-269.993,-15.599,49.251
reverse
// Pedestrian number 143
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-275.307,-15.612,50.411
point
-274.073,-15.604,50.194
point
-267.833,-15.599,48.906
reverse
// Pedestrian number 144
3				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-268.077,-15.599,45.919
point
-270.539,-15.599,46.626
point
-271.840,-15.599,47.562
point
-274.421,-15.604,47.757
point
-276.369,-15.619,47.718
reverse
// Pedestrian number 145
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-266.716,-15.599,48.695
point
-263.974,-15.599,47.846
point
-261.122,-15.599,44.348
reverse
// Pedestrian number 146
29				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-273.751,-15.599,47.079
point
-271.455,-15.599,47.075
point
-270.293,-15.599,48.141
point
-267.297,-15.599,47.593
point
-264.722,-15.599,48.203
reverse
// Pedestrian number 147
3				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-262.696,-15.599,44.762
point
-257.263,-15.627,43.881
point
-253.610,-15.627,42.867
reverse
// Pedestrian number 148
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-282.000,-15.625,51.855
point
-283.612,-15.627,50.231
point
-285.220,-15.627,48.205
point
-290.883,-15.627,37.644
reverse
// Pedestrian number 149
1				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-269.156,-15.599,46.071
point
-265.497,-15.599,45.847
point
-263.858,-15.599,45.177
point
-256.357,-15.627,46.578
reverse
// Pedestrian number 150
3				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-256.138,-15.649,46.817
point
-255.963,-15.783,47.965
point
-255.393,-15.998,49.747
point
-252.229,-16.263,52.093
reverse
// Pedestrian number 151
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-240.193,-14.789,40.689
point
-237.698,-14.359,39.170
point
-236.859,-13.820,34.927
reverse
// Pedestrian number 152
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-244.855,-15.619,40.005
point
-244.408,-15.513,39.803
point
-242.112,-14.883,38.503
point
-239.603,-14.414,36.895
reverse
// Pedestrian number 153
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-235.848,-13.988,37.950
point
-232.211,-13.012,35.192
point
-229.563,-12.513,32.817
reverse
// Pedestrian number 154
1				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-230.596,-12.208,29.479
point
-228.883,-11.868,28.658
point
-225.417,-11.308,27.739
point
-223.554,-11.037,25.996
reverse
// Pedestrian number 155
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-215.914,-9.122,11.075
point
-215.358,-9.078,10.006
point
-215.350,-9.078,9.436
point
-217.107,-9.078,5.180
reverse
// Pedestrian number 156
14				// Ref num
7				// Number of instructions
2				// Initial instruction
point
-216.712,-9.078,9.149
point
-215.622,-9.078,5.559
point
-215.178,-9.078,3.462
point
-215.443,-9.078,2.543
point
-214.628,-9.078,1.286
point
-215.556,-9.078,-1.573
reverse
// Pedestrian number 157
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-220.365,-9.446,14.723
point
-219.623,-9.293,12.993
point
-219.052,-9.222,12.157
point
-218.892,-9.163,10.928
reverse
// Pedestrian number 158
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-217.898,-9.078,9.322
point
-217.505,-9.078,6.830
point
-216.861,-9.078,4.397
point
-216.390,-9.078,1.667
reverse
// Pedestrian number 159
13				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-215.150,-9.078,8.818
point
-215.007,-9.078,7.951
point
-214.495,-9.078,7.136
point
-214.368,-9.078,6.415
point
-213.805,-9.078,4.554
reverse
// Pedestrian number 160
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-218.536,-9.103,9.741
point
-217.609,-9.078,7.851
point
-216.308,-9.078,5.552
point
-216.740,-9.078,4.223
reverse
// Pedestrian number 161
8				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-206.193,-8.044,-8.222
point
-205.343,-7.665,-8.595
point
-204.631,-7.562,-8.476
point
-204.049,-7.140,-8.757
point
-203.320,-6.748,-8.939
reverse
// Pedestrian number 162
5				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-204.299,-7.663,-8.118
point
-203.816,-7.387,-8.357
point
-203.330,-7.145,-8.425
point
-202.910,-7.249,-8.038
point
-201.931,-7.245,-7.347
reverse
// Pedestrian number 163
1				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-206.737,-8.135,-8.164
point
-205.643,-7.958,-7.995
point
-203.866,-7.672,-7.739
point
-203.208,-7.562,-7.607
point
-201.235,-7.058,-6.994
reverse
// Pedestrian number 164
8				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-197.295,-5.839,-1.871
point
-194.701,-5.332,-0.287
point
-193.775,-5.328,0.480
point
-193.307,-5.328,0.595
point
-192.870,-5.328,1.078
reverse
// Pedestrian number 165
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-188.596,-5.325,0.546
point
-187.717,-5.327,1.713
point
-186.019,-5.427,3.168
point
-184.273,-5.428,3.262
reverse
// Pedestrian number 166
8				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-190.226,-5.270,3.747
point
-190.782,-4.797,3.803
point
-191.406,-4.735,3.288
point
-191.612,-5.327,2.311
reverse
// Pedestrian number 167
1				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-188.997,-5.362,4.469
point
-186.993,-5.407,4.074
point
-186.415,-5.427,3.910
point
-183.962,-5.428,3.497
point
-181.176,-5.421,3.071
reverse
// Pedestrian number 168
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-184.261,-5.428,6.319
point
-185.743,-5.428,5.912
point
-187.377,-5.421,5.567
reverse
// Pedestrian number 169
8				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-185.924,-5.427,2.800
point
-185.395,-5.428,4.132
point
-183.905,-5.428,5.366
point
-181.818,-5.423,6.072
point
-179.124,-5.425,5.360
reverse
// Pedestrian number 170
1				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-174.318,-5.442,-0.457
point
-174.188,-5.446,-0.956
point
-174.107,-5.498,-4.044
point
-175.052,-5.851,-7.078
reverse
// Pedestrian number 171
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-177.642,-5.713,-5.465
point
-177.881,-5.840,-6.393
point
-178.966,-6.300,-8.660
reverse
// Pedestrian number 172
8				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-177.301,-5.594,-4.567
point
-176.429,-5.872,-6.928
point
-176.337,-6.116,-8.542
point
-176.405,-6.376,-10.122
reverse
// Pedestrian number 173
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-180.871,-8.504,-21.449
point
-180.128,-8.799,-25.143
point
-179.896,-8.854,-25.811
point
-178.526,-9.042,-27.987
reverse
// Pedestrian number 174
29				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-178.132,-9.078,-28.560
point
-175.555,-9.078,-29.629
point
-173.209,-9.078,-30.268
point
-170.662,-9.078,-32.453
reverse
// Pedestrian number 175
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-170.287,-9.078,-32.745
point
-169.972,-9.078,-34.458
point
-168.781,-9.078,-35.482
point
-164.568,-9.078,-36.741
reverse
// Pedestrian number 176
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-166.497,-9.078,-39.067
point
-164.967,-9.078,-39.826
point
-163.602,-9.078,-40.411
point
-158.816,-9.078,-39.141
reverse
// Pedestrian number 177
3				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-93.141,-10.699,-46.567
point
-90.667,-11.282,-46.195
point
-88.743,-11.763,-45.902
point
-86.841,-12.221,-46.212
point
-83.983,-12.934,-45.274
reverse
// Pedestrian number 178
8				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-79.598,-13.281,-47.890
point
-76.790,-13.067,-46.072
point
-76.641,-13.072,-45.976
point
-74.152,-13.200,-44.051
reverse
// Pedestrian number 179
5				// Ref num
7				// Number of instructions
6				// Initial instruction
point
-63.452,-15.005,-45.914
point
-59.726,-15.561,-45.200
point
-56.465,-15.561,-44.719
point
-55.502,-15.561,-44.850
point
-54.827,-15.561,-44.541
point
-54.827,-15.561,-44.541
reverse
// Pedestrian number 180
8				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-50.902,-15.561,-41.216
point
-48.469,-15.561,-41.442
point
-46.856,-15.561,-41.425
point
-44.620,-15.561,-41.528
reverse
// Pedestrian number 181
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-51.913,-15.561,-41.452
point
-54.157,-15.561,-41.768
point
-56.903,-15.561,-42.016
reverse
// Pedestrian number 182
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-58.522,-15.561,-45.328
point
-57.228,-15.561,-44.640
point
-53.892,-15.561,-44.153
point
-52.330,-15.561,-44.363
reverse
// Pedestrian number 183
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-60.416,-15.465,-45.270
point
-61.681,-15.280,-45.454
point
-64.002,-14.903,-45.808
point
-65.282,-14.658,-46.072
reverse
// Pedestrian number 184
29				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-33.680,-15.561,-48.367
point
-29.151,-15.561,-47.717
point
-23.574,-15.561,-49.720
reverse
// Pedestrian number 185
29				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-28.036,-15.561,-52.219
point
-29.046,-15.561,-51.305
point
-30.114,-15.561,-50.544
point
-31.076,-15.561,-50.004
reverse
// Pedestrian number 186
29				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-27.654,-15.561,-47.388
point
-28.060,-15.561,-45.289
point
-28.902,-15.561,-43.269
reverse
// Pedestrian number 187
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-18.146,-15.561,-61.368
point
-16.833,-15.561,-64.439
point
-15.727,-15.547,-68.677
reverse
// Pedestrian number 188
3				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-18.611,-15.561,-60.084
point
-18.493,-15.561,-61.007
point
-15.497,-15.515,-70.280
reverse
// Pedestrian number 189
1				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-18.380,-15.539,-69.591
point
-18.681,-15.518,-68.230
point
-19.311,-15.562,-66.305
point
-19.974,-15.561,-64.060
point
-20.299,-15.561,-63.560
reverse
// Pedestrian number 190
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-18.388,-15.521,-70.426
point
-17.230,-15.495,-71.950
point
-15.033,-15.495,-73.694
point
-15.044,-15.495,-75.395
reverse
// Pedestrian number 191
3				// Ref num
7				// Number of instructions
2				// Initial instruction
point
-14.173,-14.288,-115.232
point
-12.458,-14.162,-117.244
point
-11.531,-14.109,-118.322
point
-11.367,-14.010,-120.702
point
-11.328,-14.015,-120.886
point
-11.564,-14.210,-121.700
reverse
// Pedestrian number 192
13				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-11.554,-14.326,-114.336
point
-12.126,-14.253,-115.646
point
-13.671,-14.128,-118.100
point
-13.738,-14.154,-118.514
point
-14.235,-14.340,-120.942
reverse
// Pedestrian number 193
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-14.431,-14.362,-114.006
point
-14.209,-14.161,-117.414
point
-14.245,-14.245,-119.162
reverse
// Pedestrian number 194
29				// Ref num
8				// Number of instructions
3				// Initial instruction
point
-14.019,-14.830,-124.818
point
-13.509,-15.444,-127.889
point
-11.893,-15.631,-131.178
point
-12.495,-15.631,-131.975
point
-12.980,-15.631,-133.519
point
-14.167,-15.631,-134.831
point
-15.643,-15.631,-136.253
reverse
// Pedestrian number 195
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-15.503,-15.631,-132.103
point
-11.967,-15.594,-130.452
point
-11.549,-15.528,-129.287
reverse
// Pedestrian number 196
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-11.584,-15.483,-128.504
point
-11.700,-15.576,-130.153
point
-12.536,-15.631,-132.708
reverse
// Pedestrian number 197
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-17.200,-15.631,-133.775
point
-19.067,-15.629,-134.677
point
-21.511,-15.585,-137.659
reverse
// Pedestrian number 198
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-30.188,-15.562,-137.478
point
-33.425,-15.562,-137.417
point
-38.063,-15.555,-137.825
reverse
// Pedestrian number 199
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-37.519,-15.562,-134.767
point
-41.532,-15.437,-137.507
point
-42.737,-15.345,-137.747
reverse
// Pedestrian number 2
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-52.536,-14.601,-134.892
point
-54.431,-14.461,-134.946
point
-58.037,-14.201,-137.413
point
-59.248,-14.119,-138.455
reverse
// Pedestrian number 2
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-61.996,-13.901,-136.617
point
-61.204,-13.916,-136.545
point
-58.575,-14.148,-134.805
reverse
// Pedestrian number 2
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-61.172,-13.901,-133.827
point
-62.598,-13.901,-135.916
point
-64.597,-13.901,-135.750
reverse
// Pedestrian number 2
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-78.384,-13.021,-140.037
point
-82.901,-12.812,-137.255
point
-86.013,-12.670,-137.159
reverse
// Pedestrian number 2
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-89.978,-12.488,-137.208
point
-92.780,-12.357,-137.667
point
-98.558,-12.093,-137.310
reverse
// Pedestrian number 2
3				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-164.897,-9.029,-141.292
point
-168.279,-8.767,-140.352
point
-169.487,-8.668,-139.876
point
-171.154,-8.530,-139.352
reverse
// Pedestrian number 2
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-167.121,-8.860,-137.879
point
-168.014,-8.788,-137.578
point
-169.239,-8.690,-136.999
reverse
// Pedestrian number 2
1				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-174.566,-8.230,-136.773
point
-175.795,-8.117,-135.328
point
-176.785,-8.026,-134.361
point
-177.411,-7.967,-133.357
point
-178.164,-7.895,-132.071
reverse
// Pedestrian number 2
5				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-175.648,-8.132,-130.543
point
-176.472,-8.055,-129.160
point
-176.824,-8.022,-127.301
point
-177.463,-7.962,-123.708
reverse
// Pedestrian number 2
8				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-179.881,-7.728,-118.107
point
-182.502,-7.468,-115.060
point
-183.518,-7.358,-113.824
point
-183.699,-6.793,-112.925
reverse
// Pedestrian number 2~
29				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-188.039,-6.870,-114.709
point
-190.069,-6.641,-113.765
point
-191.402,-6.484,-113.622
point
-193.168,-6.279,-113.335
reverse
// Pedestrian number 2~
8				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-199.733,-5.456,-110.360
point
-199.119,-5.069,-109.733
point
-198.364,-4.985,-109.470
point
-196.892,-5.166,-109.341
point
-195.723,-5.966,-109.956
reverse
// Pedestrian number 2~
5				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-201.463,-5.228,-110.850
point
-199.630,-5.469,-110.555
point
-198.233,-5.649,-110.207
point
-196.739,-5.838,-110.503
point
-196.414,-5.879,-110.232
reverse
// Pedestrian number 2~
5				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-195.802,-5.956,-113.173
point
-198.498,-5.616,-113.263
point
-200.035,-5.416,-113.415
point
-201.760,-5.191,-113.866
point
-203.892,-4.901,-114.969
reverse
// Pedestrian number 2~
1				// Ref num
7				// Number of instructions
4				// Initial instruction
point
-203.170,-4.999,-111.287
point
-204.126,-4.867,-112.350
point
-205.630,-4.660,-112.790
point
-206.713,-4.508,-113.248
point
-208.206,-4.297,-114.389
point
-209.045,-4.174,-114.956
reverse
// Pedestrian number 2~
1				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-208.288,-4.285,-118.682
point
-209.033,-4.169,-119.281
point
-209.737,-4.050,-120.532
point
-210.064,-3.995,-121.123
point
-210.623,-3.889,-123.040
reverse
// Pedestrian number 2~
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-214.008,-3.465,-124.467
point
-213.698,-3.484,-122.753
point
-213.185,-3.555,-121.988
point
-213.022,-3.582,-121.021
reverse
// Pedestrian number 2~
29				// Ref num
9				// Number of instructions
5				// Initial instruction
point
-210.892,-3.885,-123.878
point
-212.017,-3.744,-126.687
point
-211.713,-3.774,-127.972
point
-212.090,-3.720,-128.330
point
-212.071,-3.717,-128.962
point
-211.915,-3.737,-130.228
point
-212.109,-3.715,-131.658
point
-212.803,-3.621,-134.944
reverse
// Pedestrian number 2~
13				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-214.005,-3.464,-137.958
point
-214.545,-3.400,-139.444
point
-215.451,-3.325,-141.219
point
-215.887,-3.274,-141.797
point
-216.623,-3.208,-143.140
reverse
// Pedestrian number 2~
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-220.808,-2.963,-142.879
point
-220.916,-2.427,-142.407
point
-220.608,-2.227,-141.860
reverse
// Pedestrian number 2}
13				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-217.864,-3.159,-139.088
point
-217.953,-2.966,-138.941
point
-217.926,-2.739,-138.378
point
-217.757,-2.537,-137.481
reverse
// Pedestrian number 2}
8				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-218.020,-3.154,-139.890
point
-218.784,-3.133,-141.209
point
-219.332,-3.118,-142.147
point
-220.767,-3.087,-143.468
point
-222.002,-3.059,-144.447
reverse
// Pedestrian number 2}
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-221.117,-3.071,-147.339
point
-221.770,-3.063,-147.743
point
-223.903,-3.018,-148.851
point
-226.591,-2.962,-150.613
reverse
// Pedestrian number 2}
5				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-230.681,-2.863,-152.229
point
-229.772,-2.879,-151.728
point
-228.778,-2.899,-151.598
point
-227.521,-2.465,-151.751
reverse
// Pedestrian number 2}
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-231.665,-2.845,-152.564
point
-233.043,-2.856,-152.639
point
-234.060,-2.806,-152.317
reverse
// Pedestrian number 2}
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-235.199,-2.734,-148.686
point
-235.321,-2.719,-148.387
point
-235.541,-2.713,-147.544
reverse
// Pedestrian number 2}
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-237.421,-2.731,-150.636
point
-237.956,-2.717,-150.020
point
-239.148,-2.700,-147.260
reverse
// Pedestrian number 2}
3				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-239.394,-2.695,-146.363
point
-238.514,-2.706,-148.017
point
-238.122,-2.711,-148.836
point
-237.989,-2.714,-149.518
reverse
// Pedestrian number 2}
12				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-234.193,-2.780,-149.292
point
-234.523,-2.762,-149.024
point
-235.733,-2.741,-147.978
point
-236.225,-2.705,-146.210
reverse
// Pedestrian number 2}
3				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-233.743,-2.796,-149.489
point
-233.018,-2.828,-149.670
point
-231.980,-2.846,-149.519
reverse
// Pedestrian number 2|
1				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-237.762,-2.682,-142.292
point
-238.988,-2.665,-139.503
point
-240.981,-2.654,-138.347
point
-243.640,-2.635,-136.066
point
-244.050,-2.630,-135.209
reverse
// Pedestrian number 2|
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-242.575,-2.650,-138.481
point
-241.791,-2.662,-139.986
point
-240.409,-2.682,-144.017
reverse
// Pedestrian number 2|
5				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-235.696,-2.711,-147.185
point
-236.687,-2.708,-146.130
point
-236.887,-2.693,-144.744
point
-237.605,-2.685,-142.872
reverse
// Pedestrian number 2|
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-237.685,-2.683,-142.634
point
-238.632,-2.674,-141.185
point
-240.579,-2.640,-135.349
reverse
// Pedestrian number 2|
29				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-241.063,-2.634,-134.364
point
-241.720,-2.626,-133.080
point
-242.694,-2.611,-130.614
point
-243.371,-2.601,-128.796
reverse
// Pedestrian number 2|
29				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-246.510,-2.595,-129.308
point
-246.510,-2.595,-129.308
point
-241.963,-2.618,-131.668
point
-241.075,-1.949,-132.197
reverse
// Pedestrian number 2|
17				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-246.760,-2.592,-128.747
point
-247.714,-2.576,-125.882
point
-248.654,-2.565,-124.034
reverse
// Pedestrian number 2|
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-250.127,-2.552,-120.536
point
-250.502,-2.552,-119.241
point
-251.703,-2.552,-118.814
reverse
// Pedestrian number 2|
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-252.670,-2.555,-115.362
point
-255.373,-2.552,-114.200
point
-256.381,-2.552,-113.722
reverse
// Pedestrian number 2|
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-257.974,-2.552,-116.086
point
-258.710,-2.553,-113.521
point
-258.878,-2.552,-111.778
reverse
// Pedestrian number 2{
17				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-259.951,-2.552,-111.080
point
-261.131,-2.552,-110.314
point
-262.437,-2.552,-108.285
point
-263.675,-2.552,-105.560
reverse
// Pedestrian number 2{
14				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-249.319,-2.552,-113.961
point
-248.765,-2.556,-115.149
point
-248.531,-2.556,-116.031
reverse
// Pedestrian number 2{
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-251.094,-2.553,-118.841
point
-251.966,-2.553,-118.639
point
-254.392,-2.553,-114.695
reverse
// Pedestrian number 2{
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-252.938,-2.553,-118.360
point
-254.900,-2.553,-117.529
point
-255.599,-2.553,-117.270
point
-256.842,-2.552,-116.703
reverse
// Pedestrian number 2{
13				// Ref num
7				// Number of instructions
4				// Initial instruction
point
-256.254,-1.949,-118.131
point
-254.857,-2.538,-117.934
point
-254.685,-2.551,-117.868
point
-252.227,-2.555,-115.463
point
-249.649,-2.552,-113.015
point
-249.474,-2.375,-112.792
reverse
// Pedestrian number 2{
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-248.059,-2.552,-116.864
point
-253.718,-2.552,-118.154
point
-255.578,-2.553,-116.628
point
-263.178,-2.552,-112.017
reverse
// Pedestrian number 2{
12				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-267.119,-2.552,-105.096
point
-268.950,-2.552,-100.688
point
-268.972,-2.552,-99.885
point
-268.770,-2.552,-98.700
reverse
// Pedestrian number 2{
17				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-265.747,-2.552,-102.873
point
-266.213,-2.552,-102.369
point
-267.388,-2.552,-101.191
point
-268.140,-2.552,-99.290
reverse
// Pedestrian number 2{
12				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-268.510,-2.552,-96.082
point
-269.419,-2.552,-95.982
point
-269.996,-2.552,-96.009
point
-270.965,-2.552,-95.727
reverse
// Pedestrian number 2{
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-270.612,-2.552,-93.539
point
-272.192,-2.552,-92.011
point
-273.328,-2.552,-89.927
reverse
// Pedestrian number 2z
17				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-271.353,-2.552,-86.780
point
-270.768,-2.552,-88.015
point
-271.118,-2.552,-89.710
point
-271.604,-2.552,-94.356
reverse
// Pedestrian number 2z
14				// Ref num
7				// Number of instructions
3				// Initial instruction
point
-273.074,-2.552,-90.576
point
-271.751,-2.552,-91.215
point
-270.852,-2.552,-92.071
point
-270.782,-2.552,-92.561
point
-270.966,-2.552,-93.711
point
-270.543,-2.552,-94.764
reverse
// Pedestrian number 2z
13				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-269.747,-2.552,-95.901
point
-269.889,-2.552,-96.406
point
-269.582,-2.552,-97.218
point
-269.587,-2.552,-99.100
reverse
// Pedestrian number 2z
3				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-270.059,-2.552,-97.862
point
-270.202,-2.552,-96.389
point
-269.989,-2.552,-96.204
point
-269.321,-2.552,-95.592
point
-268.932,-2.552,-95.083
reverse
// Pedestrian number 2z
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-270.161,-2.552,-95.634
point
-270.684,-2.552,-95.088
point
-271.006,-2.552,-93.934
point
-270.847,-2.552,-93.521
reverse
// Pedestrian number 2z
8				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-269.579,-2.552,-93.592
point
-270.703,-2.552,-92.680
point
-270.711,-2.552,-91.995
point
-271.785,-2.552,-89.840
point
-274.849,-2.552,-86.565
reverse
// Pedestrian number 2z
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-276.199,-2.552,-83.962
point
-275.976,-2.552,-81.561
point
-276.119,-2.552,-78.714
reverse
// Pedestrian number 2z
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-277.056,-2.552,-77.404
point
-279.163,-2.552,-76.725
point
-282.674,-2.552,-75.077
reverse
// Pedestrian number 2z
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-282.977,-2.552,-74.724
point
-283.517,-2.543,-71.793
point
-284.632,-2.543,-66.837
reverse
// Pedestrian number 2z
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-285.338,-2.538,-71.991
point
-283.194,-2.549,-72.864
point
-280.490,-2.558,-73.152
reverse
// Pedestrian number 2y
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-283.911,-2.549,-73.598
point
-283.794,-2.544,-72.309
point
-283.355,-2.540,-70.791
point
-283.430,-2.549,-66.934
reverse
// Pedestrian number 2y
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-283.092,-2.539,-70.381
point
-282.657,-2.547,-71.956
point
-281.994,-2.552,-75.766
reverse
// Pedestrian number 2y
13				// Ref num
7				// Number of instructions
3				// Initial instruction
point
-290.901,-2.611,-66.648
point
-288.910,-2.545,-67.798
point
-285.894,-2.539,-70.891
point
-285.276,-2.538,-71.726
point
-285.246,-2.538,-72.306
point
-284.425,-2.536,-73.187
reverse
// Pedestrian number 2y
5				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-301.475,-3.692,-66.697
point
-302.839,-3.869,-66.676
point
-304.337,-3.982,-66.926
point
-304.980,-4.043,-66.621
point
-305.100,-4.048,-66.229
reverse
// Pedestrian number 2y
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-305.706,-4.048,-65.861
point
-307.220,-4.048,-65.232
point
-308.040,-4.048,-64.304
point
-308.729,-4.048,-62.258
reverse
// Pedestrian number 2y
12				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-303.969,-3.932,-69.400
point
-305.848,-4.041,-69.120
point
-306.448,-4.048,-68.937
point
-308.740,-4.048,-67.573
point
-309.267,-4.048,-67.093
reverse
// Pedestrian number 2y
17				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-307.891,-4.048,-64.913
point
-308.340,-4.048,-64.183
point
-309.051,-4.048,-61.428
point
-309.025,-4.048,-59.326
reverse
// Pedestrian number 2y
12				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-308.805,-4.048,-58.997
point
-308.080,-4.048,-57.100
point
-307.767,-4.048,-56.761
point
-307.414,-4.048,-56.369
reverse
// Pedestrian number 2y
17				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-309.587,-4.048,-54.168
point
-310.881,-4.048,-57.725
point
-312.007,-4.048,-60.843
reverse
// Pedestrian number 2y
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-311.804,-4.048,-61.502
point
-310.921,-4.048,-64.048
point
-310.213,-4.048,-66.074
reverse
// Pedestrian number 2x
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-308.079,-4.048,-68.005
point
-308.182,-4.048,-63.287
point
-306.977,-3.161,-62.076
point
-306.926,-3.032,-61.235
reverse
// Pedestrian number 2x
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-307.824,-3.507,-61.157
point
-308.813,-4.048,-59.570
point
-308.793,-4.048,-58.301
reverse
// Pedestrian number 2x
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-307.130,-4.048,-55.946
point
-306.899,-4.048,-55.779
point
-305.834,-4.096,-55.090
reverse
// Pedestrian number 2x
17				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-304.480,-4.189,-54.490
point
-301.394,-4.602,-53.573
point
-298.731,-5.309,-52.973
reverse
// Pedestrian number 2x
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-301.548,-4.739,-50.540
point
-298.747,-5.509,-49.881
point
-294.961,-6.758,-49.008
reverse
// Pedestrian number 2x
29				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-294.532,-6.654,-51.923
point
-291.191,-7.824,-50.756
point
-290.127,-7.884,-50.524
reverse
// Pedestrian number 2x
5				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-289.188,-7.940,-50.205
point
-287.985,-8.005,-49.575
point
-286.891,-8.005,-45.905
point
-287.160,-8.005,-42.215
point
-287.398,-8.005,-40.596
reverse
// Pedestrian number 2x
3				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-284.490,-8.005,-43.511
point
-284.121,-8.005,-42.692
point
-283.543,-7.696,-41.533
point
-282.199,-6.852,-41.083
reverse
// Pedestrian number 2x
1				// Ref num
9				// Number of instructions
7				// Initial instruction
point
-284.061,-8.005,-41.127
point
-284.608,-8.005,-40.453
point
-284.884,-8.005,-39.560
point
-284.993,-8.005,-37.977
point
-287.371,-8.005,-34.764
point
-287.551,-7.986,-34.585
point
-287.611,-7.921,-34.413
point
-288.716,-7.151,-32.136
reverse
// Pedestrian number 2x
29				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-289.499,-8.005,-37.279
point
-288.412,-8.004,-38.154
point
-287.520,-8.005,-38.325
point
-284.597,-8.005,-39.560
reverse
// Pedestrian number 2w
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-287.740,-8.005,-39.147
point
-284.316,-8.005,-42.046
point
-284.425,-8.005,-44.507
reverse
// Pedestrian number 2w
8				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-284.152,-7.877,-44.685
point
-284.000,-7.508,-45.728
point
-283.980,-7.130,-46.951
point
-283.854,-6.798,-47.763
reverse
// Pedestrian number 2w
5				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-285.223,-8.005,-46.513
point
-286.407,-8.005,-43.838
point
-286.426,-8.005,-42.530
point
-287.079,-8.005,-41.616
point
-288.226,-8.005,-38.548
reverse
// Pedestrian number 2w
8				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-286.337,-8.005,-35.899
point
-290.809,-8.008,-35.344
point
-293.451,-8.166,-35.358
point
-296.326,-8.525,-35.300
reverse
// Pedestrian number 2w
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-294.880,-8.344,-35.505
point
-296.654,-8.568,-35.057
point
-298.035,-9.013,-34.785
point
-299.920,-9.442,-35.244
reverse
// Pedestrian number 2w
29				// Ref num
9				// Number of instructions
4				// Initial instruction
point
-298.103,-9.166,-32.271
point
-298.430,-9.285,-32.439
point
-298.882,-9.455,-32.377
point
-299.777,-9.776,-32.361
point
-300.623,-9.943,-32.472
point
-301.872,-10.077,-33.420
point
-303.143,-10.477,-33.677
point
-304.486,-10.909,-34.832
reverse
// Pedestrian number 2w
29				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-307.012,-11.793,-31.538
point
-309.669,-11.971,-32.758
point
-311.882,-11.971,-33.109
point
-313.365,-11.971,-32.132
reverse
// Pedestrian number 2w
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-312.356,-11.971,-32.852
point
-313.862,-11.971,-31.535
point
-315.467,-11.971,-29.014
reverse
// Pedestrian number 2w
17				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-312.483,-11.971,-28.242
point
-313.842,-11.971,-28.279
point
-315.790,-11.970,-27.237
point
-316.223,-11.971,-25.335
reverse
// Pedestrian number 2w
29				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-310.193,-11.971,-30.589
point
-311.153,-11.971,-30.196
point
-312.376,-11.970,-28.775
point
-313.233,-11.971,-26.534
point
-313.226,-11.971,-25.457
reverse
// Pedestrian number 2v
12				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-315.747,-11.971,-28.199
point
-316.031,-11.971,-26.501
point
-316.089,-11.970,-24.197
point
-314.094,-11.971,-19.618
reverse
// Pedestrian number 2v
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-311.120,-11.971,-20.670
point
-315.798,-11.970,-23.028
point
-316.008,-11.970,-23.627
reverse
// Pedestrian number 2v
8				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-315.036,-11.971,-21.178
point
-313.307,-11.971,-25.137
point
-312.906,-11.971,-28.068
point
-312.947,-11.971,-32.545
reverse
// Pedestrian number 2v
1				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-311.320,-11.971,-33.469
point
-309.793,-11.956,-33.640
point
-308.575,-11.841,-34.222
point
-307.413,-11.808,-34.660
reverse
// Pedestrian number 2v
12				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-310.494,-11.971,-33.931
point
-312.101,-11.970,-28.817
point
-313.131,-11.971,-26.533
point
-313.080,-11.971,-24.407
point
-312.879,-11.971,-23.506
reverse
// Pedestrian number 2v
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-309.599,-12.052,-19.766
point
-307.176,-12.105,-18.568
point
-304.902,-12.106,-18.046
reverse
// Pedestrian number 2v
3				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-303.618,-12.106,-17.323
point
-297.948,-12.106,-11.354
point
-295.342,-12.106,-9.547
reverse
// Pedestrian number 2v
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-294.592,-12.106,-12.659
point
-293.640,-12.106,-11.881
point
-290.160,-12.119,-9.516
reverse
// Pedestrian number 2v
8				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-293.474,-12.106,-8.167
point
-292.018,-12.119,-7.229
point
-291.375,-12.134,-6.629
point
-290.872,-12.106,-6.118
reverse
// Pedestrian number 2v
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-287.163,-12.203,-7.032
point
-286.617,-11.939,-7.076
point
-285.686,-11.252,-7.410
reverse
// Pedestrian number 300
8				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-285.871,-12.313,-5.671
point
-283.815,-12.540,-3.074
point
-283.024,-12.625,-2.703
point
-282.159,-12.592,-2.212
reverse
// Pedestrian number 301
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-275.947,-15.455,15.963
point
-274.709,-15.615,18.590
point
-268.921,-15.627,21.687
reverse
// Pedestrian number 302
13				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-269.260,-15.627,21.154
point
-269.260,-15.627,21.154
point
-274.742,-15.616,19.025
point
-274.987,-15.613,18.556
reverse
// Pedestrian number 303
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-275.048,-15.617,19.181
point
-275.296,-15.626,21.891
point
-274.156,-15.627,26.848
point
-275.075,-15.627,28.241
reverse
// Pedestrian number 304
13				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-276.114,-15.627,28.865
point
-276.806,-15.627,28.757
point
-276.806,-15.627,28.757
point
-278.927,-15.627,27.563
point
-279.874,-15.627,27.672
reverse
// Pedestrian number 305
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-275.915,-15.627,28.331
point
-274.419,-15.627,26.937
point
-273.867,-15.627,26.357
reverse
// Pedestrian number 306
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-275.798,-15.627,23.631
point
-275.376,-15.627,22.759
point
-269.842,-15.625,20.327
point
-269.526,-15.626,20.538
reverse
// Pedestrian number 307
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-269.464,-15.627,20.822
point
-271.195,-15.627,21.548
point
-273.283,-15.622,20.901
point
-275.121,-15.621,20.428
reverse
// Pedestrian number 308
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-271.521,-15.627,23.166
point
-270.772,-15.627,23.565
point
-267.721,-15.627,22.818
reverse
// Pedestrian number 309
13				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-264.867,-15.627,23.968
point
-266.649,-15.627,23.637
point
-269.462,-15.627,22.086
point
-275.319,-15.623,21.089
reverse
// Pedestrian number 310
13				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-270.668,-15.621,19.419
point
-269.911,-15.627,20.721
point
-270.254,-15.629,22.299
point
-270.389,-15.627,23.600
point
-269.725,-15.627,24.812
reverse
// Pedestrian number 311
14				// Ref num
7				// Number of instructions
2				// Initial instruction
point
-272.612,-15.627,23.147
point
-273.271,-15.627,24.415
point
-273.594,-15.627,24.889
point
-273.671,-15.627,25.698
point
-275.341,-15.627,26.548
point
-278.109,-15.627,26.682
reverse
// Pedestrian number 312
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-280.589,-15.627,33.937
point
-280.646,-15.627,35.766
point
-279.847,-15.627,37.526
reverse
// Pedestrian number 313
14				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-282.105,-15.627,40.554
point
-281.144,-15.627,41.464
point
-280.896,-15.627,45.967
reverse
// Pedestrian number 314
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-275.261,-16.364,57.993
point
-275.306,-16.591,59.619
point
-274.518,-16.875,61.463
reverse
// Pedestrian number 315
17				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-274.434,-16.902,61.736
point
-275.504,-17.083,63.476
point
-276.184,-17.419,66.389
point
-275.677,-17.638,68.356
reverse
// Pedestrian number 316
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-276.525,-17.276,65.334
point
-276.656,-17.120,64.043
point
-277.100,-16.921,62.514
reverse
// Pedestrian number 317
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-274.600,-16.823,61.127
point
-277.527,-16.613,60.288
point
-277.928,-16.431,59.083
reverse
// Pedestrian number 318
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-277.329,-16.783,61.450
point
-274.153,-17.132,63.567
point
-273.629,-17.375,65.448
reverse
// Pedestrian number 319
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-272.091,-18.286,72.098
point
-273.900,-18.648,76.202
point
-273.648,-18.772,77.788
reverse
// Pedestrian number 320
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-273.480,-18.815,78.534
point
-272.702,-18.907,81.642
point
-272.380,-18.909,83.736
reverse
// Pedestrian number 321
3				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-272.125,-18.910,84.419
point
-268.699,-18.913,87.433
point
-268.551,-18.914,88.454
reverse
// Pedestrian number 322
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-267.860,-18.915,90.476
point
-267.589,-18.915,92.464
point
-267.190,-18.917,93.251
reverse
// Pedestrian number 323
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-267.361,-18.915,93.750
point
-267.103,-18.915,94.906
point
-266.904,-18.915,96.369
reverse
// Pedestrian number 324
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-266.662,-18.915,97.291
point
-265.214,-18.915,103.269
point
-263.493,-18.915,105.492
reverse
// Pedestrian number 325
12				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-264.258,-18.915,103.497
point
-262.888,-18.915,103.594
point
-259.906,-18.916,102.546
point
-258.473,-18.916,102.074
reverse
// Pedestrian number 326
12				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-260.209,-18.915,104.902
point
-261.442,-18.915,105.097
point
-262.568,-18.915,105.461
point
-264.052,-18.915,105.634
reverse
// Pedestrian number 327
17				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-264.786,-18.914,105.968
point
-266.973,-18.915,105.454
point
-268.860,-18.916,104.565
reverse
// Pedestrian number 328
17				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-265.318,-18.915,102.577
point
-267.780,-18.916,104.111
point
-271.038,-18.916,107.321
reverse
// Pedestrian number 329
14				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-271.659,-18.916,107.585
point
-272.700,-18.916,107.682
point
-275.621,-18.916,108.434
reverse
// Pedestrian number 330
12				// Ref num
7				// Number of instructions
5				// Initial instruction
point
-277.279,-18.916,106.409
point
-278.052,-18.916,106.785
point
-279.855,-18.916,106.897
point
-280.732,-18.916,107.190
point
-281.522,-18.916,107.353
point
-287.395,-18.916,108.702
reverse
// Pedestrian number 331
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-287.781,-18.915,109.007
point
-287.005,-18.915,109.530
point
-284.483,-18.915,110.371
reverse
// Pedestrian number 332
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-285.320,-18.915,110.565
point
-283.753,-18.914,110.043
point
-282.909,-18.914,108.214
point
-282.223,-18.916,107.447
reverse
// Pedestrian number 333
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-278.529,-18.914,108.997
point
-276.784,-18.916,108.745
point
-272.298,-18.916,105.406
reverse
// Pedestrian number 334
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-271.767,-18.916,105.116
point
-270.238,-18.916,105.152
point
-268.600,-18.916,104.356
reverse
// Pedestrian number 335
29				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-257.403,-18.916,104.343
point
-256.166,-18.915,103.924
point
-253.647,-18.916,101.001
reverse
// Pedestrian number 336
29				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-251.203,-18.916,100.337
point
-248.252,-18.916,101.620
point
-243.938,-18.915,100.866
reverse
// Pedestrian number 337
12				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-241.681,-18.915,100.247
point
-239.599,-18.916,97.883
point
-236.994,-18.916,97.068
point
-236.052,-18.916,96.823
reverse
// Pedestrian number 338
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-230.100,-18.916,95.496
point
-227.497,-18.916,96.367
point
-224.827,-18.916,96.739
reverse
// Pedestrian number 339
17				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-224.247,-18.916,96.663
point
-223.229,-18.916,95.255
point
-222.475,-18.916,93.876
reverse
// Pedestrian number 340
17				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-222.129,-18.916,96.112
point
-225.941,-18.916,95.009
point
-227.570,-18.916,94.916
reverse
// Pedestrian number 341
29				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-230.675,-18.916,95.681
point
-232.337,-18.916,98.317
point
-234.208,-18.916,98.923
reverse
// Pedestrian number 342
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-236.473,-18.916,99.195
point
-237.403,-18.916,99.547
point
-239.771,-18.916,99.977
reverse
// Pedestrian number 343
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-244.636,-18.916,101.256
point
-243.045,-18.915,100.927
point
-240.603,-18.916,100.428
reverse
// Pedestrian number 344
17				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-241.676,-18.916,97.872
point
-242.133,-18.915,99.371
point
-243.668,-18.916,101.059
reverse
// Pedestrian number 345
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-258.016,-18.916,101.915
point
-256.635,-18.915,101.778
point
-251.856,-18.916,102.896
reverse
// Pedestrian number 346
3				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-242.661,-18.915,94.750
point
-243.590,-18.915,93.460
point
-245.618,-18.915,91.881
point
-245.822,-18.915,91.091
point
-246.407,-18.915,89.219
reverse
// Pedestrian number 347
1				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-248.346,-18.916,88.619
point
-248.651,-18.916,88.589
point
-250.594,-18.916,89.034
point
-253.616,-18.916,89.690
reverse
// Pedestrian number 348
5				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-256.635,-18.916,90.560
point
-253.937,-18.916,89.438
point
-252.016,-18.916,89.394
point
-250.196,-18.916,87.138
reverse
// Pedestrian number 349
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-248.563,-18.916,86.478
point
-249.387,-18.916,87.020
point
-253.946,-18.916,87.627
reverse
// Pedestrian number 350
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-255.604,-18.916,87.920
point
-257.768,-18.915,90.792
point
-258.445,-18.916,90.861
reverse
// Pedestrian number 351
17				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-240.526,-18.915,84.616
point
-239.882,-18.915,84.350
point
-235.910,-18.915,83.580
reverse
// Pedestrian number 352
8				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-235.968,-18.916,85.765
point
-239.119,-18.916,86.048
point
-240.148,-18.916,86.797
point
-241.421,-18.916,86.919
point
-242.623,-18.916,87.273
reverse
// Pedestrian number 353
1				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-243.849,-18.916,87.634
point
-244.802,-18.915,85.567
point
-245.180,-18.914,83.335
point
-245.664,-18.913,82.051
point
-245.604,-18.912,81.275
reverse
// Pedestrian number 354
17				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-249.726,-18.892,75.676
point
-247.778,-18.859,74.234
point
-247.643,-18.786,72.308
point
-247.717,-18.737,71.682
reverse
// Pedestrian number 355
14				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-246.677,-18.906,75.374
point
-248.844,-18.909,77.993
point
-248.383,-18.911,80.406
reverse
// Pedestrian number 356
12				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-249.638,-18.916,89.036
point
-246.949,-18.915,88.290
point
-244.024,-18.916,87.838
point
-242.617,-18.915,85.084
point
-241.820,-18.915,84.752
reverse
// Pedestrian number 357
29				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-230.822,-18.916,84.707
point
-229.908,-18.916,84.146
point
-228.819,-18.916,84.256
point
-226.632,-18.916,83.831
point
-224.363,-18.916,81.696
reverse
// Pedestrian number 358
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-223.842,-18.916,82.470
point
-225.192,-18.916,81.939
point
-227.269,-18.916,81.629
reverse
// Pedestrian number 359
17				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-225.378,-18.916,81.111
point
-227.952,-18.917,81.760
point
-232.958,-18.916,85.192
reverse
// Pedestrian number 360
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-233.629,-18.916,85.244
point
-235.137,-18.915,85.428
point
-237.883,-18.916,84.002
reverse
// Pedestrian number 361
1				// Ref num
7				// Number of instructions
5				// Initial instruction
point
-234.603,-18.916,83.075
point
-237.291,-18.916,84.277
point
-239.141,-18.916,84.414
point
-240.060,-18.916,84.651
point
-241.329,-18.914,84.995
point
-243.182,-18.916,87.368
reverse
// Pedestrian number 362
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-243.846,-18.915,89.669
point
-243.772,-18.915,91.633
point
-242.658,-18.915,94.584
reverse
// Pedestrian number 363
17				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-225.214,-18.916,96.958
point
-224.474,-18.916,96.468
point
-224.210,-18.916,95.897
point
-223.458,-18.916,94.270
reverse
// Pedestrian number 364
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-289.800,-18.915,98.099
point
-287.528,-18.915,97.391
point
-286.992,-18.915,95.275
reverse
// Pedestrian number 365
1				// Ref num
7				// Number of instructions
3				// Initial instruction
point
-286.584,-18.916,95.062
point
-285.122,-18.916,94.775
point
-284.024,-18.916,94.553
point
-282.993,-18.916,94.208
point
-281.769,-18.916,94.357
point
-279.257,-18.916,93.459
reverse
// Pedestrian number 366
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-278.403,-18.916,93.124
point
-276.421,-18.916,92.787
point
-273.351,-18.916,92.168
reverse
// Pedestrian number 367
12				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-276.536,-18.916,95.028
point
-277.883,-18.916,95.336
point
-279.189,-18.916,95.195
point
-281.667,-18.916,96.371
reverse
// Pedestrian number 368
17				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-280.027,-18.916,95.991
point
-278.853,-18.916,95.361
point
-277.985,-18.916,93.932
point
-277.008,-18.916,92.852
reverse
// Pedestrian number 369
8				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-275.923,-18.916,92.597
point
-274.557,-18.916,92.760
point
-272.792,-18.916,92.171
point
-267.385,-18.915,90.680
reverse
// Pedestrian number 370
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-249.956,-17.586,62.402
point
-253.447,-17.126,59.029
point
-253.663,-16.985,57.797
reverse
// Pedestrian number 371
17				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-252.848,-17.401,61.382
point
-251.877,-16.860,56.561
point
-251.740,-16.522,54.063
point
-252.232,-16.232,51.727
reverse
// Pedestrian number 372
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-255.093,-16.136,51.243
point
-255.367,-16.081,50.658
point
-253.478,-15.866,48.171
reverse
// Pedestrian number 373
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-259.604,-15.627,19.171
point
-263.137,-15.657,16.034
point
-263.787,-15.657,14.920
reverse
// Pedestrian number 374
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-266.962,-15.680,-2.238
point
-267.167,-15.791,-4.341
point
-267.122,-15.904,-6.260
reverse
// Pedestrian number 375
1				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-264.090,-15.692,-2.653
point
-264.235,-15.791,-4.428
point
-264.105,-15.851,-5.513
point
-264.434,-16.113,-10.220
point
-264.228,-16.144,-10.802
reverse
// Pedestrian number 376
8				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-264.208,-16.184,-11.530
point
-264.744,-16.682,-17.259
point
-265.236,-16.733,-17.799
point
-265.035,-16.840,-18.964
reverse
// Pedestrian number 377
3				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-119.834,-13.901,-123.061
point
-117.564,-13.901,-123.633
point
-115.680,-13.901,-123.977
reverse
// Pedestrian number 378
29				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-109.031,-13.901,-125.677
point
-105.715,-13.901,-126.182
point
-102.975,-13.901,-127.024
reverse
// Pedestrian number 379
1				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-101.611,-13.901,-127.207
point
-99.451,-13.901,-127.706
point
-96.372,-13.901,-128.519
point
-93.558,-13.901,-129.240
reverse
// Pedestrian number 380
5				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-91.666,-13.901,-126.863
point
-90.408,-13.901,-126.956
point
-87.817,-13.901,-127.590
point
-86.489,-13.901,-128.258
point
-85.750,-13.901,-130.193
reverse
// Pedestrian number 381
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-84.949,-13.901,-131.149
point
-80.765,-13.901,-129.335
point
-79.234,-13.901,-129.693
reverse
// Pedestrian number 382
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-77.973,-13.901,-129.919
point
-76.168,-13.900,-133.065
point
-73.672,-13.901,-133.667
reverse
// Pedestrian number 383
13				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-83.065,-13.901,-131.665
point
-84.022,-13.901,-131.468
point
-87.263,-13.901,-130.582
point
-88.684,-13.901,-130.165
point
-89.755,-13.901,-129.999
reverse
// Pedestrian number 384
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-91.735,-13.901,-126.627
point
-93.750,-13.901,-126.619
point
-97.768,-13.901,-125.274
reverse
// Pedestrian number 385
29				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-98.194,-13.901,-125.123
point
-101.434,-13.901,-124.704
point
-103.321,-13.901,-124.105
point
-104.968,-13.901,-123.493
reverse
// Pedestrian number 386
5				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-111.649,-13.901,-124.905
point
-113.716,-13.901,-122.206
point
-115.137,-13.901,-121.271
point
-116.340,-13.901,-120.804
point
-118.246,-13.901,-120.392
reverse
// Pedestrian number 387
3				// Ref num
7				// Number of instructions
4				// Initial instruction
point
-121.292,-13.901,-119.788
point
-123.196,-13.901,-119.728
point
-124.535,-13.901,-118.956
point
-125.394,-13.901,-118.697
point
-126.965,-13.901,-118.549
point
-128.145,-13.901,-118.237
reverse
// Pedestrian number 388
1				// Ref num
7				// Number of instructions
3				// Initial instruction
point
-132.275,-13.901,-119.952
point
-135.456,-13.817,-119.294
point
-137.788,-13.901,-118.554
point
-140.212,-13.901,-118.253
point
-140.870,-13.901,-117.947
point
-141.976,-13.977,-117.808
reverse
// Pedestrian number 389
3				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-145.000,-14.111,-114.419
point
-147.714,-14.343,-113.757
point
-148.978,-14.441,-113.374
point
-150.077,-14.520,-113.405
point
-151.259,-14.618,-112.759
reverse
// Pedestrian number 390
29				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-154.072,-14.744,-114.431
point
-156.939,-14.906,-113.855
point
-158.349,-14.962,-112.972
point
-160.074,-15.001,-112.697
reverse
// Pedestrian number 391
13				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-163.051,-15.344,-108.087
point
-164.301,-15.485,-107.578
point
-166.077,-15.909,-106.568
point
-166.565,-16.010,-106.127
point
-167.904,-16.244,-105.358
reverse
// Pedestrian number 392
8				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-169.241,-16.457,-104.871
point
-170.250,-16.652,-104.404
point
-172.089,-17.158,-102.408
point
-173.911,-17.623,-100.836
reverse
// Pedestrian number 393
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-183.381,-17.667,-94.703
point
-185.582,-17.667,-93.495
point
-187.395,-17.667,-92.805
point
-188.499,-17.667,-92.221
reverse
// Pedestrian number 394
13				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-189.212,-17.667,-92.062
point
-193.357,-17.667,-93.250
point
-194.419,-17.667,-93.268
point
-195.772,-17.667,-92.864
point
-196.934,-17.667,-92.532
reverse
// Pedestrian number 395
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-200.913,-17.667,-89.040
point
-202.033,-17.667,-88.797
point
-204.014,-17.667,-88.626
point
-205.983,-17.667,-88.356
reverse
// Pedestrian number 396
1				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-205.578,-17.667,-91.182
point
-207.331,-17.667,-90.489
point
-208.538,-17.667,-90.705
point
-209.648,-17.667,-91.079
point
-212.465,-17.667,-91.333
reverse
// Pedestrian number 397
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-222.421,-17.667,-90.108
point
-225.237,-17.667,-90.657
point
-228.646,-17.667,-94.731
reverse
// Pedestrian number 398
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-222.851,-17.667,-92.715
point
-225.380,-17.667,-93.718
point
-230.772,-17.667,-92.287
reverse
// Pedestrian number 399
13				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-231.315,-17.667,-92.144
point
-236.308,-17.667,-91.844
point
-237.168,-17.667,-90.632
point
-238.428,-17.667,-88.917
reverse
// Pedestrian number 400
14				// Ref num
7				// Number of instructions
4				// Initial instruction
point
-234.244,-17.667,-90.010
point
-234.876,-17.667,-89.574
point
-235.287,-17.667,-88.471
point
-236.050,-17.667,-87.275
point
-237.103,-17.667,-85.875
point
-237.296,-17.667,-85.318
reverse
// Pedestrian number 401
8				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-239.589,-17.667,-87.027
point
-238.759,-17.667,-88.124
point
-233.632,-17.667,-90.893
point
-233.018,-17.667,-91.433
point
-231.069,-17.667,-95.099
reverse
// Pedestrian number 402
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-229.490,-17.667,-94.925
point
-232.882,-17.667,-94.231
point
-234.970,-17.667,-93.341
reverse
// Pedestrian number 403
29				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-235.881,-17.667,-92.742
point
-237.468,-17.667,-89.190
point
-237.576,-17.667,-86.398
point
-237.810,-17.667,-84.738
point
-239.074,-17.667,-83.249
reverse
// Pedestrian number 404
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-239.940,-17.667,-81.940
point
-241.389,-17.667,-80.509
point
-242.760,-17.667,-79.235
point
-243.512,-17.667,-78.624
reverse
// Pedestrian number 405
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-245.986,-17.667,-80.303
point
-244.407,-17.667,-81.344
point
-243.769,-17.667,-82.153
point
-242.335,-17.667,-83.856
reverse
// Pedestrian number 406
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-241.138,-17.667,-85.195
point
-241.675,-17.667,-83.809
point
-242.744,-17.667,-82.883
point
-243.966,-17.667,-78.255
reverse
// Pedestrian number 407
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-245.521,-17.667,-77.607
point
-247.017,-17.667,-77.002
point
-249.465,-17.667,-76.193
reverse
// Pedestrian number 408
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-251.893,-17.667,-74.479
point
-256.607,-17.667,-74.979
point
-259.508,-17.667,-74.238
reverse
// Pedestrian number 409
13				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-264.458,-17.667,-70.671
point
-265.318,-17.667,-65.596
point
-266.224,-17.667,-63.769
point
-266.944,-17.667,-63.032
point
-267.397,-17.667,-61.949
reverse
// Pedestrian number 410
14				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-268.182,-17.667,-60.830
point
-267.928,-17.667,-62.571
point
-266.643,-17.667,-64.806
point
-266.713,-17.667,-67.852
point
-265.824,-17.667,-68.878
reverse
// Pedestrian number 411
3				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-264.989,-17.667,-69.779
point
-262.826,-17.667,-72.031
point
-262.093,-17.667,-72.685
point
-260.609,-17.667,-73.550
point
-257.839,-17.667,-74.706
reverse
// Pedestrian number 412
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-255.378,-17.667,-75.598
point
-252.351,-17.667,-77.418
point
-250.216,-17.667,-79.156
reverse
// Pedestrian number 413
29				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-252.969,-17.667,-73.850
point
-256.132,-17.667,-73.995
point
-258.440,-17.667,-73.304
point
-261.503,-17.667,-69.874
point
-264.039,-17.667,-66.725
reverse
// Pedestrian number 414
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-271.027,-17.667,-61.583
point
-272.535,-17.667,-58.840
point
-274.032,-17.667,-52.526
reverse
// Pedestrian number 415
8				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-271.331,-17.667,-49.860
point
-271.311,-17.667,-48.130
point
-271.297,-17.667,-46.380
point
-271.427,-17.667,-44.970
point
-271.157,-17.667,-43.681
reverse
// Pedestrian number 416
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-268.855,-17.667,-30.778
point
-268.559,-17.667,-30.243
point
-267.896,-17.667,-29.450
reverse
// Pedestrian number 417
3				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-271.924,-17.667,-32.767
point
-272.570,-17.667,-36.082
point
-272.706,-17.667,-37.178
point
-273.465,-17.667,-39.753
reverse
// Pedestrian number 418
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-270.747,-17.667,-40.455
point
-272.866,-17.667,-36.484
point
-272.339,-17.667,-34.237
reverse
// Pedestrian number 419
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-271.845,-17.667,-31.923
point
-269.676,-17.667,-34.570
point
-270.281,-17.667,-37.579
reverse
// Pedestrian number 420
3				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-270.493,-17.667,-38.015
point
-271.410,-17.667,-36.914
point
-272.664,-17.667,-35.041
point
-272.133,-17.667,-33.504
reverse
// Pedestrian number 421
8				// Ref num
7				// Number of instructions
4				// Initial instruction
point
-271.174,-17.667,-31.072
point
-271.721,-17.667,-33.570
point
-272.730,-17.667,-35.622
point
-273.163,-17.667,-37.531
point
-271.921,-17.667,-39.174
point
-271.089,-17.667,-42.821
reverse
// Pedestrian number 422
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-270.053,-17.667,-26.369
point
-269.945,-17.667,-27.000
point
-270.647,-17.667,-28.010
reverse
// Pedestrian number 423
13				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-269.690,-17.667,-25.496
point
-269.842,-17.667,-25.983
point
-270.298,-17.667,-26.927
point
-270.337,-17.667,-28.194
point
-270.756,-17.667,-28.940
reverse
// Pedestrian number 424
14				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-269.406,-17.667,-25.153
point
-268.996,-17.666,-24.854
point
-268.898,-17.355,-22.439
reverse
// Pedestrian number 425
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-266.252,-17.443,-23.823
point
-265.947,-17.238,-22.254
point
-267.972,-16.891,-18.890
reverse
// Pedestrian number 426
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-267.071,-17.667,-26.394
point
-266.334,-17.478,-24.081
point
-266.049,-17.349,-23.131
reverse
// Pedestrian number 427
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-267.927,-17.000,-19.824
point
-268.300,-17.152,-21.026
point
-266.443,-17.541,-24.563
reverse
// Pedestrian number 428
8				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-266.648,-17.641,-25.315
point
-266.742,-17.514,-24.281
point
-266.126,-17.317,-22.841
point
-265.068,-16.746,-17.961
reverse
// Pedestrian number 429
29				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-269.300,-17.624,-24.315
point
-268.899,-17.480,-23.371
point
-268.473,-17.260,-21.869
point
-265.572,-17.078,-21.051
reverse
// Pedestrian number 430
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-287.459,-15.627,39.118
reverse
// Pedestrian number 431
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-287.210,-15.627,40.372
reverse
// Pedestrian number 432
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-286.898,-15.627,41.898
reverse
// Pedestrian number 433
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-280.139,-15.627,35.601
reverse
// Pedestrian number 434
130				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-239.364,-18.916,86.650
reverse
// Pedestrian number 435
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-271.043,-18.916,91.502
reverse
// Pedestrian number 436
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-271.787,-18.916,91.665
reverse
// Pedestrian number 437
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-277.022,-18.916,95.333
reverse
// Pedestrian number 438
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-278.585,-18.916,95.637
reverse
// Pedestrian number 439
129				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-287.680,-18.915,96.539
reverse
// Pedestrian number 440
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-288.693,-18.915,96.701
reverse
// Pedestrian number 441
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-286.898,-18.915,109.796
reverse
// Pedestrian number 442
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-285.751,-18.915,109.419
reverse
// Pedestrian number 443
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-275.152,-18.916,105.913
reverse
// Pedestrian number 444
130				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-267.579,-18.915,103.067
reverse
// Pedestrian number 445
130				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-253.508,-18.916,101.013
reverse
// Pedestrian number 446
130				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-234.220,-18.916,96.708
reverse
// Pedestrian number 447
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-233.295,-18.916,96.507
reverse
// Pedestrian number 448
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-227.150,-18.916,97.137
reverse
// Pedestrian number 449
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-226.593,-18.916,97.000
reverse
// Pedestrian number 450
129				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-222.481,-18.916,94.977
reverse
// Pedestrian number 451
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-221.543,-18.916,95.059
reverse
// Pedestrian number 452
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-221.642,-18.916,94.409
reverse
// Pedestrian number 453
131				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-226.181,-18.916,82.248
reverse
// Pedestrian number 454
131				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-226.707,-18.916,82.354
reverse
// Pedestrian number 455
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-274.307,-17.667,-46.446
reverse
// Pedestrian number 456
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-274.257,-17.667,-44.535
reverse
// Pedestrian number 457
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-274.284,-17.667,-49.706
reverse
// Pedestrian number 458
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-259.818,-17.667,-70.806
reverse
// Pedestrian number 459
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-259.365,-17.667,-71.060
reverse
// Pedestrian number 460
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-260.450,-17.667,-70.372
reverse
// Pedestrian number 461
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-134.149,-13.901,-116.744
reverse
// Pedestrian number 462
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-133.133,-13.901,-116.986
reverse
// Pedestrian number 463
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-94.608,-13.901,-125.770
reverse
// Pedestrian number 464
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-93.850,-13.901,-125.954
reverse
// Pedestrian number 465
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-55.923,-13.561,-133.129
reverse
// Pedestrian number 466
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-87.012,-11.865,-136.051
reverse
// Pedestrian number 467
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-88.779,-12.543,-137.107
reverse
// Pedestrian number 468
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-99.301,-12.059,-137.304
reverse
// Pedestrian number 469
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-177.768,-7.933,-122.214
reverse
// Pedestrian number 470
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-178.348,-7.878,-120.801
reverse
// Pedestrian number 471
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-208.762,-4.206,-119.494
reverse
// Pedestrian number 472
129				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-209.185,-4.137,-120.047
reverse
// Pedestrian number 473
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-258.207,-2.552,-100.866
reverse
// Pedestrian number 474
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-260.159,-2.552,-96.271
reverse
// Pedestrian number 475
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-260.816,-2.552,-94.565
reverse
// Pedestrian number 476
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-268.781,-2.552,-98.559
reverse
// Pedestrian number 477
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-269.871,-2.552,-90.295
reverse
// Pedestrian number 478
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-269.961,-2.552,-90.025
reverse
// Pedestrian number 479
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-301.068,-3.636,-66.648
reverse
// Pedestrian number 480
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-306.901,-4.048,-65.192
reverse
// Pedestrian number 481
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-307.481,-4.048,-64.478
reverse
// Pedestrian number 482
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-307.952,-4.048,-63.872
reverse
// Pedestrian number 483
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-287.591,-8.005,-40.262
reverse
// Pedestrian number 484
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-302.234,-12.106,-16.937
reverse
// Pedestrian number 485
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-301.804,-12.106,-16.744
reverse
// Pedestrian number 486
138				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-271.668,-15.627,24.710
reverse
// Pedestrian number 487
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-272.063,-15.627,24.805
reverse
// Pedestrian number 488
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-271.201,-15.627,24.549
reverse
// Pedestrian number 489
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-272.084,-15.627,23.357
reverse
// Pedestrian number 490
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-214.152,-8.352,-7.375
reverse
// Pedestrian number 491
129				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-213.866,-8.290,-7.552
reverse
// Pedestrian number 492
129				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-202.868,-7.280,-4.228
reverse
// Pedestrian number 493
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-182.746,-5.425,6.452
reverse
// Pedestrian number 494
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-188.515,-5.380,4.779
reverse
// Pedestrian number 495
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-179.419,-5.431,2.074
reverse
// Pedestrian number 496
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-178.465,-5.432,1.182
reverse
// Pedestrian number 497
125				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-146.391,-7.508,-46.202
reverse
// Pedestrian number 498
125				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-135.465,-7.487,-49.345
reverse
// Pedestrian number 499
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-135.327,-18.640,-34.027
reverse
// Pedestrian number 500
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-135.395,-18.641,-34.552
reverse
// Pedestrian number 501
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-83.241,-13.039,-45.299
reverse
// Pedestrian number 502
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-82.370,-13.120,-45.117
reverse
// Pedestrian number 503
129				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-23.442,-15.561,-51.867
reverse
// Pedestrian number 504
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-19.152,-14.991,-77.396
reverse
// Pedestrian number 505
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-19.127,-14.982,-78.241
reverse
// Pedestrian number 506
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-14.327,-15.489,-128.504
reverse
// Pedestrian number 507
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-16.435,-15.631,-132.987
reverse
// Pedestrian number 508
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-43.317,-14.684,-133.268
reverse
// Pedestrian number 509
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-42.642,-14.745,-133.291
reverse
// Pedestrian number 510
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-61.800,-13.901,-133.221
reverse
// Pedestrian number 511
130				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-62.341,-13.901,-136.832
reverse
// Pedestrian number 512
99				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-259.817,-2.552,-96.894
point
-257.866,-2.552,-100.811
point
-256.953,-2.552,-103.715
reverse
START OF OPPONENT PATHS
143                             // Number of path nodes
-250.508,  -15.624,   29.209   // Node #0
-248.031,  -15.627,   38.838   // Node #1
-243.893,  -15.508,   41.091   // Node #2
-229.045,  -11.606,   30.295   // Node #3
-219.342,   -9.352,   16.413   // Node #4
-211.405,   -8.951,   -5.008   // Node #5
-205.429,   -7.881,   -6.354   // Node #6
-193.708,   -5.328,   -1.252   // Node #7
-185.485,   -5.428,    4.234   // Node #8
-180.135,   -5.649,    4.007   // Node #9
-176.502,   -5.435,    0.724   // Node #10
-175.172,   -5.578,   -4.666   // Node #11
-179.573,   -8.050,  -17.537   // Node #12
-178.480,   -8.840,  -24.813   // Node #13
-170.047,   -9.078,  -35.110   // Node #14
-145.562,   -8.802,  -44.806   // Node #15
-134.637,   -8.880,  -48.147   // Node #16
-114.706,   -8.874,  -52.829   // Node #17
-98.251,   -9.426,  -49.700   // Node #18
-70.570,  -12.833,  -45.715   // Node #19
-49.297,  -14.595,  -42.864   // Node #20
-29.777,  -14.596,  -49.524   // Node #21
-21.244,  -14.596,  -58.412   // Node #22
-16.074,  -14.536,  -74.221   // Node #23
-13.154,  -13.419, -116.560   // Node #24
-13.090,  -14.543, -129.299   // Node #25
-15.123,  -14.656, -134.091   // Node #26
-18.705,  -14.657, -136.028   // Node #27
-54.190,  -13.641, -136.953   // Node #28
-152.848,  -13.820, -114.594   // Node #29
-182.531,  -17.667,  -97.063   // Node #30
-196.978,  -17.667,  -91.815   // Node #31
-213.702,  -16.453,  -90.431   // Node #32
-231.135,  -16.453,  -94.236   // Node #33
-235.669,  -16.453,  -91.053   // Node #34
-239.736,  -16.453,  -84.356   // Node #35
-262.737,  -16.453,  -70.095   // Node #36
-271.548,  -16.453,  -59.852   // Node #37
-272.065,  -16.453,  -44.221   // Node #38
-266.345,  -15.303,  -13.850   // Node #39
-264.770,  -14.680,    3.261   // Node #40
-254.830,  -15.627,   43.612   // Node #41
-246.000,  -15.631,   41.796   // Node #42
-164.508,  -15.443, -109.296   // Node #43
-261.168,  -14.680,   17.931   // Node #44
-42.843,  -14.595,  -43.566   // Node #45
-61.143,  -13.907, -135.604   // Node #46
-61.029,  -14.008, -137.895   // Node #47
-63.087,  -13.880, -138.545   // Node #48
-165.655,   -8.969, -139.964   // Node #49
-169.548,   -8.663, -138.876   // Node #50
-173.986,   -8.280, -135.278   // Node #51
-177.553,   -7.952, -129.515   // Node #52
-179.660,   -7.749, -122.705   // Node #53
-182.390,   -7.474, -117.350   // Node #54
-186.456,   -7.046, -113.764   // Node #55
-194.200,   -6.154, -111.558   // Node #56
-201.944,   -5.168, -112.301   // Node #57
-207.828,   -4.353, -115.465   // Node #58
-211.222,   -3.839, -120.541   // Node #59
-214.289,   -3.446, -132.081   // Node #60
-217.671,   -3.160, -141.537   // Node #61
-222.794,   -3.040, -146.983   // Node #62
-231.198,   -2.851, -151.002   // Node #63
-234.592,   -2.789, -150.888   // Node #64
-236.819,   -2.714, -148.580   // Node #65
-248.357,   -2.552, -120.940   // Node #66
-263.688,   -2.553,  -83.516   // Node #67
-269.866,   -2.554,  -75.771   // Node #68
-277.831,   -2.553,  -70.214   // Node #69
-287.929,   -2.543,  -68.170   // Node #70
-303.068,   -3.882,  -68.291   // Node #71
-308.129,   -4.050,  -66.676   // Node #72
-310.546,   -4.048,  -61.708   // Node #73
-309.817,   -4.051,  -56.793   // Node #74
-305.228,   -4.165,  -53.014   // Node #75
-290.748,   -7.872,  -49.147   // Node #76
-286.828,   -8.007,  -46.024   // Node #77
-285.659,   -8.007,  -41.168   // Node #78
-287.814,   -8.006,  -36.492   // Node #79
-292.722,   -8.112,  -34.205   // Node #80
-308.248,  -11.861,  -33.059   // Node #81
-312.892,  -11.973,  -30.429   // Node #82
-314.787,  -11.972,  -24.998   // Node #83
-313.710,  -11.972,  -21.294   // Node #84
-311.184,  -11.997,  -18.843   // Node #85
-298.018,  -12.107,  -13.002   // Node #86
-287.082,  -12.304,   -4.837   // Node #87
-275.559,  -15.002,   12.043   // Node #88
-273.364,  -15.620,   19.899   // Node #89
-275.513,  -15.628,   26.232   // Node #90
-279.528,  -15.628,   29.152   // Node #91
-287.257,  -15.630,   30.917   // Node #92
-289.703,  -15.627,   34.061   // Node #93
-289.404,  -15.627,   37.637   // Node #94
-287.760,  -15.627,   47.198   // Node #95
-286.602,  -15.627,   48.854   // Node #96
-283.707,  -15.627,   50.241   // Node #97
-278.500,  -15.622,   50.878   // Node #98
-259.234,  -15.607,   46.407   // Node #99
-256.702,  -15.627,   46.017   // Node #100
-254.571,  -15.627,   45.821   // Node #101
-253.865,  -15.810,   47.777   // Node #102
-243.116,  -18.915,   98.813   // Node #103
-244.045,  -18.915,   99.848   // Node #104
-263.285,  -18.915,  104.667   // Node #105
-265.357,  -18.915,  103.936   // Node #106
-266.277,  -18.915,  102.814   // Node #107
-249.110,   -2.552, -118.924   // Node #108
-258.219,   -2.552, -113.832   // Node #109
-264.577,   -2.553, -106.675   // Node #110
-272.315,   -2.552,  -88.420   // Node #111
-281.437,   -2.552,  -74.518   // Node #112
-251.441,  -15.623,   26.693   // Node #113
-252.870,  -15.622,   24.867   // Node #114
-255.388,  -15.622,   23.642   // Node #115
-257.148,  -15.621,   23.266   // Node #116
-259.491,  -15.621,   23.901   // Node #117
-266.616,  -15.620,   24.606   // Node #118
-121.550,   -9.078,  -51.179   // Node #119
-123.816,   -9.356,  -45.510   // Node #120
-125.287,  -10.162,  -38.526   // Node #121
-131.912,  -13.190,  -32.790   // Node #122
-140.261,  -13.512,  -30.740   // Node #123
-145.006,  -12.423,  -30.887   // Node #124
-152.848,  -10.049,  -33.455   // Node #125
-155.717,   -8.795,  -36.452   // Node #126
-157.728,   -9.078,  -41.463   // Node #127
-136.791,  -14.001,  -31.257   // Node #128
-143.569,  -18.690,  -47.648   // Node #129
-142.298,  -18.654,  -39.284   // Node #130
-147.869,  -18.642,  -36.886   // Node #131
-151.331,  -18.664,  -39.018   // Node #132
-140.591,  -18.730,  -50.247   // Node #133
-138.024,  -18.671,  -49.664   // Node #134
-136.208,  -18.636,  -45.375   // Node #135
-134.454,  -18.587,  -41.220   // Node #136
-127.194,  -18.571,  -41.632   // Node #137
-126.725,  -18.567,  -41.644   // Node #138
-213.557,   -9.078,    0.401   // Node #139
-271.215,  -18.907,   81.140   // Node #140
-248.192,  -18.907,   75.861   // Node #141
-284.540,  -12.656,   -1.126   // Node #142
149                                           // Number of path sections
0,   1,   0, 255,   0, 255,    1.0,    0   // Section #0
1,   2,   0, 255,   0, 255,    1.0,    0   // Section #1
2,   3,   0, 255,   0, 255,    1.0,    0   // Section #2
3,   4,   0, 255,   0, 255,    1.0,    0   // Section #3
4, 139,   0, 255,   0, 255,    1.0,    0   // Section #4
5,   6,   0, 255,   0, 255,    1.0,    0   // Section #5
6,   7,   0, 255,   0, 255,    1.0,    0   // Section #6
7,   8,   0, 255,   0, 255,    1.0,    0   // Section #7
8,   9,   0, 255,   0, 255,    1.0,    0   // Section #8
9,  10,   0, 255,   0, 255,    1.0,    0   // Section #9
10,  11,   0, 255,   0, 255,    1.0,    0   // Section #10
11,  12,   0, 170,   0, 255,    1.0,    0   // Section #11
12,  13,   0, 255,   0, 255,    1.0,    0   // Section #12
13,  14,   0, 255,   0, 255,    1.0,    0   // Section #13
14, 127,   0, 255,   0, 255,    1.0,    0   // Section #14
15,  16,   0, 255,   0, 255,    1.0,    0   // Section #15
16, 119,   0, 255,   0, 255,    1.0,    0   // Section #16
17,  18,   0, 255,   0, 255,    1.0,    0   // Section #17
18,  19,   0, 255,   0, 255,    1.0,    0   // Section #18
19,  20,   0, 255,   0, 255,    1.0,    0   // Section #19
20,  45,   0, 255,   0, 255,    1.0,    0   // Section #20
21,  22,   0, 255,   0, 255,    1.0,    0   // Section #21
22,  23,   0, 255,   0, 255,    1.0,    0   // Section #22
23,  24,   0, 255,   0,  40,    1.0,    0   // Section #23
24,  25,   0, 255,   0, 255,    1.0,    0   // Section #24
25,  26,   0, 255,   0, 255,    1.0,    0   // Section #25
26,  27,   0, 255,   0, 255,    1.0,    0   // Section #26
27,  28,   0, 255,   0, 255,    1.0,    0   // Section #27
28,  46,   0, 255,   0, 255,    1.0,    0   // Section #28
43,  29,   0,  70,   0, 255,    1.0,    1   // Section #29
31,  30,   0, 255,   0, 255,    1.0,    1   // Section #30
32,  31,   0, 255,   0, 255,    1.0,    1   // Section #31
33,  32,   0,  35,   0, 255,    1.0,    1   // Section #32
34,  33,   0, 255,   0,  35,    1.0,    1   // Section #33
35,  34,   0, 255,   0, 255,    1.0,    1   // Section #34
36,  35,   0, 255,   0, 255,    0.6,    1   // Section #35
37,  36,   0, 255,   0, 255,    0.6,    1   // Section #36
38,  37,   0, 255,   0, 255,    0.6,    1   // Section #37
39,  38,   0, 255,   0, 255,    0.6,    1   // Section #38
40,  39,   0, 255,   0, 255,    0.6,    1   // Section #39
44,  40,   0, 255,   0, 255,    1.1,    1   // Section #40
41,  42,   0, 255,   0, 255,    1.1,    0   // Section #41
30,  43,   0, 255,   0, 255,    1.0,    1   // Section #42
41, 117,   0,  15,   0, 255,    1.1,    1   // Section #43
42,   2,   0, 255,   0, 255,    1.1,    0   // Section #44
45,  21,   0, 255,   0, 255,    1.0,    0   // Section #45
46,  47,   0, 255,   0, 255,    1.0,    1   // Section #46
29,  46,   0, 255,   0, 255,    1.0,    1   // Section #47
47,  48,   0, 255,   0, 255,    1.0,    1   // Section #48
48,  49,   0, 255,   0, 255,    1.0,    1   // Section #49
49,  50,   0,  65,   0,  65,    1.0,    1   // Section #50
50,  51,   0,  50,   0,  45,    1.0,    1   // Section #51
51,  52,   0,  40,   0,  50,    1.0,    1   // Section #52
52,  53,   0, 255,   0, 255,    1.0,    1   // Section #53
53,  54,   0, 255,   0,  70,    1.0,    1   // Section #54
54,  55,   0,  55,   0,  40,    1.0,    1   // Section #55
55,  56,   0,  45,   0,  40,    1.0,    1   // Section #56
56,  57,   0,  40,   0,  30,    1.0,    1   // Section #57
57,  58,   0,  35,   0,  40,    1.0,    1   // Section #58
58,  59,   0,  45,   0,  50,    1.0,    1   // Section #59
59,  60,   0, 255,   0, 255,    1.0,    1   // Section #60
60,  61,   0, 255,   0, 255,    1.0,    1   // Section #61
61,  62,   0, 255,   0, 255,    1.0,    1   // Section #62
62,  63,   0,  65,   0,  40,    1.0,    1   // Section #63
63,  64,   0,  35,   0,  30,    1.0,    1   // Section #64
64,  65,   0,  25,   0,  35,    1.0,    1   // Section #65
65,  66,   0, 255,   0, 255,    1.0,    1   // Section #66
66, 108,   0, 255,   0, 255,    1.0,    1   // Section #67
67,  68,   0, 255,   0, 255,    1.0,    1   // Section #68
68,  69,   0, 255,   0, 255,    1.0,    1   // Section #69
69,  70,   0, 255,   0, 255,    1.0,    1   // Section #70
70,  71,   0, 255,   0, 255,    1.0,    1   // Section #71
71,  72,   0, 255,   0, 255,    1.0,    1   // Section #72
72,  73,   0, 255,   0, 255,    1.0,    1   // Section #73
73,  74,   0, 255,   0, 255,    1.0,    1   // Section #74
74,  75,   0, 255,   0, 255,    1.0,    1   // Section #75
75,  76,   0, 255,   0, 255,    1.0,    1   // Section #76
76,  77,   0, 255,   0, 255,    1.0,    1   // Section #77
77,  78,   0, 255,   0, 255,    1.0,    1   // Section #78
78,  79,   0, 255,   0, 255,    1.0,    1   // Section #79
79,  80,   0, 255,   0, 255,    1.0,    1   // Section #80
80,  81,   0, 255,   0, 255,    1.0,    1   // Section #81
81,  82,   0, 255,   0, 255,    1.0,    1   // Section #82
82,  83,   0, 255,   0, 255,    1.0,    1   // Section #83
83,  84,   0, 255,   0, 255,    1.0,    1   // Section #84
84,  85,   0, 255,   0, 255,    1.0,    1   // Section #85
85,  86,   0, 255,   0, 255,    1.0,    1   // Section #86
86,  87,   0, 255,   0, 255,    1.0,    1   // Section #87
87, 142,   0, 255,   0, 255,    1.0,    1   // Section #88
88,  89,   0, 255,   0, 255,    1.0,    1   // Section #89
89,  90,   0, 255,   0, 255,    1.0,    1   // Section #90
90,  91,   0, 255,   0, 255,    1.0,    1   // Section #91
91,  92,   0, 255,   0, 255,    1.0,    1   // Section #92
92,  93,   0, 255,   0, 255,    1.0,    1   // Section #93
93,  94,   0, 255,   0, 255,    1.0,    1   // Section #94
94,  95,   0, 255,   0, 255,    1.0,    1   // Section #95
95,  96,   0, 255,   0, 255,    1.0,    1   // Section #96
96,  97,   0, 255,   0, 255,    1.0,    1   // Section #97
97,  98,   0, 255,   0, 255,    1.0,    1   // Section #98
98,  99,   0, 255,   0, 255,    1.0,    0   // Section #99
99, 100,   0, 255,   0, 255,    1.0,    0   // Section #100
100, 101,   0, 255,   0, 255,    1.0,    0   // Section #101
102, 101,   0, 255,   0, 255,    1.0,    1   // Section #102
103, 141,   0, 255,   0, 255,    1.0,    1   // Section #103
104, 103,   0, 255,   0, 255,    1.0,    1   // Section #104
105, 104,   0, 255,   0, 255,    1.0,    1   // Section #105
106, 105,   0, 255,   0, 255,    1.0,    1   // Section #106
107, 106,   0, 255,   0, 255,    1.0,    1   // Section #107
98, 140,   0, 255,   0, 255,    1.0,    1   // Section #108
108, 109,   0, 255,   0, 255,    1.0,    0   // Section #109
108,  67,   0, 255,   0, 255,    1.0,    1   // Section #110
109, 110,   0, 255,   0, 255,    1.0,    0   // Section #111
110, 111,   0, 255,   0, 255,    1.0,    0   // Section #112
111, 112,   0, 255,   0, 255,    1.0,    0   // Section #113
112,  70,   0, 255,   0, 255,    1.0,    0   // Section #114
101,  41,   0, 255,   0, 255,    1.0,    1   // Section #115
0, 113,   0, 255,   0, 255,    1.0,    0   // Section #116
113, 114,   0, 255,   0, 255,    1.0,    0   // Section #117
114, 115,   0, 255,   0, 255,    0.9,    0   // Section #118
115, 116,   0, 255,   0, 255,    0.7,    0   // Section #119
116, 117,   0, 255,   0, 255,    0.7,    0   // Section #120
117,  44,   0, 255,   0,  25,    1.1,    1   // Section #121
89, 118,   0, 255,   0, 255,    0.8,    0   // Section #122
118, 117,   0, 255,   0, 255,    0.5,    0   // Section #123
119, 120,   0, 255,   0, 255,    1.0,    0   // Section #124
119,  17,   0, 255,   0, 255,    1.0,    0   // Section #125
120, 121,   0, 255,   0, 255,    1.0,    0   // Section #126
121, 122,   0, 255,   0, 255,    1.0,    0   // Section #127
122, 128,   0, 255,   0, 255,    1.0,    0   // Section #128
123, 124,   0, 255,   0, 255,    1.0,    0   // Section #129
124, 125,   0, 255,   0, 255,    1.0,    0   // Section #130
125, 126,   0, 255,   0, 255,    1.0,    0   // Section #131
126, 127,   0, 255,   0, 255,    1.0,    0   // Section #132
127,  15,   0, 255,   0, 255,    1.0,    0   // Section #133
128, 133,   0, 255,   0, 255,    1.0,    0   // Section #134
128, 123,   0, 255,   0, 255,    1.0,    0   // Section #135
129, 130,   0, 255,   0, 255,    1.3,    0   // Section #136
130, 131,   0, 255,   0, 255,    1.3,    0   // Section #137
131, 132,   0, 255,   0, 255,    1.5,    0   // Section #138
133, 134,   0, 255,   0, 255,    1.0,    0   // Section #139
133, 129,   0, 255,   0, 255,    1.0,    0   // Section #140
134, 135,   0, 255,   0, 255,    1.3,    0   // Section #141
135, 136,   0, 255,   0, 255,    1.3,    0   // Section #142
136, 137,   0, 255,   0, 255,    1.5,    0   // Section #143
137, 138,   0, 255,   0, 255,    1.5,    0   // Section #144
139,   5,   0, 255,   0,  25,    1.0,    0   // Section #145
140, 107,   0, 255,   0, 255,    1.0,    1   // Section #146
141, 102,   0, 255,   0, 255,    1.0,    1   // Section #147
142,  88,   0, 255,   0, 255,    1.0,    1   // Section #148
5                                                             // Number of cop start points
-62.305,    5.485,   20.401,    0.000,    0.000,    0.000   // Cop start point #0
-265.382,   -2.552, -104.894,    0.000,    0.000,    0.000   // Cop start point #1
-14.368,  -15.631, -131.297,    0.000,    0.000,    0.000   // Cop start point #2
-30.700,  -15.561,  -44.719,    0.000,    0.000,    0.000   // Cop start point #3
-215.508,   -9.078,    7.052,    0.000,    0.000,    0.000   // Cop start point #4
END OF OPPONENT PATHS
7										// number of material modifiers
// default material
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
ROAD1.MAT							// skid mark material
//	material '0'
1										// car wall friction
1										// tyre road friction
0.90										// down force
6.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
0										// sparkiness
3										// room for expansion
MUD2.MAT										// room for expansion
//	material '1'
1.2										// car wall friction
1.2										// tyre road friction
1.0										// down force
10.0										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
2.0										// sparkiness
4										// room for expansion
SAND2.MAT										// room for expansion
//	material '2'
1.2										// car wall friction
1										// tyre road friction
1.0										// down force
5										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
0.0										// sparkiness
3										// room for expansion
MUD1.MAT										// room for expansion
//	material '3'
1.2										// car wall friction
1.00										// tyre road friction
1.0										// down force
8.0										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
0.0										// sparkiness
3										// room for expansion
MUD2.MAT										// room for expansion
//	material '4'
1										// car wall friction
1										// tyre road friction
2										// down force
1										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
20										// sparkiness
1										// room for expansion
none									// room for expansion
//	material '5'
1										// car wall friction
1										// tyre road friction
2.0										// down force
4.0										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
1										// sparkiness
4										// room for expansion
SAND2.MAT										// room for expansion
// Non CarObjects
5										// number of non car objects
GASPUMP.TXT
GREENCAR.TXT
WRECK.TXT
PALM2.TXT
PHONE.TXT
3										// number of dust shade tables
61, 84, 33								// r g b values
0.25, 0.5, 0.75							// quarter, half and three quarter "strength"
92, 51, 34							// r g b values
0.25, 0.5, 0.75							// quarter, half and three quarter "strength"
117, 94, 38							// r g b values
0.25, 0.5, 0.75							// quarter, half and three quarter "strength"
12										// Number of network start points
-225.935,-18.923,95.733							//1
100													
-285.004,-18.921,109.366							//2						
279									
-289.563,-18.929,96.926							//3						
280									
-230.433,-18.924,83.239							//4						
101									
-250.041,15.627,31.341							//5						
189									
-289.175,-15.627,38.198							//6						
190									
-268.443,-2.552,-100.573							//7						
339									
-146.921,-9.864,-139.297							//8						
77									
-56.239,-14.331,-135.497							//9						
79									
-30.041,-15.562,-45.459							//10						
91									
-137.211,-14.009,-31.616							//11						
101									
-226.325,-17.668,-92.217							//12						
77									
1										// number of splash files
SPLSHBLU.PIX 								//  name of pixelmapfile for splashes
1
COASTA1.TXT
