VERSION 6							// V1 expects map checkpoint rectangles
// V2 and above expect map checkpoint points
// V3 and above expect splash file stuff at the end
// V4 and above expect two sets of PIX and MAT and ped substitution entry
-256.540,-2.555,-102.5						// Position of centre of start of grid
160									// Direction that grid faces in
// Direction that grid faces in
// Laps, checkpoints etc
60,30,10							// Initial timer count for each skill level
4									// # laps
5000,5000,5000						// Race completed bonus (all laps raced) for each skill level
10000,10000,10000					// Race completed bonus (all peds killed) for each skill level
10000,10000,10000					// Race completed bonus (all oppos wasted) for each skill level
// Width and height of map checkpoint rectangles
9,18
11,26
0									// # checkpoints
6									// # pixelmap files to load
NYSKY1.PIX
C3SKY2.PIX
COASTA1.pix
NCHORIZN.PIX
DRKSCRN.PIX
FOGSCRN.PIX
6									// # pixelmap files to load (low memory)
NYSKY1.PIX
C3SKY2.PIX
COA8TA3.pix
NCHORIZN.PIX
DRKSCRN.PIX
FOGSCRN.PIX
2									// # shade table files to load
COASTA1.TAB
identity.tab
9									// # material files to load
YWW.MAT
WATTY.MAT
NYSKY1.MAT
C3SKY2.MAT
COASTA1.MAT
DARKSKY.MAT
DRKSCRN.MAT
FOGSCRN.MAT
SKIDMARK.MAT
9
YWW.MAT									// # material files to load (low memory)
WATTY.MAT
NYSKY1.MAT
C3SKY2.MAT
COA8TA3.MAT
DARKSKY.MAT
DRKSCRN.MAT
FOGSCRN.MAT
SKIDMARK.MAT
1									// # model files to load
NETCOSTA.dat
1									// # model files to load
NETCSTA8.dat
NETCOSTA.ACT							// Track actor
NETCSTA8.ACT							// Track actor
NETCSTAX.ACT							// Additional actor
// HORIZON STUFF
NCHORIZN.PIX						// Name of sky texture pixelmap (or "none")
4									// Horizontal repetitions of sky texture
66									// Vertical size of sky texture (degrees)
128									// Position of horizon (pixels below top)
dark								// Depth cue mode ("none", "dark" or "fog")
8,0									// Degree of fog/darkness
// DEFAULT ENGINE NOISE
0
// SPECIAL EFFECTS VOLUMES
11				// # special effects volumes
DEFAULT WATER
0.2									// gravity multiplier
50									// viscosity multiplier
0									// Car damage per millisecond
0.002								// Pedestrian damage per millisecond
0									// camera effect index
1									// Sky colour
WATTY.MAT								// Windscreen material to use
5100								// Sound ID of entry noise
5100								// Sound ID of exit noise
2									// Engine noise index
0									// material index
NEW IMPROVED!
8.702, -0.080, -1.941
0.031, 3.583, -0.007
12.018, 0.007, 53.882
-267.444, -15.562, -32.364
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index
NEW IMPROVED!
5.124, 0.000, 5.680
0.000, 1.000, 0.000
-40.065, 0.000, 22.294
-254.058, -16.907, -75.250
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index
NEW IMPROVED!
0.022, 0.000, 1.728
0.000, 2.074, 0.000
-3.583, 0.000, 0.046
-212.111, -17.667, -89.661
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index
NEW IMPROVED!
-0.416, 0.000, -1.677
0.003, 1.728, -0.001
1.398, -0.002, -0.347
-193.901, -17.667, -91.913
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index
NEW IMPROVED!
-0.940, 0.000, -1.848
0.000, 1.000, 0.000
1.283, 0.000, -0.653
-181.791, -16.747, -97.209
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index
NEW IMPROVED!
1.262, 0.000, 1.645
0.000, 1.728, 0.000
-1.143, 0.000, 0.876
-171.178, -16.427, -105.123
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index
NEW IMPROVED!
1.210, 0.000, 1.684
0.014, 1.440, -0.010
-0.975, 0.014, 0.700
-165.651, -14.506, -108.596
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index
NEW IMPROVED!
-0.462, 0.000, -2.022
0.000, 1.000, 0.000
1.170, 0.000, -0.267
-133.374, -12.981, -118.326
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index
NEW IMPROVED!
-0.472, 0.000, -2.019
0.013, 1.000, -0.003
1.402, -0.020, -0.328
-93.955, -12.942, -127.460
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index
NEW IMPROVED!
-0.444, 0.000, -1.831
0.000, 1.000, 0.000
9.804, 0.000, -2.379
-72.472, -13.061, -132.528
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index
// REFLECTIVE WINDSCREEN SPECIFICATIONS
NYSKY1.MAT							// Material to use for default screens
DRKSCRN.MAT							// Material to use for default screens during darkness
FOGSCRN.MAT							// Material to use for default screens during fog
0									// # areas with different screens
// MAP DETAILS
NCSTAMAP.PIX						// Map pixelmap name
0.744,		0,			0			// World->map transformation matrix
0,			0,			0
0,			0.744, 		0
282.4,		114.9,		0
// ****** START OF FUNK AND GROOVE STUFF ******
START OF FUNK
!!WATER.MAT
constant
slither
harmonic
0.20,0
5,5
no fucking lighting
no animation you cunt
END OF FUNK
START OF GROOVE
&YAC0001.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.07,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
2							// max angle of rock
NEXT GROOVE
&YAC0002.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.07,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
2							// max angle of rock
NEXT GROOVE
&YAC0003.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.23							// Cycles per second
0,.08,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
8							// max angle of rock
NEXT GROOVE
&YAC0004.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.23							// Cycles per second
0,.08,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.14							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
7							// max angle of rock
NEXT GROOVE
&YAC0005.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.07,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
8							// max angle of rock
NEXT GROOVE
&YAC0006.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.23							// Cycles per second
0,.05,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
7							// max angle of rock
NEXT GROOVE
&YAC0007.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.16							// Cycles per second
0,.08,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
8							// max angle of rock
NEXT GROOVE
&YAC0008.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.15							// Cycles per second
0,.05,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
8							// max angle of rock
NEXT GROOVE
&YAC0009.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.08,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
7							// max angle of rock
NEXT GROOVE
&YAC0010.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.15							// Cycles per second
0,.08,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.17							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
8							// max angle of rock
NEXT GROOVE
&YAC0011.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0012.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0013.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.15							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0014.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.16							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.16							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0015.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.17							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0016.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.15							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.17							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0017.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.15							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0018.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.14							// Cycles per second
0,.9,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.14							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0018.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.14							// Cycles per second
0,.1,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.14							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0019.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.14							// Cycles per second
0,.12,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.14							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
11							// max angle of rock
NEXT GROOVE
&YAC0020.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.18							// Cycles per second
0,.12,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0020.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0021.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.17							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0022.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0023.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.17							// Cycles per second
0,.06,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0024.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.18							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0025.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.16							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0026.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.15,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
11							// max angle of rock
NEXT GROOVE
&YAC0027.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0028.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.16							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0029.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.16							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0030.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.18							// Cycles per second
0,.06,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock
NEXT GROOVE
&YAC0031.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.18							// Cycles per second
0,.05,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock
END OF GROOVE
// ****** START OF PEDESTRIAN STUFF ******
3
511				// Number of pedestrians
// M*^n{b"XlSWw<joo
1				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-270.099,-2.552,-90.191
point
-270.283,-2.552,-90.262
point
-270.642,-2.552,-90.240
point
-270.750,-2.552,-90.830
point
-270.106,-2.552,-94.390
reverse
// M*^n{b"XlSWw<joo
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-269.542,-2.552,-93.851
point
-269.226,-2.552,-94.602
point
-268.805,-2.552,-97.226
point
-269.183,-2.552,-97.602
reverse
// M*^n{b"XlSWw<joo
3				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-269.651,-2.552,-96.212
point
-270.692,-2.552,-96.146
point
-271.176,-2.552,-93.826
point
-270.885,-2.550,-90.653
point
-269.978,-2.552,-89.883
reverse
// M*^n{b"XlSWw<joo
3				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-283.484,-2.539,-69.888
point
-283.344,-2.539,-70.484
point
-282.090,-2.547,-71.521
point
-281.665,-2.552,-75.949
reverse
// M*^n{b"XlSWw<joo
1				// Ref num
7				// Number of instructions
2				// Initial instruction
point
-273.553,-2.552,-71.184
point
-274.416,-2.552,-70.664
point
-276.012,-2.552,-69.593
point
-282.558,-2.541,-69.943
point
-283.671,-2.538,-70.196
point
-285.278,-2.538,-71.625
reverse
// M*^n{b"XlSWw<joo
5				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-267.804,-2.552,-75.968
point
-269.345,-2.552,-74.693
point
-270.275,-2.552,-73.536
point
-272.513,-2.552,-72.074
point
-272.953,-2.552,-71.371
reverse
// M*^n{b"XlSWw<joo
8				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-283.972,-2.540,-69.747
point
-285.354,-2.540,-66.865
point
-287.150,-2.531,-66.831
point
-287.955,-2.543,-68.800
point
-288.656,-2.544,-69.908
reverse
// M*^n{b"XlSWw<joo
1				// Ref num
7				// Number of instructions
2				// Initial instruction
point
-313.628,-11.971,-26.568
point
-313.384,-11.971,-24.033
point
-312.579,-11.971,-22.773
point
-312.587,-11.971,-21.316
point
-312.863,-11.971,-19.602
point
-312.938,-11.971,-18.287
reverse
// M*^n{b"XlSWw<joo
1				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-273.343,-15.627,25.364
point
-272.440,-15.626,22.412
point
-271.392,-15.627,22.991
point
-270.066,-15.627,23.992
point
-266.453,-15.627,23.741
reverse
// Pedestrian number 10
8				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-256.908,-15.622,24.732
point
-258.387,-15.620,25.909
point
-261.283,-15.627,26.499
point
-261.930,-15.627,25.909
point
-262.724,-15.627,24.242
reverse
// Pedestrian number 11
1				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-259.411,-15.657,19.155
point
-259.250,-15.651,21.396
point
-258.661,-15.627,22.942
point
-257.584,-15.627,22.954
point
-254.533,-15.627,25.546
reverse
// Pedestrian number 12
5				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-261.806,-15.627,23.787
point
-260.932,-15.627,24.492
point
-260.637,-15.631,25.771
point
-261.612,-15.627,26.439
point
-263.339,-15.627,27.132
reverse
// Pedestrian number 13
8				// Ref num
7				// Number of instructions
3				// Initial instruction
point
-259.648,-15.627,26.691
point
-260.517,-15.634,24.927
point
-260.682,-15.634,24.331
point
-259.094,-15.652,22.352
point
-259.229,-15.655,20.294
point
-263.211,-15.657,16.713
reverse
// Pedestrian number 14
3				// Ref num
5				// Number of instructions
4				// Initial instruction
point
-258.070,-15.645,23.910
point
-258.197,-15.634,25.400
point
-258.889,-15.628,26.320
point
-260.490,-15.627,27.624
reverse
// Pedestrian number 15
8				// Ref num
7				// Number of instructions
3				// Initial instruction
point
-260.701,-15.599,47.238
point
-259.289,-15.606,46.406
point
-257.955,-15.616,46.773
point
-256.369,-15.627,46.363
point
-254.084,-15.627,46.205
point
-253.703,-15.666,46.495
reverse
// Pedestrian number 16
8				// Ref num
5				// Number of instructions
5				// Initial instruction
point
-253.063,-15.627,45.480
point
-254.008,-15.627,44.645
point
-254.846,-15.627,44.699
point
-257.222,-15.627,43.235
reverse
// Pedestrian number 17
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-255.654,-15.627,46.287
point
-253.574,-15.627,43.281
point
-246.306,-15.632,43.864
reverse
// Pedestrian number 18
3				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-254.375,-15.627,42.839
point
-252.268,-15.627,44.870
point
-251.614,-15.627,45.550
reverse
// Pedestrian number 19
1				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-277.839,-15.626,46.964
point
-278.242,-15.626,48.289
point
-278.639,-15.626,48.814
point
-279.885,-15.622,51.172
point
-280.454,-15.622,51.603
reverse
// Pedestrian number 20
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-279.755,-15.627,47.717
point
-280.472,-15.627,48.585
point
-282.667,-15.627,49.018
reverse
// Pedestrian number 21
1				// Ref num
4				// Number of instructions
3				// Initial instruction
point
-273.077,-15.595,49.765
point
-277.955,-15.626,48.609
point
-278.568,-15.627,47.785
reverse
// Pedestrian number 22
1				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-261.550,-15.627,24.535
point
-259.447,-15.657,20.859
point
-259.724,-15.657,19.231
point
-260.028,-15.657,17.513
point
-261.038,-15.657,13.342
point
-264.753,-15.657,11.104
// Pedestrian number 23
8				// Ref num
9				// Number of instructions
5				// Initial instruction
point
-266.082,-2.553,-107.261
point
-264.257,-2.552,-109.714
point
-261.583,-2.552,-110.630
point
-254.872,-2.555,-114.747
point
-251.657,-2.553,-118.503
point
-250.448,-2.553,-118.685
point
-248.889,-2.553,-119.259
point
-247.098,-2.551,-119.696
reverse
// Pedestrian number 24
1				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-246.091,-2.560,-122.113
point
-245.615,-2.566,-123.061
point
-245.679,-2.573,-124.489
point
-246.242,-2.578,-125.649
point
-247.503,-2.581,-126.887
reverse
// Pedestrian number 25
1				// Ref num
8				// Number of instructions
5				// Initial instruction
point
-266.410,998.041,-108.087
point
-265.176,997.648,-109.687
point
-264.586,-2.552,-109.784
point
-263.782,-2.552,-111.050
point
-262.242,-2.552,-111.443
point
-261.234,-2.552,-111.416
point
-256.954,-2.552,-113.230
reverse
// Pedestrian number 26
5				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-263.329,-2.552,-106.691
point
-264.653,-2.552,-106.833
point
-265.447,-2.552,-106.684
point
-265.923,-2.552,-106.075
point
-266.551,-2.552,-106.131
reverse
// Pedestrian number 27
3				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-267.692,-2.552,-101.129
point
-265.751,-2.552,-104.003
point
-265.192,-2.552,-104.223
point
-264.814,-2.552,-104.245
point
-264.475,-2.552,-103.716
reverse
// Pedestrian number 28
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-288.495,-2.544,-69.925
point
-287.502,-2.542,-70.409
point
-285.983,-2.538,-71.673
point
-282.791,-2.544,-71.385
reverse
// Pedestrian number 29
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-294.143,-2.791,-66.783
point
-295.765,-2.911,-66.707
point
-298.187,996.963,-66.782
point
-301.141,997.563,-65.627
reverse
// Pedestrian number 30
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-309.792,-4.048,-66.420
point
-310.831,-4.048,-65.068
point
-308.452,-4.048,-62.614
point
-307.596,996.743,-61.857
reverse
// Pedestrian number 31
3				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-287.373,-8.005,-48.814
point
-286.748,-8.005,-48.424
point
-285.763,-8.005,-47.190
point
-284.516,-8.005,-44.545
reverse
// Pedestrian number 32
3				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-288.702,-8.004,-37.911
point
-289.819,-8.005,-36.912
point
-291.675,-8.005,-35.896
point
-293.116,-8.132,-35.655
reverse
// Pedestrian number 33
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-316.138,-11.971,-26.853
point
-315.844,-11.971,-24.747
point
-315.337,-11.971,-23.907
point
-314.748,-11.971,-20.162
reverse
// Pedestrian number 34
8				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-280.964,-13.137,0.325
point
-279.881,-14.067,6.853
point
-279.061,-14.283,8.372
point
-278.439,-14.469,9.711
reverse
// Pedestrian number 35
1				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-281.143,-13.637,4.305
point
-279.878,-13.759,4.398
point
-277.683,-14.024,5.166
point
-277.137,-14.175,6.063
point
-276.633,-14.232,6.556
reverse
// Pedestrian number 36
1				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-279.125,-13.614,2.765
point
-278.599,-13.753,3.557
point
-278.165,-13.871,4.247
point
-278.714,-14.200,7.385
point
-279.385,-14.220,7.974
reverse
// Pedestrian number 37
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-276.482,-14.300,7.130
point
-276.218,-14.378,7.742
point
-276.264,-14.536,9.064
point
-276.652,-15.143,13.609
reverse
// Pedestrian number 38
3				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-275.002,-15.619,19.806
point
-274.496,-15.618,19.663
point
-268.392,-15.627,22.206
reverse
// Pedestrian number 39
3				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-272.264,-15.588,17.210
point
-275.058,-15.622,20.682
point
-274.902,-15.625,21.666
point
-278.184,-15.627,30.167
reverse
// Pedestrian number 40
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-277.417,-15.627,29.835
point
-279.133,-15.627,30.441
point
-280.492,-15.627,30.747
reverse
// Pedestrian number 41
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-282.975,-15.627,28.137
point
-283.564,-15.627,28.642
point
-284.591,-15.627,31.486
reverse
// Pedestrian number 42
5				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-280.448,-15.627,34.628
point
-282.453,-15.627,32.370
point
-284.006,-15.627,31.417
point
-284.666,-15.627,28.681
reverse
// Pedestrian number 43
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-281.126,-15.627,31.345
point
-281.238,-15.627,31.978
point
-283.168,-15.627,35.341
reverse
// Pedestrian number 44
8				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-285.095,-15.627,28.814
point
-286.271,-15.627,29.022
point
-287.036,-15.627,29.290
point
-287.996,-15.627,29.336
reverse
// Pedestrian number 45
3				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-289.209,-15.627,30.392
point
-288.316,-15.627,34.406
point
-288.427,-15.627,35.933
point
-284.900,-15.627,51.411
reverse
// Pedestrian number 46
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-288.387,-15.627,48.459
point
-287.352,-15.627,49.820
point
-276.078,-15.617,50.597
reverse
// Pedestrian number 47
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-59.975,-14.067,-138.803
point
-60.505,-14.035,-138.556
point
-61.242,-13.918,-136.903
point
-62.150,-13.901,-136.874
reverse
// Pedestrian number 48
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-62.775,-13.901,-136.216
point
-60.787,-13.911,-134.451
point
-57.955,-14.207,-135.354
reverse
// Pedestrian number 49
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-56.289,-14.327,-137.813
point
-58.024,-14.202,-137.874
point
-60.730,-13.909,-134.134
point
-61.790,-13.901,-132.943
reverse
// Pedestrian number 50
1				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-65.611,-13.901,-132.644
point
-64.250,-13.901,-133.070
point
-62.385,-13.901,-136.494
point
-62.564,-13.916,-137.158
point
-66.376,-13.713,-136.860
reverse
// Pedestrian number 51
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-69.041,-13.532,-139.787
point
-67.521,-13.635,-139.776
point
-62.387,-13.925,-137.424
point
-62.022,-13.949,-137.335
reverse
// Pedestrian number 52
13				// Ref num
7				// Number of instructions
2				// Initial instruction
point
-75.245,-13.901,-133.507
point
-73.024,-13.906,-133.906
point
-71.821,-13.901,-133.901
point
-70.394,-13.901,-134.566
point
-61.138,-13.915,-136.228
point
-58.166,-14.192,-136.758
reverse
// Pedestrian number 53
13				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-97.076,-13.901,-125.689
point
-99.376,-13.901,-124.838
point
-106.368,-13.901,-123.246
point
-109.898,-13.901,-125.363
point
-111.093,-13.901,-125.195
reverse
// Pedestrian number 54
13				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-112.755,-13.901,-121.814
point
-111.085,-13.901,-122.181
point
-109.744,-13.901,-122.466
point
-106.911,-13.901,-125.959
reverse
// Pedestrian number 55
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-175.042,-17.667,-100.004
point
-179.117,-17.667,-100.649
point
-181.253,-17.667,-99.148
point
-181.745,-17.667,-95.709
reverse
// Pedestrian number 56
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-179.293,-17.667,-97.039
point
-176.732,-17.667,-98.838
point
-175.654,-17.667,-99.802
point
-174.310,-17.667,-100.624
reverse
// Pedestrian number 57
13				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-170.557,-16.453,-106.909
point
-174.975,-17.426,-103.830
point
-176.094,-17.667,-102.846
point
-177.133,-17.667,-101.969
point
-178.138,-17.667,-101.345
reverse
// Pedestrian number 58
13				// Ref num
7				// Number of instructions
4				// Initial instruction
point
-203.787,-17.667,-91.459
point
-207.159,-17.667,-88.463
point
-209.744,-17.667,-88.486
point
-211.957,-17.667,-88.351
point
-213.212,-17.667,-88.337
point
-214.288,-17.667,-91.441
reverse
// Pedestrian number 59
3				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-214.358,-17.667,-88.482
point
-212.875,-17.667,-88.949
point
-210.600,-17.667,-88.317
point
-208.806,-17.667,-89.242
point
-207.125,-17.667,-91.163
reverse
// Pedestrian number 60
5				// Ref num
5				// Number of instructions
4				// Initial instruction
point
-244.356,-17.667,-77.863
point
-245.862,-17.667,-77.901
point
-248.054,-17.667,-78.765
point
-252.012,-17.667,-78.072
reverse
// Pedestrian number 61
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-250.827,-17.667,-75.431
point
-250.251,-17.667,-75.935
point
-247.056,-17.667,-80.030
reverse
// Pedestrian number 62
13				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-261.819,-17.667,-73.050
point
-260.784,-17.667,-73.119
point
-259.624,-17.667,-71.430
point
-257.921,-17.667,-71.828
point
-254.443,-17.667,-72.824
reverse
// Pedestrian number 63
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-261.064,-17.667,-70.032
point
-260.448,-17.667,-70.677
point
-259.825,-17.667,-74.013
reverse
// Pedestrian number 64
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-265.666,-15.657,7.363
point
-265.003,-15.657,8.315
point
-262.073,-15.657,10.449
reverse
// Pedestrian number 65
13				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-264.227,-15.657,12.830
point
-264.807,-15.657,10.788
point
-262.833,-15.657,7.393
point
-263.603,-15.657,2.374
reverse
// Pedestrian number 66
14				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-266.605,-15.657,0.758
point
-266.129,-15.657,3.554
point
-264.564,-15.657,9.533
point
-263.000,-15.657,11.069
point
-261.491,-15.657,11.978
reverse
// Pedestrian number 67
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-262.447,-15.657,8.891
point
-262.242,-15.657,9.640
point
-262.573,-15.657,10.781
point
-263.959,-15.657,13.668
reverse
// Pedestrian number 68
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-259.638,-15.657,18.489
point
-261.348,-15.657,12.474
point
-264.456,-15.657,10.126
point
-264.992,-15.657,9.778
reverse
// Pedestrian number 69
13				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-263.145,-15.657,5.505
point
-263.338,-15.657,6.703
point
-262.725,-15.657,8.248
point
-261.501,-15.657,11.636
reverse
// Pedestrian number 70
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-257.690,-15.632,24.742
point
-257.953,-15.627,26.535
point
-257.212,-15.627,28.230
point
-259.492,-15.627,31.657
reverse
// Pedestrian number 71
13				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-256.166,-15.627,33.743
point
-256.624,-15.627,33.108
point
-257.324,-15.627,29.408
point
-257.476,-15.627,25.473
point
-255.290,-15.627,22.277
reverse
// Pedestrian number 72
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-257.372,-15.627,22.881
point
-256.107,-15.627,22.939
point
-250.981,-15.627,24.575
reverse
// Pedestrian number 73
14				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-252.187,-15.627,28.373
point
-252.575,-15.627,27.283
point
-251.458,-15.627,23.884
reverse
// Pedestrian number 74
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-261.113,-15.628,25.080
point
-261.443,-15.630,22.852
point
-262.229,-15.657,20.201
point
-259.412,-15.657,19.456
reverse
// Pedestrian number 75
17				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-245.970,-15.627,39.348
point
-249.793,-15.627,39.942
point
-250.178,-15.626,41.146
reverse
// Pedestrian number 76
8				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-251.313,-15.627,42.251
point
-250.581,-15.627,41.983
point
-249.967,-15.627,41.610
point
-246.073,-15.632,42.138
point
-245.368,-15.627,39.850
reverse
// Pedestrian number 77
12				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-244.877,-15.635,43.594
point
-247.082,-15.631,43.610
point
-248.305,-15.628,42.389
point
-251.868,-15.627,23.453
reverse
// Pedestrian number 78
8				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-254.490,-15.627,41.847
point
-257.747,-15.627,39.460
point
-258.167,-15.627,37.313
point
-258.321,-15.654,23.099
reverse
// Pedestrian number 79
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-261.943,-15.627,25.544
point
-263.120,-15.627,26.106
point
-267.710,-15.627,26.051
reverse
// Pedestrian number 80
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-268.220,-15.627,25.990
point
-268.947,-15.627,25.494
point
-269.505,-15.627,20.972
reverse
// Pedestrian number 81
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-280.302,-15.627,27.697
point
-281.003,-15.627,27.992
point
-282.525,-15.627,38.145
reverse
// Pedestrian number 82
3				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-279.237,-15.627,47.436
point
-279.147,-15.627,46.697
point
-280.958,-15.627,32.440
reverse
// Pedestrian number 83
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-283.974,-15.627,31.730
point
-283.756,-15.627,32.563
point
-283.491,-15.627,33.863
point
-278.829,-15.627,47.333
reverse
// Pedestrian number 84
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-278.011,-15.627,46.284
point
-278.348,-15.627,45.160
point
-281.207,-15.627,44.482
reverse
// Pedestrian number 85
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-278.334,-15.708,52.126
point
-276.456,-15.917,53.527
point
-276.025,-16.174,56.155
point
-277.909,-16.318,58.276
reverse
// Pedestrian number 86
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-272.600,-18.908,82.287
point
-269.042,-18.912,86.156
point
-269.557,-18.914,89.312
point
-270.740,-18.916,92.449
reverse
// Pedestrian number 87
13				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-267.411,-18.915,94.181
point
-269.126,-18.915,92.989
point
-270.514,-18.916,93.653
point
-274.046,-18.916,92.297
point
-290.575,-18.915,96.467
reverse
// Pedestrian number 88
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-290.535,-18.915,97.563
point
-274.153,-18.915,94.451
point
-268.527,-18.915,89.919
reverse
// Pedestrian number 89
13				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-267.077,-18.915,92.468
point
-267.702,-18.915,91.826
point
-268.247,-18.915,90.436
point
-270.731,-18.914,89.718
reverse
// Pedestrian number 90
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-266.066,-18.913,106.289
point
-269.661,-18.914,94.163
point
-267.923,-18.915,90.522
reverse
// Pedestrian number 91
17				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-246.888,-18.915,85.598
point
-246.557,-18.915,88.305
point
-246.116,-18.915,89.756
reverse
// Pedestrian number 92
5				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-242.658,-18.915,100.699
point
-242.385,-18.915,96.290
point
-244.021,-18.915,89.483
point
-244.344,-18.914,85.812
reverse
// Pedestrian number 93
17				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-224.432,-18.915,81.168
point
-225.555,-18.916,82.652
point
-228.229,-18.916,84.140
reverse
// Pedestrian number 94
12				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-224.098,-18.916,82.961
point
-224.899,-18.916,82.519
point
-225.427,-18.916,82.805
point
-232.529,-18.916,82.657
reverse
// Pedestrian number 95
13				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-224.172,-18.916,82.005
point
-243.623,-18.915,87.028
point
-244.561,-18.915,86.304
point
-245.521,-18.913,82.788
point
-248.219,-18.911,80.794
reverse
// Pedestrian number 96
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-246.298,-18.910,78.252
point
-246.004,-18.911,79.590
point
-247.313,-18.916,88.406
reverse
// Pedestrian number 97
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-245.505,-18.915,92.686
point
-245.012,-18.915,94.175
point
-244.207,-18.916,100.898
reverse
// Pedestrian number 98
8				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-221.401,-18.916,95.766
point
-222.908,-18.916,95.051
point
-227.663,-18.916,95.340
point
-230.000,-18.916,96.978
point
-244.157,-18.915,98.220
reverse
// Pedestrian number 99
3				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-238.820,-18.915,99.952
point
-241.360,-18.915,98.651
point
-244.445,-18.915,96.720
point
-244.997,-18.915,95.096
reverse
// Pedestrian number 100
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-242.120,-18.915,97.469
point
-244.093,-18.915,98.859
point
-245.851,-18.916,101.360
point
-287.253,-18.914,110.686
reverse
// Pedestrian number 101
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-245.032,-18.916,101.345
point
-244.585,-18.915,98.971
point
-242.312,-18.914,96.801
reverse
// Pedestrian number 102
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-251.461,-18.916,100.610
reverse
// Pedestrian number 103
129				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-253.398,-15.627,45.697
reverse
// Pedestrian number 104
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-257.272,-15.627,42.491
reverse
// Pedestrian number 105
129				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-256.284,-15.627,33.307
reverse
// Pedestrian number 106
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-254.620,-15.627,22.531
reverse
// Pedestrian number 107
130				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-250.575,-15.627,41.531
reverse
// Pedestrian number 108
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-254.042,-17.667,-73.114
reverse
// Pedestrian number 109
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-252.533,-17.667,-77.667
reverse
// Pedestrian number 110
129				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-226.823,-17.667,-91.019
reverse
// Pedestrian number 111
129				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-27.743,-15.561,-44.497
reverse
// Pedestrian number 112
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-26.788,-15.561,-45.238
reverse
// Pedestrian number 113
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-25.847,-15.561,-45.968
reverse
// Pedestrian number 114
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-82.993,-13.028,-48.234
reverse
// Pedestrian number 115
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-129.713,-18.645,-45.533
reverse
// Pedestrian number 116
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-127.573,-18.655,-46.141
reverse
// Pedestrian number 117
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-125.686,-18.634,-45.420
reverse
// Pedestrian number 118
129				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-138.923,-18.725,-58.154
reverse
// Pedestrian number 119
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-141.695,-18.737,-59.375
reverse
// Pedestrian number 120
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-145.946,-18.665,-48.496
reverse
// Pedestrian number 121
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-145.198,-18.670,-46.779
reverse
// Pedestrian number 122
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-139.581,-16.166,-39.660
reverse
// Pedestrian number 123
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-137.255,-14.010,-30.646
reverse
// Pedestrian number 124
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-136.103,-13.938,-30.522
reverse
// Pedestrian number 125
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-132.813,-9.082,-50.595
reverse
// Pedestrian number 126
130				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-133.365,-9.082,-50.436
reverse
// Pedestrian number 127
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-264.404,-2.552,-104.048
reverse
// Pedestrian number 128
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-264.253,-2.552,-104.536
reverse
// Pedestrian number 129
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-268.549,-2.552,-98.537
reverse
// Pedestrian number 130
1				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-154.797,-8.795,-37.416
point
-155.758,-9.008,-39.093
point
-155.682,-9.077,-40.053
point
-146.436,-9.077,-42.540
reverse
// Pedestrian number 131
3				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-146.536,-9.077,-45.589
point
-148.877,-9.077,-44.903
point
-149.937,-9.077,-44.138
point
-150.793,-9.077,-41.614
reverse
// Pedestrian number 132
13				// Ref num
4				// Number of instructions
1				// Initial instruction
point
-144.951,-8.822,-45.084
point
-146.179,-9.077,-44.767
point
-147.609,-9.077,-45.393
reverse
// Pedestrian number 133
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-135.266,-8.919,-46.250
point
-134.767,-9.089,-46.979
point
-132.236,-9.084,-46.497
point
-121.404,-9.078,-49.433
reverse
// Pedestrian number 134
13				// Ref num
7				// Number of instructions
4				// Initial instruction
point
-132.587,-9.081,-50.555
point
-132.074,-8.967,-50.100
point
-131.552,-9.077,-49.757
point
-128.024,-9.077,-49.940
point
-124.245,-9.078,-48.738
point
-122.163,-9.338,-46.182
reverse
// Pedestrian number 135
14				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-125.546,-9.934,-40.050
point
-123.504,-9.673,-41.952
point
-124.452,-9.143,-47.802
point
-121.549,-9.096,-49.138
reverse
// Pedestrian number 136
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-127.186,-9.077,-48.003
point
-128.893,-9.077,-48.697
point
-134.625,-9.081,-48.200
point
-136.083,-8.818,-47.566
reverse
// Pedestrian number 137
8				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-134.164,-9.096,-46.011
point
-133.139,-9.080,-47.536
point
-131.164,-9.077,-48.998
point
-125.868,-9.078,-51.521
reverse
// Pedestrian number 138
14				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-23.454,-15.561,-49.659
point
-25.541,-15.561,-45.735
point
-28.159,-15.561,-43.634
point
-37.209,-15.561,-46.669
reverse
// Pedestrian number 139
3				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-31.746,-15.561,-44.197
point
-29.092,-15.561,-44.828
point
-23.428,-15.561,-47.823
reverse
// Pedestrian number 140
1				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-23.237,-15.561,-51.567
point
-24.452,-15.560,-51.263
point
-27.403,-15.561,-49.276
point
-29.418,-15.561,-46.721
point
-28.054,-15.561,-43.551
reverse
// Pedestrian number 141
5				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-24.211,-15.561,-46.619
point
-25.772,-15.561,-47.198
point
-26.246,-15.561,-49.840
point
-24.516,-15.561,-50.401
reverse
// Pedestrian number 142
1				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-274.111,-15.600,47.219
point
-273.015,-15.599,47.834
point
-271.303,-15.599,49.503
point
-269.993,-15.599,49.251
reverse
// Pedestrian number 143
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-275.307,-15.612,50.411
point
-274.073,-15.604,50.194
point
-267.833,-15.599,48.906
reverse
// Pedestrian number 144
3				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-268.077,-15.599,45.919
point
-270.539,-15.599,46.626
point
-271.840,-15.599,47.562
point
-274.421,-15.604,47.757
point
-276.369,-15.619,47.718
reverse
// Pedestrian number 145
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-266.716,-15.599,48.695
point
-263.974,-15.599,47.846
point
-261.122,-15.599,44.348
reverse
// Pedestrian number 146
29				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-273.751,-15.599,47.079
point
-271.455,-15.599,47.075
point
-270.293,-15.599,48.141
point
-267.297,-15.599,47.593
point
-264.722,-15.599,48.203
reverse
// Pedestrian number 147
3				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-262.696,-15.599,44.762
point
-257.263,-15.627,43.881
point
-253.610,-15.627,42.867
reverse
// Pedestrian number 148
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-282.000,-15.625,51.855
point
-283.612,-15.627,50.231
point
-285.220,-15.627,48.205
point
-290.883,-15.627,37.644
reverse
// Pedestrian number 149
1				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-269.156,-15.599,46.071
point
-265.497,-15.599,45.847
point
-263.858,-15.599,45.177
point
-256.357,-15.627,46.578
reverse
// Pedestrian number 150
3				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-256.138,-15.649,46.817
point
-255.963,-15.783,47.965
point
-255.393,-15.998,49.747
point
-252.229,-16.263,52.093
reverse
// Pedestrian number 151
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-240.193,-14.789,40.689
point
-237.698,-14.359,39.170
point
-236.859,-13.820,34.927
reverse
// Pedestrian number 152
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-244.855,-15.619,40.005
point
-244.408,-15.513,39.803
point
-242.112,-14.883,38.503
point
-239.603,-14.414,36.895
reverse
// Pedestrian number 153
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-235.848,-13.988,37.950
point
-232.211,-13.012,35.192
point
-229.563,-12.513,32.817
reverse
// Pedestrian number 154
1				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-230.596,-12.208,29.479
point
-228.883,-11.868,28.658
point
-225.417,-11.308,27.739
point
-223.554,-11.037,25.996
reverse
// Pedestrian number 155
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-215.914,-9.122,11.075
point
-215.358,-9.078,10.006
point
-215.350,-9.078,9.436
point
-217.107,-9.078,5.180
reverse
// Pedestrian number 156
14				// Ref num
7				// Number of instructions
2				// Initial instruction
point
-216.712,-9.078,9.149
point
-215.622,-9.078,5.559
point
-215.178,-9.078,3.462
point
-215.443,-9.078,2.543
point
-214.628,-9.078,1.286
point
-215.556,-9.078,-1.573
reverse
// Pedestrian number 157
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-220.365,-9.446,14.723
point
-219.623,-9.293,12.993
point
-219.052,-9.222,12.157
point
-218.892,-9.163,10.928
reverse
// Pedestrian number 158
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-217.898,-9.078,9.322
point
-217.505,-9.078,6.830
point
-216.861,-9.078,4.397
point
-216.390,-9.078,1.667
reverse
// Pedestrian number 159
13				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-215.150,-9.078,8.818
point
-215.007,-9.078,7.951
point
-214.495,-9.078,7.136
point
-214.368,-9.078,6.415
point
-213.805,-9.078,4.554
reverse
// Pedestrian number 160
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-218.536,-9.103,9.741
point
-217.609,-9.078,7.851
point
-216.308,-9.078,5.552
point
-216.740,-9.078,4.223
reverse
// Pedestrian number 161
8				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-206.193,-8.044,-8.222
point
-205.343,-7.665,-8.595
point
-204.631,-7.562,-8.476
point
-204.049,-7.140,-8.757
point
-203.320,-6.748,-8.939
reverse
// Pedestrian number 162
5				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-204.299,-7.663,-8.118
point
-203.816,-7.387,-8.357
point
-203.330,-7.145,-8.425
point
-202.910,-7.249,-8.038
point
-201.931,-7.245,-7.347
reverse
// Pedestrian number 163
1				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-206.737,-8.135,-8.164
point
-205.643,-7.958,-7.995
point
-203.866,-7.672,-7.739
point
-203.208,-7.562,-7.607
point
-201.235,-7.058,-6.994
reverse
// Pedestrian number 164
8				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-197.295,-5.839,-1.871
point
-194.701,-5.332,-0.287
point
-193.775,-5.328,0.480
point
-193.307,-5.328,0.595
point
-192.870,-5.328,1.078
reverse
// Pedestrian number 165
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-188.596,-5.325,0.546
point
-187.717,-5.327,1.713
point
-186.019,-5.427,3.168
point
-184.273,-5.428,3.262
reverse
// Pedestrian number 166
8				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-190.226,-5.270,3.747
point
-190.782,-4.797,3.803
point
-191.406,-4.735,3.288
point
-191.612,-5.327,2.311
reverse
// Pedestrian number 167
1				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-188.997,-5.362,4.469
point
-186.993,-5.407,4.074
point
-186.415,-5.427,3.910
point
-183.962,-5.428,3.497
point
-181.176,-5.421,3.071
reverse
// Pedestrian number 168
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-184.261,-5.428,6.319
point
-185.743,-5.428,5.912
point
-187.377,-5.421,5.567
reverse
// Pedestrian number 169
8				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-185.924,-5.427,2.800
point
-185.395,-5.428,4.132
point
-183.905,-5.428,5.366
point
-181.818,-5.423,6.072
point
-179.124,-5.425,5.360
reverse
// Pedestrian number 170
1				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-174.318,-5.442,-0.457
point
-174.188,-5.446,-0.956
point
-174.107,-5.498,-4.044
point
-175.052,-5.851,-7.078
reverse
// Pedestrian number 171
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-177.642,-5.713,-5.465
point
-177.881,-5.840,-6.393
point
-178.966,-6.300,-8.660
reverse
// Pedestrian number 172
8				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-177.301,-5.594,-4.567
point
-176.429,-5.872,-6.928
point
-176.337,-6.116,-8.542
point
-176.405,-6.376,-10.122
reverse
// Pedestrian number 173
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-180.871,-8.504,-21.449
point
-180.128,-8.799,-25.143
point
-179.896,-8.854,-25.811
point
-178.526,-9.042,-27.987
reverse
// Pedestrian number 174
29				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-178.132,-9.078,-28.560
point
-175.555,-9.078,-29.629
point
-173.209,-9.078,-30.268
point
-170.662,-9.078,-32.453
reverse
// Pedestrian number 175
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-170.287,-9.078,-32.745
point
-169.972,-9.078,-34.458
point
-168.781,-9.078,-35.482
point
-164.568,-9.078,-36.741
reverse
// Pedestrian number 176
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-166.497,-9.078,-39.067
point
-164.967,-9.078,-39.826
point
-163.602,-9.078,-40.411
point
-158.816,-9.078,-39.141
reverse
// Pedestrian number 177
3				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-93.141,-10.699,-46.567
point
-90.667,-11.282,-46.195
point
-88.743,-11.763,-45.902
point
-86.841,-12.221,-46.212
point
-83.983,-12.934,-45.274
reverse
// Pedestrian number 178
8				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-79.598,-13.281,-47.890
point
-76.790,-13.067,-46.072
point
-76.641,-13.072,-45.976
point
-74.152,-13.200,-44.051
reverse
// Pedestrian number 179
5				// Ref num
7				// Number of instructions
6				// Initial instruction
point
-63.452,-15.005,-45.914
point
-59.726,-15.561,-45.200
point
-56.465,-15.561,-44.719
point
-55.502,-15.561,-44.850
point
-54.827,-15.561,-44.541
point
-54.827,-15.561,-44.541
reverse
// Pedestrian number 180
8				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-50.902,-15.561,-41.216
point
-48.469,-15.561,-41.442
point
-46.856,-15.561,-41.425
point
-44.620,-15.561,-41.528
reverse
// Pedestrian number 181
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-51.913,-15.561,-41.452
point
-54.157,-15.561,-41.768
point
-56.903,-15.561,-42.016
reverse
// Pedestrian number 182
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-58.522,-15.561,-45.328
point
-57.228,-15.561,-44.640
point
-53.892,-15.561,-44.153
point
-52.330,-15.561,-44.363
reverse
// Pedestrian number 183
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-60.416,-15.465,-45.270
point
-61.681,-15.280,-45.454
point
-64.002,-14.903,-45.808
point
-65.282,-14.658,-46.072
reverse
// Pedestrian number 184
29				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-33.680,-15.561,-48.367
point
-29.151,-15.561,-47.717
point
-23.574,-15.561,-49.720
reverse
// Pedestrian number 185
29				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-28.036,-15.561,-52.219
point
-29.046,-15.561,-51.305
point
-30.114,-15.561,-50.544
point
-31.076,-15.561,-50.004
reverse
// Pedestrian number 186
29				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-27.654,-15.561,-47.388
point
-28.060,-15.561,-45.289
point
-28.902,-15.561,-43.269
reverse
// Pedestrian number 187
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-18.146,-15.561,-61.368
point
-16.833,-15.561,-64.439
point
-15.727,-15.547,-68.677
reverse
// Pedestrian number 188
3				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-18.611,-15.561,-60.084
point
-18.493,-15.561,-61.007
point
-15.497,-15.515,-70.280
reverse
// Pedestrian number 189
1				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-18.380,-15.539,-69.591
point
-18.681,-15.518,-68.230
point
-19.311,-15.562,-66.305
point
-19.974,-15.561,-64.060
point
-20.299,-15.561,-63.560
reverse
// Pedestrian number 190
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-18.388,-15.521,-70.426
point
-17.230,-15.495,-71.950
point
-15.033,-15.495,-73.694
point
-15.044,-15.495,-75.395
reverse
// Pedestrian number 191
3				// Ref num
7				// Number of instructions
2				// Initial instruction
point
-14.173,-14.288,-115.232
point
-12.458,-14.162,-117.244
point
-11.531,-14.109,-118.322
point
-11.367,-14.010,-120.702
point
-11.328,-14.015,-120.886
point
-11.564,-14.210,-121.700
reverse
// Pedestrian number 192
13				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-11.554,-14.326,-114.336
point
-12.126,-14.253,-115.646
point
-13.671,-14.128,-118.100
point
-13.738,-14.154,-118.514
point
-14.235,-14.340,-120.942
reverse
// Pedestrian number 193
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-14.431,-14.362,-114.006
point
-14.209,-14.161,-117.414
point
-14.245,-14.245,-119.162
reverse
// Pedestrian number 194
29				// Ref num
8				// Number of instructions
3				// Initial instruction
point
-14.019,-14.830,-124.818
point
-13.509,-15.444,-127.889
point
-11.893,-15.631,-131.178
point
-12.495,-15.631,-131.975
point
-12.980,-15.631,-133.519
point
-14.167,-15.631,-134.831
point
-15.643,-15.631,-136.253
reverse
// Pedestrian number 195
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-15.503,-15.631,-132.103
point
-11.967,-15.594,-130.452
point
-11.549,-15.528,-129.287
reverse
// Pedestrian number 196
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-11.584,-15.483,-128.504
point
-11.700,-15.576,-130.153
point
-12.536,-15.631,-132.708
reverse
// Pedestrian number 197
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-17.200,-15.631,-133.775
point
-19.067,-15.629,-134.677
point
-21.511,-15.585,-137.659
reverse
// Pedestrian number 198
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-30.188,-15.562,-137.478
point
-33.425,-15.562,-137.417
point
-38.063,-15.555,-137.825
reverse
// Pedestrian number 199
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-37.519,-15.562,-134.767
point
-41.532,-15.437,-137.507
point
-42.737,-15.345,-137.747
reverse
// Pedestrian number 2
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-52.536,-14.601,-134.892
point
-54.431,-14.461,-134.946
point
-58.037,-14.201,-137.413
point
-59.248,-14.119,-138.455
reverse
// Pedestrian number 2
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-61.996,-13.901,-136.617
point
-61.204,-13.916,-136.545
point
-58.575,-14.148,-134.805
reverse
// Pedestrian number 2
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-61.172,-13.901,-133.827
point
-62.598,-13.901,-135.916
point
-64.597,-13.901,-135.750
reverse
// Pedestrian number 2
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-78.384,-13.021,-140.037
point
-82.901,-12.812,-137.255
point
-86.013,-12.670,-137.159
reverse
// Pedestrian number 2
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-89.978,-12.488,-137.208
point
-92.780,-12.357,-137.667
point
-98.558,-12.093,-137.310
reverse
// Pedestrian number 2
3				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-164.897,-9.029,-141.292
point
-168.279,-8.767,-140.352
point
-169.487,-8.668,-139.876
point
-171.154,-8.530,-139.352
reverse
// Pedestrian number 2
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-167.121,-8.860,-137.879
point
-168.014,-8.788,-137.578
point
-169.239,-8.690,-136.999
reverse
// Pedestrian number 2
1				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-174.566,-8.230,-136.773
point
-175.795,-8.117,-135.328
point
-176.785,-8.026,-134.361
point
-177.411,-7.967,-133.357
point
-178.164,-7.895,-132.071
reverse
// Pedestrian number 2
5				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-175.648,-8.132,-130.543
point
-176.472,-8.055,-129.160
point
-176.824,-8.022,-127.301
point
-177.463,-7.962,-123.708
reverse
// Pedestrian number 2
8				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-179.881,-7.728,-118.107
point
-182.502,-7.468,-115.060
point
-183.518,-7.358,-113.824
point
-183.699,-6.793,-112.925
reverse
// Pedestrian number 2~
29				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-188.039,-6.870,-114.709
point
-190.069,-6.641,-113.765
point
-191.402,-6.484,-113.622
point
-193.168,-6.279,-113.335
reverse
// Pedestrian number 2~
8				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-199.733,-5.456,-110.360
point
-199.119,-5.069,-109.733
point
-198.364,-4.985,-109.470
point
-196.892,-5.166,-109.341
point
-195.723,-5.966,-109.956
reverse
// Pedestrian number 2~
5				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-201.463,-5.228,-110.850
point
-199.630,-5.469,-110.555
point
-198.233,-5.649,-110.207
point
-196.739,-5.838,-110.503
point
-196.414,-5.879,-110.232
reverse
// Pedestrian number 2~
5				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-195.802,-5.956,-113.173
point
-198.498,-5.616,-113.263
point
-200.035,-5.416,-113.415
point
-201.760,-5.191,-113.866
point
-203.892,-4.901,-114.969
reverse
// Pedestrian number 2~
1				// Ref num
7				// Number of instructions
4				// Initial instruction
point
-203.170,-4.999,-111.287
point
-204.126,-4.867,-112.350
point
-205.630,-4.660,-112.790
point
-206.713,-4.508,-113.248
point
-208.206,-4.297,-114.389
point
-209.045,-4.174,-114.956
reverse
// Pedestrian number 2~
1				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-208.288,-4.285,-118.682
point
-209.033,-4.169,-119.281
point
-209.737,-4.050,-120.532
point
-210.064,-3.995,-121.123
point
-210.623,-3.889,-123.040
reverse
// Pedestrian number 2~
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-214.008,-3.465,-124.467
point
-213.698,-3.484,-122.753
point
-213.185,-3.555,-121.988
point
-213.022,-3.582,-121.021
reverse
// Pedestrian number 2~
29				// Ref num
9				// Number of instructions
5				// Initial instruction
point
-210.892,-3.885,-123.878
point
-212.017,-3.744,-126.687
point
-211.713,-3.774,-127.972
point
-212.090,-3.720,-128.330
point
-212.071,-3.717,-128.962
point
-211.915,-3.737,-130.228
point
-212.109,-3.715,-131.658
point
-212.803,-3.621,-134.944
reverse
// Pedestrian number 2~
13				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-214.005,-3.464,-137.958
point
-214.545,-3.400,-139.444
point
-215.451,-3.325,-141.219
point
-215.887,-3.274,-141.797
point
-216.623,-3.208,-143.140
reverse
// Pedestrian number 2~
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-220.808,-2.963,-142.879
point
-220.916,-2.427,-142.407
point
-220.608,-2.227,-141.860
reverse
// Pedestrian number 2}
13				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-217.864,-3.159,-139.088
point
-217.953,-2.966,-138.941
point
-217.926,-2.739,-138.378
point
-217.757,-2.537,-137.481
reverse
// Pedestrian number 2}
8				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-218.020,-3.154,-139.890
point
-218.784,-3.133,-141.209
point
-219.332,-3.118,-142.147
point
-220.767,-3.087,-143.468
point
-222.002,-3.059,-144.447
reverse
// Pedestrian number 2}
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-221.117,-3.071,-147.339
point
-221.770,-3.063,-147.743
point
-223.903,-3.018,-148.851
point
-226.591,-2.962,-150.613
reverse
// Pedestrian number 2}
5				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-230.681,-2.863,-152.229
point
-229.772,-2.879,-151.728
point
-228.778,-2.899,-151.598
point
-227.521,-2.465,-151.751
reverse
// Pedestrian number 2}
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-231.665,-2.845,-152.564
point
-233.043,-2.856,-152.639
point
-234.060,-2.806,-152.317
reverse
// Pedestrian number 2}
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-235.199,-2.734,-148.686
point
-235.321,-2.719,-148.387
point
-235.541,-2.713,-147.544
reverse
// Pedestrian number 2}
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-237.421,-2.731,-150.636
point
-237.956,-2.717,-150.020
point
-239.148,-2.700,-147.260
reverse
// Pedestrian number 2}
3				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-239.394,-2.695,-146.363
point
-238.514,-2.706,-148.017
point
-238.122,-2.711,-148.836
point
-237.989,-2.714,-149.518
reverse
// Pedestrian number 2}
12				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-234.193,-2.780,-149.292
point
-234.523,-2.762,-149.024
point
-235.733,-2.741,-147.978
point
-236.225,-2.705,-146.210
reverse
// Pedestrian number 2}
3				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-233.743,-2.796,-149.489
point
-233.018,-2.828,-149.670
point
-231.980,-2.846,-149.519
reverse
// Pedestrian number 2|
1				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-237.762,-2.682,-142.292
point
-238.988,-2.665,-139.503
point
-240.981,-2.654,-138.347
point
-243.640,-2.635,-136.066
point
-244.050,-2.630,-135.209
reverse
// Pedestrian number 2|
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-242.575,-2.650,-138.481
point
-241.791,-2.662,-139.986
point
-240.409,-2.682,-144.017
reverse
// Pedestrian number 2|
5				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-235.696,-2.711,-147.185
point
-236.687,-2.708,-146.130
point
-236.887,-2.693,-144.744
point
-237.605,-2.685,-142.872
reverse
// Pedestrian number 2|
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-237.685,-2.683,-142.634
point
-238.632,-2.674,-141.185
point
-240.579,-2.640,-135.349
reverse
// Pedestrian number 2|
29				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-241.063,-2.634,-134.364
point
-241.720,-2.626,-133.080
point
-242.694,-2.611,-130.614
point
-243.371,-2.601,-128.796
reverse
// Pedestrian number 2|
29				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-246.510,-2.595,-129.308
point
-246.510,-2.595,-129.308
point
-241.963,-2.618,-131.668
point
-241.075,-1.949,-132.197
reverse
// Pedestrian number 2|
17				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-246.760,-2.592,-128.747
point
-247.714,-2.576,-125.882
point
-248.654,-2.565,-124.034
reverse
// Pedestrian number 2|
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-250.127,-2.552,-120.536
point
-250.502,-2.552,-119.241
point
-251.703,-2.552,-118.814
reverse
// Pedestrian number 2|
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-252.670,-2.555,-115.362
point
-255.373,-2.552,-114.200
point
-256.381,-2.552,-113.722
reverse
// Pedestrian number 2|
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-257.974,-2.552,-116.086
point
-258.710,-2.553,-113.521
point
-258.878,-2.552,-111.778
reverse
// Pedestrian number 2{
17				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-259.951,-2.552,-111.080
point
-261.131,-2.552,-110.314
point
-262.437,-2.552,-108.285
point
-263.675,-2.552,-105.560
reverse
// Pedestrian number 2{
14				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-249.319,-2.552,-113.961
point
-248.765,-2.556,-115.149
point
-248.531,-2.556,-116.031
reverse
// Pedestrian number 2{
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-251.094,-2.553,-118.841
point
-251.966,-2.553,-118.639
point
-254.392,-2.553,-114.695
reverse
// Pedestrian number 2{
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-252.938,-2.553,-118.360
point
-254.900,-2.553,-117.529
point
-255.599,-2.553,-117.270
point
-256.842,-2.552,-116.703
reverse
// Pedestrian number 2{
13				// Ref num
7				// Number of instructions
4				// Initial instruction
point
-256.254,-1.949,-118.131
point
-254.857,-2.538,-117.934
point
-254.685,-2.551,-117.868
point
-252.227,-2.555,-115.463
point
-249.649,-2.552,-113.015
point
-249.474,-2.375,-112.792
reverse
// Pedestrian number 2{
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-248.059,-2.552,-116.864
point
-253.718,-2.552,-118.154
point
-255.578,-2.553,-116.628
point
-263.178,-2.552,-112.017
reverse
// Pedestrian number 2{
12				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-267.119,-2.552,-105.096
point
-268.950,-2.552,-100.688
point
-268.972,-2.552,-99.885
point
-268.770,-2.552,-98.700
reverse
// Pedestrian number 2{
17				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-265.747,-2.552,-102.873
point
-266.213,-2.552,-102.369
point
-267.388,-2.552,-101.191
point
-268.140,-2.552,-99.290
reverse
// Pedestrian number 2{
12				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-268.510,-2.552,-96.082
point
-269.419,-2.552,-95.982
point
-269.996,-2.552,-96.009
point
-270.965,-2.552,-95.727
reverse
// Pedestrian number 2{
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-270.612,-2.552,-93.539
point
-272.192,-2.552,-92.011
point
-273.328,-2.552,-89.927
reverse
// Pedestrian number 2z
17				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-271.353,-2.552,-86.780
point
-270.768,-2.552,-88.015
point
-271.118,-2.552,-89.710
point
-271.604,-2.552,-94.356
reverse
// Pedestrian number 2z
14				// Ref num
7				// Number of instructions
3				// Initial instruction
point
-273.074,-2.552,-90.576
point
-271.751,-2.552,-91.215
point
-270.852,-2.552,-92.071
point
-270.782,-2.552,-92.561
point
-270.966,-2.552,-93.711
point
-270.543,-2.552,-94.764
reverse
// Pedestrian number 2z
13				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-269.747,-2.552,-95.901
point
-269.889,-2.552,-96.406
point
-269.582,-2.552,-97.218
point
-269.587,-2.552,-99.100
reverse
// Pedestrian number 2z
3				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-270.059,-2.552,-97.862
point
-270.202,-2.552,-96.389
point
-269.989,-2.552,-96.204
point
-269.321,-2.552,-95.592
point
-268.932,-2.552,-95.083
reverse
// Pedestrian number 2z
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-270.161,-2.552,-95.634
point
-270.684,-2.552,-95.088
point
-271.006,-2.552,-93.934
point
-270.847,-2.552,-93.521
reverse
// Pedestrian number 2z
8				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-269.579,-2.552,-93.592
point
-270.703,-2.552,-92.680
point
-270.711,-2.552,-91.995
point
-271.785,-2.552,-89.840
point
-274.849,-2.552,-86.565
reverse
// Pedestrian number 2z
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-276.199,-2.552,-83.962
point
-275.976,-2.552,-81.561
point
-276.119,-2.552,-78.714
reverse
// Pedestrian number 2z
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-277.056,-2.552,-77.404
point
-279.163,-2.552,-76.725
point
-282.674,-2.552,-75.077
reverse
// Pedestrian number 2z
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-282.977,-2.552,-74.724
point
-283.517,-2.543,-71.793
point
-284.632,-2.543,-66.837
reverse
// Pedestrian number 2z
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-285.338,-2.538,-71.991
point
-283.194,-2.549,-72.864
point
-280.490,-2.558,-73.152
reverse
// Pedestrian number 2y
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-283.911,-2.549,-73.598
point
-283.794,-2.544,-72.309
point
-283.355,-2.540,-70.791
point
-283.430,-2.549,-66.934
reverse
// Pedestrian number 2y
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-283.092,-2.539,-70.381
point
-282.657,-2.547,-71.956
point
-281.994,-2.552,-75.766
reverse
// Pedestrian number 2y
13				// Ref num
7				// Number of instructions
3				// Initial instruction
point
-290.901,-2.611,-66.648
point
-288.910,-2.545,-67.798
point
-285.894,-2.539,-70.891
point
-285.276,-2.538,-71.726
point
-285.246,-2.538,-72.306
point
-284.425,-2.536,-73.187
reverse
// Pedestrian number 2y
5				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-301.475,-3.692,-66.697
point
-302.839,-3.869,-66.676
point
-304.337,-3.982,-66.926
point
-304.980,-4.043,-66.621
point
-305.100,-4.048,-66.229
reverse
// Pedestrian number 2y
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-305.706,-4.048,-65.861
point
-307.220,-4.048,-65.232
point
-308.040,-4.048,-64.304
point
-308.729,-4.048,-62.258
reverse
// Pedestrian number 2y
12				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-303.969,-3.932,-69.400
point
-305.848,-4.041,-69.120
point
-306.448,-4.048,-68.937
point
-308.740,-4.048,-67.573
point
-309.267,-4.048,-67.093
reverse
// Pedestrian number 2y
17				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-307.891,-4.048,-64.913
point
-308.340,-4.048,-64.183
point
-309.051,-4.048,-61.428
point
-309.025,-4.048,-59.326
reverse
// Pedestrian number 2y
12				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-308.805,-4.048,-58.997
point
-308.080,-4.048,-57.100
point
-307.767,-4.048,-56.761
point
-307.414,-4.048,-56.369
reverse
// Pedestrian number 2y
17				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-309.587,-4.048,-54.168
point
-310.881,-4.048,-57.725
point
-312.007,-4.048,-60.843
reverse
// Pedestrian number 2y
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-311.804,-4.048,-61.502
point
-310.921,-4.048,-64.048
point
-310.213,-4.048,-66.074
reverse
// Pedestrian number 2x
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-308.079,-4.048,-68.005
point
-308.182,-4.048,-63.287
point
-306.977,-3.161,-62.076
point
-306.926,-3.032,-61.235
reverse
// Pedestrian number 2x
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-307.824,-3.507,-61.157
point
-308.813,-4.048,-59.570
point
-308.793,-4.048,-58.301
reverse
// Pedestrian number 2x
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-307.130,-4.048,-55.946
point
-306.899,-4.048,-55.779
point
-305.834,-4.096,-55.090
reverse
// Pedestrian number 2x
17				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-304.480,-4.189,-54.490
point
-301.394,-4.602,-53.573
point
-298.731,-5.309,-52.973
reverse
// Pedestrian number 2x
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-301.548,-4.739,-50.540
point
-298.747,-5.509,-49.881
point
-294.961,-6.758,-49.008
reverse
// Pedestrian number 2x
29				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-294.532,-6.654,-51.923
point
-291.191,-7.824,-50.756
point
-290.127,-7.884,-50.524
reverse
// Pedestrian number 2x
5				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-289.188,-7.940,-50.205
point
-287.985,-8.005,-49.575
point
-286.891,-8.005,-45.905
point
-287.160,-8.005,-42.215
point
-287.398,-8.005,-40.596
reverse
// Pedestrian number 2x
3				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-284.490,-8.005,-43.511
point
-284.121,-8.005,-42.692
point
-283.543,-7.696,-41.533
point
-282.199,-6.852,-41.083
reverse
// Pedestrian number 2x
1				// Ref num
9				// Number of instructions
7				// Initial instruction
point
-284.061,-8.005,-41.127
point
-284.608,-8.005,-40.453
point
-284.884,-8.005,-39.560
point
-284.993,-8.005,-37.977
point
-287.371,-8.005,-34.764
point
-287.551,-7.986,-34.585
point
-287.611,-7.921,-34.413
point
-288.716,-7.151,-32.136
reverse
// Pedestrian number 2x
29				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-289.499,-8.005,-37.279
point
-288.412,-8.004,-38.154
point
-287.520,-8.005,-38.325
point
-284.597,-8.005,-39.560
reverse
// Pedestrian number 2w
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-287.740,-8.005,-39.147
point
-284.316,-8.005,-42.046
point
-284.425,-8.005,-44.507
reverse
// Pedestrian number 2w
8				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-284.152,-7.877,-44.685
point
-284.000,-7.508,-45.728
point
-283.980,-7.130,-46.951
point
-283.854,-6.798,-47.763
reverse
// Pedestrian number 2w
5				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-285.223,-8.005,-46.513
point
-286.407,-8.005,-43.838
point
-286.426,-8.005,-42.530
point
-287.079,-8.005,-41.616
point
-288.226,-8.005,-38.548
reverse
// Pedestrian number 2w
8				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-286.337,-8.005,-35.899
point
-290.809,-8.008,-35.344
point
-293.451,-8.166,-35.358
point
-296.326,-8.525,-35.300
reverse
// Pedestrian number 2w
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-294.880,-8.344,-35.505
point
-296.654,-8.568,-35.057
point
-298.035,-9.013,-34.785
point
-299.920,-9.442,-35.244
reverse
// Pedestrian number 2w
29				// Ref num
9				// Number of instructions
4				// Initial instruction
point
-298.103,-9.166,-32.271
point
-298.430,-9.285,-32.439
point
-298.882,-9.455,-32.377
point
-299.777,-9.776,-32.361
point
-300.623,-9.943,-32.472
point
-301.872,-10.077,-33.420
point
-303.143,-10.477,-33.677
point
-304.486,-10.909,-34.832
reverse
// Pedestrian number 2w
29				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-307.012,-11.793,-31.538
point
-309.669,-11.971,-32.758
point
-311.882,-11.971,-33.109
point
-313.365,-11.971,-32.132
reverse
// Pedestrian number 2w
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-312.356,-11.971,-32.852
point
-313.862,-11.971,-31.535
point
-315.467,-11.971,-29.014
reverse
// Pedestrian number 2w
17				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-312.483,-11.971,-28.242
point
-313.842,-11.971,-28.279
point
-315.790,-11.970,-27.237
point
-316.223,-11.971,-25.335
reverse
// Pedestrian number 2w
29				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-310.193,-11.971,-30.589
point
-311.153,-11.971,-30.196
point
-312.376,-11.970,-28.775
point
-313.233,-11.971,-26.534
point
-313.226,-11.971,-25.457
reverse
// Pedestrian number 2v
12				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-315.747,-11.971,-28.199
point
-316.031,-11.971,-26.501
point
-316.089,-11.970,-24.197
point
-314.094,-11.971,-19.618
reverse
// Pedestrian number 2v
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-311.120,-11.971,-20.670
point
-315.798,-11.970,-23.028
point
-316.008,-11.970,-23.627
reverse
// Pedestrian number 2v
8				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-315.036,-11.971,-21.178
point
-313.307,-11.971,-25.137
point
-312.906,-11.971,-28.068
point
-312.947,-11.971,-32.545
reverse
// Pedestrian number 2v
1				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-311.320,-11.971,-33.469
point
-309.793,-11.956,-33.640
point
-308.575,-11.841,-34.222
point
-307.413,-11.808,-34.660
reverse
// Pedestrian number 2v
12				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-310.494,-11.971,-33.931
point
-312.101,-11.970,-28.817
point
-313.131,-11.971,-26.533
point
-313.080,-11.971,-24.407
point
-312.879,-11.971,-23.506
reverse
// Pedestrian number 2v
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-309.599,-12.052,-19.766
point
-307.176,-12.105,-18.568
point
-304.902,-12.106,-18.046
reverse
// Pedestrian number 2v
3				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-303.618,-12.106,-17.323
point
-297.948,-12.106,-11.354
point
-295.342,-12.106,-9.547
reverse
// Pedestrian number 2v
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-294.592,-12.106,-12.659
point
-293.640,-12.106,-11.881
point
-290.160,-12.119,-9.516
reverse
// Pedestrian number 2v
8				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-293.474,-12.106,-8.167
point
-292.018,-12.119,-7.229
point
-291.375,-12.134,-6.629
point
-290.872,-12.106,-6.118
reverse
// Pedestrian number 2v
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-287.163,-12.203,-7.032
point
-286.617,-11.939,-7.076
point
-285.686,-11.252,-7.410
reverse
// Pedestrian number 300
8				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-285.871,-12.313,-5.671
point
-283.815,-12.540,-3.074
point
-283.024,-12.625,-2.703
point
-282.159,-12.592,-2.212
reverse
// Pedestrian number 301
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-275.947,-15.455,15.963
point
-274.709,-15.615,18.590
point
-268.921,-15.627,21.687
reverse
// Pedestrian number 302
13				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-269.260,-15.627,21.154
point
-269.260,-15.627,21.154
point
-274.742,-15.616,19.025
point
-274.987,-15.613,18.556
reverse
// Pedestrian number 303
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-275.048,-15.617,19.181
point
-275.296,-15.626,21.891
point
-274.156,-15.627,26.848
point
-275.075,-15.627,28.241
reverse
// Pedestrian number 304
13				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-276.114,-15.627,28.865
point
-276.806,-15.627,28.757
point
-276.806,-15.627,28.757
point
-278.927,-15.627,27.563
point
-279.874,-15.627,27.672
reverse
// Pedestrian number 305
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-275.915,-15.627,28.331
point
-274.419,-15.627,26.937
point
-273.867,-15.627,26.357
reverse
// Pedestrian number 306
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-275.798,-15.627,23.631
point
-275.376,-15.627,22.759
point
-269.842,-15.625,20.327
point
-269.526,-15.626,20.538
reverse
// Pedestrian number 307
13				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-269.464,-15.627,20.822
point
-271.195,-15.627,21.548
point
-273.283,-15.622,20.901
point
-275.121,-15.621,20.428
reverse
// Pedestrian number 308
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-271.521,-15.627,23.166
point
-270.772,-15.627,23.565
point
-267.721,-15.627,22.818
reverse
// Pedestrian number 309
13				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-264.867,-15.627,23.968
point
-266.649,-15.627,23.637
point
-269.462,-15.627,22.086
point
-275.319,-15.623,21.089
reverse
// Pedestrian number 310
13				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-270.668,-15.621,19.419
point
-269.911,-15.627,20.721
point
-270.254,-15.629,22.299
point
-270.389,-15.627,23.600
point
-269.725,-15.627,24.812
reverse
// Pedestrian number 311
14				// Ref num
7				// Number of instructions
2				// Initial instruction
point
-272.612,-15.627,23.147
point
-273.271,-15.627,24.415
point
-273.594,-15.627,24.889
point
-273.671,-15.627,25.698
point
-275.341,-15.627,26.548
point
-278.109,-15.627,26.682
reverse
// Pedestrian number 312
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-280.589,-15.627,33.937
point
-280.646,-15.627,35.766
point
-279.847,-15.627,37.526
reverse
// Pedestrian number 313
14				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-282.105,-15.627,40.554
point
-281.144,-15.627,41.464
point
-280.896,-15.627,45.967
reverse
// Pedestrian number 314
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-275.261,-16.364,57.993
point
-275.306,-16.591,59.619
point
-274.518,-16.875,61.463
reverse
// Pedestrian number 315
17				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-274.434,-16.902,61.736
point
-275.504,-17.083,63.476
point
-276.184,-17.419,66.389
point
-275.677,-17.638,68.356
reverse
// Pedestrian number 316
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-276.525,-17.276,65.334
point
-276.656,-17.120,64.043
point
-277.100,-16.921,62.514
reverse
// Pedestrian number 317
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-274.600,-16.823,61.127
point
-277.527,-16.613,60.288
point
-277.928,-16.431,59.083
reverse
// Pedestrian number 318
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-277.329,-16.783,61.450
point
-274.153,-17.132,63.567
point
-273.629,-17.375,65.448
reverse
// Pedestrian number 319
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-272.091,-18.286,72.098
point
-273.900,-18.648,76.202
point
-273.648,-18.772,77.788
reverse
// Pedestrian number 320
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-273.480,-18.815,78.534
point
-272.702,-18.907,81.642
point
-272.380,-18.909,83.736
reverse
// Pedestrian number 321
3				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-272.125,-18.910,84.419
point
-268.699,-18.913,87.433
point
-268.551,-18.914,88.454
reverse
// Pedestrian number 322
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-267.860,-18.915,90.476
point
-267.589,-18.915,92.464
point
-267.190,-18.917,93.251
reverse
// Pedestrian number 323
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-267.361,-18.915,93.750
point
-267.103,-18.915,94.906
point
-266.904,-18.915,96.369
reverse
// Pedestrian number 324
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-266.662,-18.915,97.291
point
-265.214,-18.915,103.269
point
-263.493,-18.915,105.492
reverse
// Pedestrian number 325
12				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-264.258,-18.915,103.497
point
-262.888,-18.915,103.594
point
-259.906,-18.916,102.546
point
-258.473,-18.916,102.074
reverse
// Pedestrian number 326
12				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-260.209,-18.915,104.902
point
-261.442,-18.915,105.097
point
-262.568,-18.915,105.461
point
-264.052,-18.915,105.634
reverse
// Pedestrian number 327
17				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-264.786,-18.914,105.968
point
-266.973,-18.915,105.454
point
-268.860,-18.916,104.565
reverse
// Pedestrian number 328
17				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-265.318,-18.915,102.577
point
-267.780,-18.916,104.111
point
-271.038,-18.916,107.321
reverse
// Pedestrian number 329
14				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-271.659,-18.916,107.585
point
-272.700,-18.916,107.682
point
-275.621,-18.916,108.434
reverse
// Pedestrian number 330
12				// Ref num
7				// Number of instructions
5				// Initial instruction
point
-277.279,-18.916,106.409
point
-278.052,-18.916,106.785
point
-279.855,-18.916,106.897
point
-280.732,-18.916,107.190
point
-281.522,-18.916,107.353
point
-287.395,-18.916,108.702
reverse
// Pedestrian number 331
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-287.781,-18.915,109.007
point
-287.005,-18.915,109.530
point
-284.483,-18.915,110.371
reverse
// Pedestrian number 332
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-285.320,-18.915,110.565
point
-283.753,-18.914,110.043
point
-282.909,-18.914,108.214
point
-282.223,-18.916,107.447
reverse
// Pedestrian number 333
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-278.529,-18.914,108.997
point
-276.784,-18.916,108.745
point
-272.298,-18.916,105.406
reverse
// Pedestrian number 334
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-271.767,-18.916,105.116
point
-270.238,-18.916,105.152
point
-268.600,-18.916,104.356
reverse
// Pedestrian number 335
29				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-257.403,-18.916,104.343
point
-256.166,-18.915,103.924
point
-253.647,-18.916,101.001
reverse
// Pedestrian number 336
29				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-251.203,-18.916,100.337
point
-248.252,-18.916,101.620
point
-243.906,-18.916,101.111
reverse
// Pedestrian number 337
12				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-241.962,-18.915,100.665
point
-239.599,-18.916,97.883
point
-236.994,-18.916,97.068
point
-236.052,-18.916,96.823
reverse
// Pedestrian number 338
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-230.100,-18.916,95.496
point
-227.497,-18.916,96.367
point
-224.827,-18.916,96.739
reverse
// Pedestrian number 339
17				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-224.247,-18.916,96.663
point
-223.229,-18.916,95.255
point
-222.475,-18.916,93.876
reverse
// Pedestrian number 340
17				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-222.129,-18.916,96.112
point
-225.941,-18.916,95.009
point
-227.570,-18.916,94.916
reverse
// Pedestrian number 341
29				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-230.675,-18.916,95.681
point
-232.337,-18.916,98.317
point
-234.208,-18.916,98.923
reverse
// Pedestrian number 342
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-236.473,-18.916,99.195
point
-237.403,-18.916,99.547
point
-239.771,-18.916,99.977
reverse
// Pedestrian number 343
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-244.636,-18.916,101.256
point
-243.045,-18.915,100.927
point
-240.603,-18.916,100.428
reverse
// Pedestrian number 344
17				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-241.676,-18.916,97.872
point
-242.133,-18.915,99.371
point
-243.668,-18.916,101.059
reverse
// Pedestrian number 345
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-258.016,-18.916,101.915
point
-256.635,-18.915,101.778
point
-251.856,-18.916,102.896
reverse
// Pedestrian number 346
3				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-242.661,-18.915,94.750
point
-243.590,-18.915,93.460
point
-245.618,-18.915,91.881
point
-245.822,-18.915,91.091
point
-246.407,-18.915,89.219
reverse
// Pedestrian number 347
1				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-248.346,-18.916,88.619
point
-248.651,-18.916,88.589
point
-250.594,-18.916,89.034
point
-253.616,-18.916,89.690
reverse
// Pedestrian number 348
5				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-256.635,-18.916,90.560
point
-253.937,-18.916,89.438
point
-252.016,-18.916,89.394
point
-250.196,-18.916,87.138
reverse
// Pedestrian number 349
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-248.563,-18.916,86.478
point
-249.387,-18.916,87.020
point
-253.946,-18.916,87.627
reverse
// Pedestrian number 350
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-255.604,-18.916,87.920
point
-257.768,-18.915,90.792
point
-258.445,-18.916,90.861
reverse
// Pedestrian number 351
17				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-240.526,-18.915,84.616
point
-239.882,-18.915,84.350
point
-235.910,-18.915,83.580
reverse
// Pedestrian number 352
8				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-235.968,-18.916,85.765
point
-239.119,-18.916,86.048
point
-240.148,-18.916,86.797
point
-241.421,-18.916,86.919
point
-242.623,-18.916,87.273
reverse
// Pedestrian number 353
1				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-243.849,-18.916,87.634
point
-244.802,-18.915,85.567
point
-245.180,-18.914,83.335
point
-245.664,-18.913,82.051
point
-245.604,-18.912,81.275
reverse
// Pedestrian number 354
17				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-249.726,-18.892,75.676
point
-247.778,-18.859,74.234
point
-247.643,-18.786,72.308
point
-247.717,-18.737,71.682
reverse
// Pedestrian number 355
14				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-246.677,-18.906,75.374
point
-248.844,-18.909,77.993
point
-248.383,-18.911,80.406
reverse
// Pedestrian number 356
12				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-249.638,-18.916,89.036
point
-246.949,-18.915,88.290
point
-244.024,-18.916,87.838
point
-242.617,-18.915,85.084
point
-241.820,-18.915,84.752
reverse
// Pedestrian number 357
29				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-230.822,-18.916,84.707
point
-229.908,-18.916,84.146
point
-228.819,-18.916,84.256
point
-226.632,-18.916,83.831
point
-224.363,-18.916,81.696
reverse
// Pedestrian number 358
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-223.842,-18.916,82.470
point
-225.192,-18.916,81.939
point
-227.269,-18.916,81.629
reverse
// Pedestrian number 359
17				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-225.378,-18.916,81.111
point
-227.952,-18.917,81.760
point
-232.958,-18.916,85.192
reverse
// Pedestrian number 360
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-233.629,-18.916,85.244
point
-235.137,-18.915,85.428
point
-237.883,-18.916,84.002
reverse
// Pedestrian number 361
1				// Ref num
7				// Number of instructions
5				// Initial instruction
point
-234.603,-18.916,83.075
point
-237.291,-18.916,84.277
point
-239.141,-18.916,84.414
point
-240.060,-18.916,84.651
point
-241.329,-18.914,84.995
point
-243.182,-18.916,87.368
reverse
// Pedestrian number 362
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-243.846,-18.915,89.669
point
-243.772,-18.915,91.633
point
-242.658,-18.915,94.584
reverse
// Pedestrian number 363
17				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-225.214,-18.916,96.958
point
-224.474,-18.916,96.468
point
-224.210,-18.916,95.897
point
-223.458,-18.916,94.270
reverse
// Pedestrian number 364
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-289.800,-18.915,98.099
point
-287.528,-18.915,97.391
point
-286.992,-18.915,95.275
reverse
// Pedestrian number 365
1				// Ref num
7				// Number of instructions
3				// Initial instruction
point
-286.584,-18.916,95.062
point
-285.122,-18.916,94.775
point
-284.024,-18.916,94.553
point
-282.993,-18.916,94.208
point
-281.769,-18.916,94.357
point
-279.257,-18.916,93.459
reverse
// Pedestrian number 366
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-278.403,-18.916,93.124
point
-276.421,-18.916,92.787
point
-273.351,-18.916,92.168
reverse
// Pedestrian number 367
12				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-276.536,-18.916,95.028
point
-277.883,-18.916,95.336
point
-279.189,-18.916,95.195
point
-281.667,-18.916,96.371
reverse
// Pedestrian number 368
17				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-280.027,-18.916,95.991
point
-278.853,-18.916,95.361
point
-277.985,-18.916,93.932
point
-277.008,-18.916,92.852
reverse
// Pedestrian number 369
8				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-275.923,-18.916,92.597
point
-274.557,-18.916,92.760
point
-272.792,-18.916,92.171
point
-267.385,-18.915,90.680
reverse
// Pedestrian number 370
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-249.956,-17.586,62.402
point
-253.447,-17.126,59.029
point
-253.663,-16.985,57.797
reverse
// Pedestrian number 371
17				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-252.848,-17.401,61.382
point
-251.877,-16.860,56.561
point
-251.740,-16.522,54.063
point
-252.232,-16.232,51.727
reverse
// Pedestrian number 372
12				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-255.093,-16.136,51.243
point
-255.367,-16.081,50.658
point
-253.478,-15.866,48.171
reverse
// Pedestrian number 373
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-259.604,-15.627,19.171
point
-263.137,-15.657,16.034
point
-263.787,-15.657,14.920
reverse
// Pedestrian number 374
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-266.962,-15.680,-2.238
point
-267.167,-15.791,-4.341
point
-267.122,-15.904,-6.260
reverse
// Pedestrian number 375
1				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-264.090,-15.692,-2.653
point
-264.235,-15.791,-4.428
point
-264.105,-15.851,-5.513
point
-264.434,-16.113,-10.220
point
-264.228,-16.144,-10.802
reverse
// Pedestrian number 376
8				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-264.208,-16.184,-11.530
point
-264.744,-16.682,-17.259
point
-265.236,-16.733,-17.799
point
-265.035,-16.840,-18.964
reverse
// Pedestrian number 377
3				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-119.834,-13.901,-123.061
point
-117.564,-13.901,-123.633
point
-115.680,-13.901,-123.977
reverse
// Pedestrian number 378
29				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-109.031,-13.901,-125.677
point
-105.715,-13.901,-126.182
point
-102.975,-13.901,-127.024
reverse
// Pedestrian number 379
1				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-101.611,-13.901,-127.207
point
-99.451,-13.901,-127.706
point
-96.372,-13.901,-128.519
point
-93.558,-13.901,-129.240
reverse
// Pedestrian number 380
5				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-91.666,-13.901,-126.863
point
-90.408,-13.901,-126.956
point
-87.817,-13.901,-127.590
point
-86.489,-13.901,-128.258
point
-85.750,-13.901,-130.193
reverse
// Pedestrian number 381
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-84.949,-13.901,-131.149
point
-80.765,-13.901,-129.335
point
-79.234,-13.901,-129.693
reverse
// Pedestrian number 382
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-77.973,-13.901,-129.919
point
-76.168,-13.900,-133.065
point
-73.672,-13.901,-133.667
reverse
// Pedestrian number 383
13				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-83.065,-13.901,-131.665
point
-84.022,-13.901,-131.468
point
-87.263,-13.901,-130.582
point
-88.684,-13.901,-130.165
point
-89.755,-13.901,-129.999
reverse
// Pedestrian number 384
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-91.735,-13.901,-126.627
point
-93.750,-13.901,-126.619
point
-97.768,-13.901,-125.274
reverse
// Pedestrian number 385
29				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-98.194,-13.901,-125.123
point
-101.434,-13.901,-124.704
point
-103.321,-13.901,-124.105
point
-104.968,-13.901,-123.493
reverse
// Pedestrian number 386
5				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-111.649,-13.901,-124.905
point
-113.716,-13.901,-122.206
point
-115.137,-13.901,-121.271
point
-116.340,-13.901,-120.804
point
-118.246,-13.901,-120.392
reverse
// Pedestrian number 387
3				// Ref num
7				// Number of instructions
4				// Initial instruction
point
-121.292,-13.901,-119.788
point
-123.196,-13.901,-119.728
point
-124.535,-13.901,-118.956
point
-125.394,-13.901,-118.697
point
-126.965,-13.901,-118.549
point
-128.145,-13.901,-118.237
reverse
// Pedestrian number 388
1				// Ref num
7				// Number of instructions
3				// Initial instruction
point
-132.275,-13.901,-119.952
point
-135.456,-13.817,-119.294
point
-137.788,-13.901,-118.554
point
-140.212,-13.901,-118.253
point
-140.870,-13.901,-117.947
point
-141.976,-13.977,-117.808
reverse
// Pedestrian number 389
3				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-145.000,-14.111,-114.419
point
-147.714,-14.343,-113.757
point
-148.978,-14.441,-113.374
point
-150.077,-14.520,-113.405
point
-151.259,-14.618,-112.759
reverse
// Pedestrian number 390
29				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-154.072,-14.744,-114.431
point
-156.939,-14.906,-113.855
point
-158.349,-14.962,-112.972
point
-160.074,-15.001,-112.697
reverse
// Pedestrian number 391
13				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-163.051,-15.344,-108.087
point
-164.301,-15.485,-107.578
point
-166.077,-15.909,-106.568
point
-166.565,-16.010,-106.127
point
-167.904,-16.244,-105.358
reverse
// Pedestrian number 392
8				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-169.241,-16.457,-104.871
point
-170.250,-16.652,-104.404
point
-172.089,-17.158,-102.408
point
-173.911,-17.623,-100.836
reverse
// Pedestrian number 393
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-183.381,-17.667,-94.703
point
-185.582,-17.667,-93.495
point
-187.395,-17.667,-92.805
point
-188.499,-17.667,-92.221
reverse
// Pedestrian number 394
13				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-189.212,-17.667,-92.062
point
-193.357,-17.667,-93.250
point
-194.419,-17.667,-93.268
point
-195.772,-17.667,-92.864
point
-196.934,-17.667,-92.532
reverse
// Pedestrian number 395
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-200.913,-17.667,-89.040
point
-202.033,-17.667,-88.797
point
-204.014,-17.667,-88.626
point
-205.983,-17.667,-88.356
reverse
// Pedestrian number 396
1				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-205.578,-17.667,-91.182
point
-207.331,-17.667,-90.489
point
-208.538,-17.667,-90.705
point
-209.648,-17.667,-91.079
point
-212.465,-17.667,-91.333
reverse
// Pedestrian number 397
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-222.421,-17.667,-90.108
point
-225.237,-17.667,-90.657
point
-228.646,-17.667,-94.731
reverse
// Pedestrian number 398
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-222.851,-17.667,-92.715
point
-225.380,-17.667,-93.718
point
-230.772,-17.667,-92.287
reverse
// Pedestrian number 399
13				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-231.315,-17.667,-92.144
point
-236.308,-17.667,-91.844
point
-237.168,-17.667,-90.632
point
-238.428,-17.667,-88.917
reverse
// Pedestrian number 400
14				// Ref num
7				// Number of instructions
4				// Initial instruction
point
-234.244,-17.667,-90.010
point
-234.876,-17.667,-89.574
point
-235.287,-17.667,-88.471
point
-236.050,-17.667,-87.275
point
-237.103,-17.667,-85.875
point
-237.296,-17.667,-85.318
reverse
// Pedestrian number 401
8				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-239.589,-17.667,-87.027
point
-238.759,-17.667,-88.124
point
-233.632,-17.667,-90.893
point
-233.018,-17.667,-91.433
point
-231.069,-17.667,-95.099
reverse
// Pedestrian number 402
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-229.490,-17.667,-94.925
point
-232.882,-17.667,-94.231
point
-234.970,-17.667,-93.341
reverse
// Pedestrian number 403
29				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-235.881,-17.667,-92.742
point
-237.468,-17.667,-89.190
point
-237.576,-17.667,-86.398
point
-237.810,-17.667,-84.738
point
-239.074,-17.667,-83.249
reverse
// Pedestrian number 404
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-239.940,-17.667,-81.940
point
-241.389,-17.667,-80.509
point
-242.760,-17.667,-79.235
point
-243.512,-17.667,-78.624
reverse
// Pedestrian number 405
5				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-245.986,-17.667,-80.303
point
-244.407,-17.667,-81.344
point
-243.769,-17.667,-82.153
point
-242.335,-17.667,-83.856
reverse
// Pedestrian number 406
1				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-241.138,-17.667,-85.195
point
-241.675,-17.667,-83.809
point
-242.744,-17.667,-82.883
point
-243.966,-17.667,-78.255
reverse
// Pedestrian number 407
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-245.521,-17.667,-77.607
point
-247.017,-17.667,-77.002
point
-249.465,-17.667,-76.193
reverse
// Pedestrian number 408
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-251.893,-17.667,-74.479
point
-256.607,-17.667,-74.979
point
-259.508,-17.667,-74.238
reverse
// Pedestrian number 409
13				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-264.458,-17.667,-70.671
point
-265.318,-17.667,-65.596
point
-266.224,-17.667,-63.769
point
-266.944,-17.667,-63.032
point
-267.397,-17.667,-61.949
reverse
// Pedestrian number 410
14				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-268.182,-17.667,-60.830
point
-267.928,-17.667,-62.571
point
-266.643,-17.667,-64.806
point
-266.713,-17.667,-67.852
point
-265.824,-17.667,-68.878
reverse
// Pedestrian number 411
3				// Ref num
6				// Number of instructions
3				// Initial instruction
point
-264.989,-17.667,-69.779
point
-262.826,-17.667,-72.031
point
-262.093,-17.667,-72.685
point
-260.609,-17.667,-73.550
point
-257.839,-17.667,-74.706
reverse
// Pedestrian number 412
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-255.378,-17.667,-75.598
point
-252.351,-17.667,-77.418
point
-250.216,-17.667,-79.156
reverse
// Pedestrian number 413
29				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-252.969,-17.667,-73.850
point
-256.132,-17.667,-73.995
point
-258.440,-17.667,-73.304
point
-261.503,-17.667,-69.874
point
-264.039,-17.667,-66.725
reverse
// Pedestrian number 414
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-271.027,-17.667,-61.583
point
-272.535,-17.667,-58.840
point
-274.032,-17.667,-52.526
reverse
// Pedestrian number 415
8				// Ref num
6				// Number of instructions
2				// Initial instruction
point
-271.331,-17.667,-49.860
point
-271.311,-17.667,-48.130
point
-271.297,-17.667,-46.380
point
-271.427,-17.667,-44.970
point
-271.157,-17.667,-43.681
reverse
// Pedestrian number 416
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-268.855,-17.667,-30.778
point
-268.559,-17.667,-30.243
point
-267.896,-17.667,-29.450
reverse
// Pedestrian number 417
3				// Ref num
5				// Number of instructions
2				// Initial instruction
point
-271.924,-17.667,-32.767
point
-272.570,-17.667,-36.082
point
-272.706,-17.667,-37.178
point
-273.465,-17.667,-39.753
reverse
// Pedestrian number 418
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-270.747,-17.667,-40.455
point
-272.866,-17.667,-36.484
point
-272.339,-17.667,-34.237
reverse
// Pedestrian number 419
8				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-271.845,-17.667,-31.923
point
-269.676,-17.667,-34.570
point
-270.281,-17.667,-37.579
reverse
// Pedestrian number 420
3				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-270.493,-17.667,-38.015
point
-271.410,-17.667,-36.914
point
-272.664,-17.667,-35.041
point
-272.133,-17.667,-33.504
reverse
// Pedestrian number 421
8				// Ref num
7				// Number of instructions
4				// Initial instruction
point
-271.174,-17.667,-31.072
point
-271.721,-17.667,-33.570
point
-272.730,-17.667,-35.622
point
-273.163,-17.667,-37.531
point
-271.921,-17.667,-39.174
point
-271.089,-17.667,-42.821
reverse
// Pedestrian number 422
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-270.053,-17.667,-26.369
point
-269.945,-17.667,-27.000
point
-270.647,-17.667,-28.010
reverse
// Pedestrian number 423
13				// Ref num
6				// Number of instructions
4				// Initial instruction
point
-269.690,-17.667,-25.496
point
-269.842,-17.667,-25.983
point
-270.298,-17.667,-26.927
point
-270.337,-17.667,-28.194
point
-270.756,-17.667,-28.940
reverse
// Pedestrian number 424
14				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-269.406,-17.667,-25.153
point
-268.996,-17.666,-24.854
point
-268.898,-17.355,-22.439
reverse
// Pedestrian number 425
5				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-266.252,-17.443,-23.823
point
-265.947,-17.238,-22.254
point
-267.972,-16.891,-18.890
reverse
// Pedestrian number 426
13				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-267.071,-17.667,-26.394
point
-266.334,-17.478,-24.081
point
-266.049,-17.349,-23.131
reverse
// Pedestrian number 427
1				// Ref num
4				// Number of instructions
2				// Initial instruction
point
-267.927,-17.000,-19.824
point
-268.300,-17.152,-21.026
point
-266.443,-17.541,-24.563
reverse
// Pedestrian number 428
8				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-266.648,-17.641,-25.315
point
-266.742,-17.514,-24.281
point
-266.126,-17.317,-22.841
point
-265.068,-16.746,-17.961
reverse
// Pedestrian number 429
29				// Ref num
5				// Number of instructions
3				// Initial instruction
point
-269.300,-17.624,-24.315
point
-268.899,-17.480,-23.371
point
-268.473,-17.260,-21.869
point
-265.572,-17.078,-21.051
reverse
// Pedestrian number 430
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-287.459,-15.627,39.118
reverse
// Pedestrian number 431
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-287.210,-15.627,40.372
reverse
// Pedestrian number 432
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-286.898,-15.627,41.898
reverse
// Pedestrian number 433
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-280.139,-15.627,35.601
reverse
// Pedestrian number 434
130				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-239.364,-18.916,86.650
reverse
// Pedestrian number 435
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-271.043,-18.916,91.502
reverse
// Pedestrian number 436
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-271.787,-18.916,91.665
reverse
// Pedestrian number 437
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-277.022,-18.916,95.333
reverse
// Pedestrian number 438
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-278.585,-18.916,95.637
reverse
// Pedestrian number 439
129				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-287.680,-18.915,96.539
reverse
// Pedestrian number 440
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-288.693,-18.915,96.701
reverse
// Pedestrian number 441
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-286.898,-18.915,109.796
reverse
// Pedestrian number 442
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-285.751,-18.915,109.419
reverse
// Pedestrian number 443
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-275.152,-18.916,105.913
reverse
// Pedestrian number 444
130				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-267.579,-18.915,103.067
reverse
// Pedestrian number 445
130				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-253.508,-18.916,101.013
reverse
// Pedestrian number 446
130				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-234.220,-18.916,96.708
reverse
// Pedestrian number 447
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-233.295,-18.916,96.507
reverse
// Pedestrian number 448
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-227.150,-18.916,97.137
reverse
// Pedestrian number 449
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-226.593,-18.916,97.000
reverse
// Pedestrian number 450
129				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-222.481,-18.916,94.977
reverse
// Pedestrian number 451
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-221.543,-18.916,95.059
reverse
// Pedestrian number 452
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-221.642,-18.916,94.409
reverse
// Pedestrian number 453
131				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-226.181,-18.916,82.248
reverse
// Pedestrian number 454
131				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-226.707,-18.916,82.354
reverse
// Pedestrian number 455
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-274.307,-17.667,-46.446
reverse
// Pedestrian number 456
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-274.257,-17.667,-44.535
reverse
// Pedestrian number 457
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-274.284,-17.667,-49.706
reverse
// Pedestrian number 458
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-259.818,-17.667,-70.806
reverse
// Pedestrian number 459
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-259.365,-17.667,-71.060
reverse
// Pedestrian number 460
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-260.450,-17.667,-70.372
reverse
// Pedestrian number 461
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-134.149,-13.901,-116.744
reverse
// Pedestrian number 462
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-133.133,-13.901,-116.986
reverse
// Pedestrian number 463
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-94.608,-13.901,-125.770
reverse
// Pedestrian number 464
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-93.850,-13.901,-125.954
reverse
// Pedestrian number 465
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-55.923,-13.561,-133.129
reverse
// Pedestrian number 466
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-87.012,-11.865,-136.051
reverse
// Pedestrian number 467
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-88.779,-12.543,-137.107
reverse
// Pedestrian number 468
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-99.301,-12.059,-137.304
reverse
// Pedestrian number 469
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-177.768,-7.933,-122.214
reverse
// Pedestrian number 470
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-178.348,-7.878,-120.801
reverse
// Pedestrian number 471
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-208.762,-4.206,-119.494
reverse
// Pedestrian number 472
129				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-209.185,-4.137,-120.047
reverse
// Pedestrian number 473
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-258.207,-2.552,-100.866
reverse
// Pedestrian number 474
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-260.159,-2.552,-96.271
reverse
// Pedestrian number 475
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-260.816,-2.552,-94.565
reverse
// Pedestrian number 476
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-268.781,-2.552,-98.559
reverse
// Pedestrian number 477
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-269.871,-2.552,-90.295
reverse
// Pedestrian number 478
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-269.961,-2.552,-90.025
reverse
// Pedestrian number 479
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-301.068,-3.636,-66.648
reverse
// Pedestrian number 480
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-306.901,-4.048,-65.192
reverse
// Pedestrian number 481
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-307.481,-4.048,-64.478
reverse
// Pedestrian number 482
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-307.952,-4.048,-63.872
reverse
// Pedestrian number 483
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-287.591,-8.005,-40.262
reverse
// Pedestrian number 484
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-302.234,-12.106,-16.937
reverse
// Pedestrian number 485
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-301.804,-12.106,-16.744
reverse
// Pedestrian number 486
138				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-271.668,-15.627,24.710
reverse
// Pedestrian number 487
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-272.063,-15.627,24.805
reverse
// Pedestrian number 488
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-271.201,-15.627,24.549
reverse
// Pedestrian number 489
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-272.084,-15.627,23.357
reverse
// Pedestrian number 490
100				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-214.152,-8.352,-7.375
reverse
// Pedestrian number 491
129				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-213.866,-8.290,-7.552
reverse
// Pedestrian number 492
129				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-202.868,-7.280,-4.228
reverse
// Pedestrian number 493
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-182.746,-5.425,6.452
reverse
// Pedestrian number 494
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-188.515,-5.380,4.779
reverse
// Pedestrian number 495
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-179.419,-5.431,2.074
reverse
// Pedestrian number 496
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-178.465,-5.432,1.182
reverse
// Pedestrian number 497
125				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-146.391,-7.508,-46.202
reverse
// Pedestrian number 498
125				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-135.465,-7.487,-49.345
reverse
// Pedestrian number 499
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-135.327,-18.640,-34.027
reverse
// Pedestrian number 500
128				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-135.395,-18.641,-34.552
reverse
// Pedestrian number 501
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-83.241,-13.039,-45.299
reverse
// Pedestrian number 502
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-82.370,-13.120,-45.117
reverse
// Pedestrian number 503
129				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-23.442,-15.561,-51.867
reverse
// Pedestrian number 504
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-19.152,-14.991,-77.396
reverse
// Pedestrian number 505
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-19.127,-14.982,-78.241
reverse
// Pedestrian number 506
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-14.327,-15.489,-128.504
reverse
// Pedestrian number 507
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-16.435,-15.631,-132.987
reverse
// Pedestrian number 508
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-43.317,-14.684,-133.268
reverse
// Pedestrian number 509
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-42.642,-14.745,-133.291
reverse
// Pedestrian number 510
112				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-61.800,-13.901,-133.221
reverse
// Pedestrian number 511
130				// Ref num
2				// Number of instructions
1				// Initial instruction
point
-62.341,-13.901,-136.832
reverse
START OF OPPONENT PATHS
143                             // Number of path nodes
-250.508,  -15.624,   29.209   // Node #0
-248.031,  -15.627,   38.838   // Node #1
-243.893,  -15.508,   41.091   // Node #2
-229.045,  -11.606,   30.295   // Node #3
-219.342,   -9.352,   16.413   // Node #4
-211.405,   -8.951,   -5.008   // Node #5
-205.429,   -7.881,   -6.354   // Node #6
-193.708,   -5.328,   -1.252   // Node #7
-185.485,   -5.428,    4.234   // Node #8
-180.135,   -5.649,    4.007   // Node #9
-176.502,   -5.435,    0.724   // Node #10
-175.172,   -5.578,   -4.666   // Node #11
-179.573,   -8.050,  -17.537   // Node #12
-178.480,   -8.840,  -24.813   // Node #13
-170.047,   -9.078,  -35.110   // Node #14
-145.562,   -8.802,  -44.806   // Node #15
-134.637,   -8.880,  -48.147   // Node #16
-114.706,   -8.874,  -52.829   // Node #17
-98.251,   -9.426,  -49.700   // Node #18
-70.570,  -12.833,  -45.715   // Node #19
-49.297,  -14.595,  -42.864   // Node #20
-29.777,  -14.596,  -49.524   // Node #21
-21.244,  -14.596,  -58.412   // Node #22
-16.074,  -14.536,  -74.221   // Node #23
-13.154,  -13.419, -116.560   // Node #24
-13.090,  -14.543, -129.299   // Node #25
-15.123,  -14.656, -134.091   // Node #26
-18.705,  -14.657, -136.028   // Node #27
-54.190,  -13.641, -136.953   // Node #28
-152.848,  -13.820, -114.594   // Node #29
-182.531,  -17.667,  -97.063   // Node #30
-196.978,  -17.667,  -91.815   // Node #31
-213.702,  -16.453,  -90.431   // Node #32
-231.135,  -16.453,  -94.236   // Node #33
-235.669,  -16.453,  -91.053   // Node #34
-239.736,  -16.453,  -84.356   // Node #35
-262.737,  -16.453,  -70.095   // Node #36
-271.548,  -16.453,  -59.852   // Node #37
-272.065,  -16.453,  -44.221   // Node #38
-266.345,  -15.303,  -13.850   // Node #39
-264.770,  -14.680,    3.261   // Node #40
-254.830,  -15.627,   43.612   // Node #41
-246.000,  -15.631,   41.796   // Node #42
-164.508,  -15.443, -109.296   // Node #43
-261.168,  -14.680,   17.931   // Node #44
-42.843,  -14.595,  -43.566   // Node #45
-61.143,  -13.907, -135.604   // Node #46
-61.029,  -14.008, -137.895   // Node #47
-63.087,  -13.880, -138.545   // Node #48
-165.655,   -8.969, -139.964   // Node #49
-169.548,   -8.663, -138.876   // Node #50
-173.986,   -8.280, -135.278   // Node #51
-177.553,   -7.952, -129.515   // Node #52
-179.660,   -7.749, -122.705   // Node #53
-182.390,   -7.474, -117.350   // Node #54
-186.456,   -7.046, -113.764   // Node #55
-194.200,   -6.154, -111.558   // Node #56
-201.944,   -5.168, -112.301   // Node #57
-207.828,   -4.353, -115.465   // Node #58
-211.222,   -3.839, -120.541   // Node #59
-214.289,   -3.446, -132.081   // Node #60
-217.671,   -3.160, -141.537   // Node #61
-222.794,   -3.040, -146.983   // Node #62
-231.198,   -2.851, -151.002   // Node #63
-234.592,   -2.789, -150.888   // Node #64
-236.819,   -2.714, -148.580   // Node #65
-248.357,   -2.552, -120.940   // Node #66
-263.688,   -2.553,  -83.516   // Node #67
-269.866,   -2.554,  -75.771   // Node #68
-277.831,   -2.553,  -70.214   // Node #69
-287.929,   -2.543,  -68.170   // Node #70
-303.068,   -3.882,  -68.291   // Node #71
-308.129,   -4.050,  -66.676   // Node #72
-310.546,   -4.048,  -61.708   // Node #73
-309.817,   -4.051,  -56.793   // Node #74
-305.228,   -4.165,  -53.014   // Node #75
-290.748,   -7.872,  -49.147   // Node #76
-286.828,   -8.007,  -46.024   // Node #77
-285.659,   -8.007,  -41.168   // Node #78
-287.814,   -8.006,  -36.492   // Node #79
-292.722,   -8.112,  -34.205   // Node #80
-308.248,  -11.861,  -33.059   // Node #81
-312.892,  -11.973,  -30.429   // Node #82
-314.787,  -11.972,  -24.998   // Node #83
-313.710,  -11.972,  -21.294   // Node #84
-311.184,  -11.997,  -18.843   // Node #85
-298.018,  -12.107,  -13.002   // Node #86
-287.082,  -12.304,   -4.837   // Node #87
-275.559,  -15.002,   12.043   // Node #88
-273.364,  -15.620,   19.899   // Node #89
-275.513,  -15.628,   26.232   // Node #90
-279.528,  -15.628,   29.152   // Node #91
-287.257,  -15.630,   30.917   // Node #92
-289.703,  -15.627,   34.061   // Node #93
-289.404,  -15.627,   37.637   // Node #94
-287.760,  -15.627,   47.198   // Node #95
-286.602,  -15.627,   48.854   // Node #96
-283.707,  -15.627,   50.241   // Node #97
-278.500,  -15.622,   50.878   // Node #98
-259.234,  -15.607,   46.407   // Node #99
-256.702,  -15.627,   46.017   // Node #100
-254.571,  -15.627,   45.821   // Node #101
-253.865,  -15.810,   47.777   // Node #102
-243.116,  -18.915,   98.813   // Node #103
-244.045,  -18.915,   99.848   // Node #104
-263.285,  -18.915,  104.667   // Node #105
-265.357,  -18.915,  103.936   // Node #106
-266.277,  -18.915,  102.814   // Node #107
-249.110,   -2.552, -118.924   // Node #108
-258.219,   -2.552, -113.832   // Node #109
-264.577,   -2.553, -106.675   // Node #110
-272.315,   -2.552,  -88.420   // Node #111
-281.437,   -2.552,  -74.518   // Node #112
-251.441,  -15.623,   26.693   // Node #113
-252.870,  -15.622,   24.867   // Node #114
-255.388,  -15.622,   23.642   // Node #115
-257.148,  -15.621,   23.266   // Node #116
-259.491,  -15.621,   23.901   // Node #117
-266.616,  -15.620,   24.606   // Node #118
-121.550,   -9.078,  -51.179   // Node #119
-123.816,   -9.356,  -45.510   // Node #120
-125.287,  -10.162,  -38.526   // Node #121
-131.912,  -13.190,  -32.790   // Node #122
-140.261,  -13.512,  -30.740   // Node #123
-145.006,  -12.423,  -30.887   // Node #124
-152.848,  -10.049,  -33.455   // Node #125
-155.717,   -8.795,  -36.452   // Node #126
-157.728,   -9.078,  -41.463   // Node #127
-136.791,  -14.001,  -31.257   // Node #128
-143.569,  -18.690,  -47.648   // Node #129
-142.298,  -18.654,  -39.284   // Node #130
-147.869,  -18.642,  -36.886   // Node #131
-151.331,  -18.664,  -39.018   // Node #132
-140.591,  -18.730,  -50.247   // Node #133
-138.024,  -18.671,  -49.664   // Node #134
-136.208,  -18.636,  -45.375   // Node #135
-134.454,  -18.587,  -41.220   // Node #136
-127.194,  -18.571,  -41.632   // Node #137
-126.725,  -18.567,  -41.644   // Node #138
-213.557,   -9.078,    0.401   // Node #139
-271.215,  -18.907,   81.140   // Node #140
-248.192,  -18.907,   75.861   // Node #141
-284.540,  -12.656,   -1.126   // Node #142
149                                           // Number of path sections
0,   1,   0, 255,   0, 255,    1.0,    0   // Section #0
1,   2,   0, 255,   0, 255,    1.0,    0   // Section #1
2,   3,   0, 255,   0, 255,    1.0,    0   // Section #2
3,   4,   0, 255,   0, 255,    1.0,    0   // Section #3
4, 139,   0, 255,   0, 255,    1.0,    0   // Section #4
5,   6,   0, 255,   0, 255,    1.0,    0   // Section #5
6,   7,   0, 255,   0, 255,    1.0,    0   // Section #6
7,   8,   0, 255,   0, 255,    1.0,    0   // Section #7
8,   9,   0, 255,   0, 255,    1.0,    0   // Section #8
9,  10,   0, 255,   0, 255,    1.0,    0   // Section #9
10,  11,   0, 255,   0, 255,    1.0,    0   // Section #10
11,  12,   0, 170,   0, 255,    1.0,    0   // Section #11
12,  13,   0, 255,   0, 255,    1.0,    0   // Section #12
13,  14,   0, 255,   0, 255,    1.0,    0   // Section #13
14, 127,   0, 255,   0, 255,    1.0,    0   // Section #14
15,  16,   0, 255,   0, 255,    1.0,    0   // Section #15
16, 119,   0, 255,   0, 255,    1.0,    0   // Section #16
17,  18,   0, 255,   0, 255,    1.0,    0   // Section #17
18,  19,   0, 255,   0, 255,    1.0,    0   // Section #18
19,  20,   0, 255,   0, 255,    1.0,    0   // Section #19
20,  45,   0, 255,   0, 255,    1.0,    0   // Section #20
21,  22,   0, 255,   0, 255,    1.0,    0   // Section #21
22,  23,   0, 255,   0, 255,    1.0,    0   // Section #22
23,  24,   0, 255,   0,  40,    1.0,    0   // Section #23
24,  25,   0, 255,   0, 255,    1.0,    0   // Section #24
25,  26,   0, 255,   0, 255,    1.0,    0   // Section #25
26,  27,   0, 255,   0, 255,    1.0,    0   // Section #26
27,  28,   0, 255,   0, 255,    1.0,    0   // Section #27
28,  46,   0, 255,   0, 255,    1.0,    0   // Section #28
43,  29,   0,  70,   0, 255,    1.0,    1   // Section #29
31,  30,   0, 255,   0, 255,    1.0,    1   // Section #30
32,  31,   0, 255,   0, 255,    1.0,    1   // Section #31
33,  32,   0,  35,   0, 255,    1.0,    1   // Section #32
34,  33,   0, 255,   0,  35,    1.0,    1   // Section #33
35,  34,   0, 255,   0, 255,    1.0,    1   // Section #34
36,  35,   0, 255,   0, 255,    0.6,    1   // Section #35
37,  36,   0, 255,   0, 255,    0.6,    1   // Section #36
38,  37,   0, 255,   0, 255,    0.6,    1   // Section #37
39,  38,   0, 255,   0, 255,    0.6,    1   // Section #38
40,  39,   0, 255,   0, 255,    0.6,    1   // Section #39
44,  40,   0, 255,   0, 255,    1.1,    1   // Section #40
41,  42,   0, 255,   0, 255,    1.1,    0   // Section #41
30,  43,   0, 255,   0, 255,    1.0,    1   // Section #42
41, 117,   0,  15,   0, 255,    1.1,    1   // Section #43
42,   2,   0, 255,   0, 255,    1.1,    0   // Section #44
45,  21,   0, 255,   0, 255,    1.0,    0   // Section #45
46,  47,   0, 255,   0, 255,    1.0,    1   // Section #46
29,  46,   0, 255,   0, 255,    1.0,    1   // Section #47
47,  48,   0, 255,   0, 255,    1.0,    1   // Section #48
48,  49,   0, 255,   0, 255,    1.0,    1   // Section #49
49,  50,   0,  65,   0,  65,    1.0,    1   // Section #50
50,  51,   0,  50,   0,  45,    1.0,    1   // Section #51
51,  52,   0,  40,   0,  50,    1.0,    1   // Section #52
52,  53,   0, 255,   0, 255,    1.0,    1   // Section #53
53,  54,   0, 255,   0,  70,    1.0,    1   // Section #54
54,  55,   0,  55,   0,  40,    1.0,    1   // Section #55
55,  56,   0,  45,   0,  40,    1.0,    1   // Section #56
56,  57,   0,  40,   0,  30,    1.0,    1   // Section #57
57,  58,   0,  35,   0,  40,    1.0,    1   // Section #58
58,  59,   0,  45,   0,  50,    1.0,    1   // Section #59
59,  60,   0, 255,   0, 255,    1.0,    1   // Section #60
60,  61,   0, 255,   0, 255,    1.0,    1   // Section #61
61,  62,   0, 255,   0, 255,    1.0,    1   // Section #62
62,  63,   0,  65,   0,  40,    1.0,    1   // Section #63
63,  64,   0,  35,   0,  30,    1.0,    1   // Section #64
64,  65,   0,  25,   0,  35,    1.0,    1   // Section #65
65,  66,   0, 255,   0, 255,    1.0,    1   // Section #66
66, 108,   0, 255,   0, 255,    1.0,    1   // Section #67
67,  68,   0, 255,   0, 255,    1.0,    1   // Section #68
68,  69,   0, 255,   0, 255,    1.0,    1   // Section #69
69,  70,   0, 255,   0, 255,    1.0,    1   // Section #70
70,  71,   0, 255,   0, 255,    1.0,    1   // Section #71
71,  72,   0, 255,   0, 255,    1.0,    1   // Section #72
72,  73,   0, 255,   0, 255,    1.0,    1   // Section #73
73,  74,   0, 255,   0, 255,    1.0,    1   // Section #74
74,  75,   0, 255,   0, 255,    1.0,    1   // Section #75
75,  76,   0, 255,   0, 255,    1.0,    1   // Section #76
76,  77,   0, 255,   0, 255,    1.0,    1   // Section #77
77,  78,   0, 255,   0, 255,    1.0,    1   // Section #78
78,  79,   0, 255,   0, 255,    1.0,    1   // Section #79
79,  80,   0, 255,   0, 255,    1.0,    1   // Section #80
80,  81,   0, 255,   0, 255,    1.0,    1   // Section #81
81,  82,   0, 255,   0, 255,    1.0,    1   // Section #82
82,  83,   0, 255,   0, 255,    1.0,    1   // Section #83
83,  84,   0, 255,   0, 255,    1.0,    1   // Section #84
84,  85,   0, 255,   0, 255,    1.0,    1   // Section #85
85,  86,   0, 255,   0, 255,    1.0,    1   // Section #86
86,  87,   0, 255,   0, 255,    1.0,    1   // Section #87
87, 142,   0, 255,   0, 255,    1.0,    1   // Section #88
88,  89,   0, 255,   0, 255,    1.0,    1   // Section #89
89,  90,   0, 255,   0, 255,    1.0,    1   // Section #90
90,  91,   0, 255,   0, 255,    1.0,    1   // Section #91
91,  92,   0, 255,   0, 255,    1.0,    1   // Section #92
92,  93,   0, 255,   0, 255,    1.0,    1   // Section #93
93,  94,   0, 255,   0, 255,    1.0,    1   // Section #94
94,  95,   0, 255,   0, 255,    1.0,    1   // Section #95
95,  96,   0, 255,   0, 255,    1.0,    1   // Section #96
96,  97,   0, 255,   0, 255,    1.0,    1   // Section #97
97,  98,   0, 255,   0, 255,    1.0,    1   // Section #98
98,  99,   0, 255,   0, 255,    1.0,    0   // Section #99
99, 100,   0, 255,   0, 255,    1.0,    0   // Section #100
100, 101,   0, 255,   0, 255,    1.0,    0   // Section #101
102, 101,   0, 255,   0, 255,    1.0,    1   // Section #102
103, 141,   0, 255,   0, 255,    1.0,    1   // Section #103
104, 103,   0, 255,   0, 255,    1.0,    1   // Section #104
105, 104,   0, 255,   0, 255,    1.0,    1   // Section #105
106, 105,   0, 255,   0, 255,    1.0,    1   // Section #106
107, 106,   0, 255,   0, 255,    1.0,    1   // Section #107
98, 140,   0, 255,   0, 255,    1.0,    1   // Section #108
108, 109,   0, 255,   0, 255,    1.0,    0   // Section #109
108,  67,   0, 255,   0, 255,    1.0,    1   // Section #110
109, 110,   0, 255,   0, 255,    1.0,    0   // Section #111
110, 111,   0, 255,   0, 255,    1.0,    0   // Section #112
111, 112,   0, 255,   0, 255,    1.0,    0   // Section #113
112,  70,   0, 255,   0, 255,    1.0,    0   // Section #114
101,  41,   0, 255,   0, 255,    1.0,    1   // Section #115
0, 113,   0, 255,   0, 255,    1.0,    0   // Section #116
113, 114,   0, 255,   0, 255,    1.0,    0   // Section #117
114, 115,   0, 255,   0, 255,    0.9,    0   // Section #118
115, 116,   0, 255,   0, 255,    0.7,    0   // Section #119
116, 117,   0, 255,   0, 255,    0.7,    0   // Section #120
117,  44,   0, 255,   0,  25,    1.1,    1   // Section #121
89, 118,   0, 255,   0, 255,    0.8,    0   // Section #122
118, 117,   0, 255,   0, 255,    0.5,    0   // Section #123
119, 120,   0, 255,   0, 255,    1.0,    0   // Section #124
119,  17,   0, 255,   0, 255,    1.0,    0   // Section #125
120, 121,   0, 255,   0, 255,    1.0,    0   // Section #126
121, 122,   0, 255,   0, 255,    1.0,    0   // Section #127
122, 128,   0, 255,   0, 255,    1.0,    0   // Section #128
123, 124,   0, 255,   0, 255,    1.0,    0   // Section #129
124, 125,   0, 255,   0, 255,    1.0,    0   // Section #130
125, 126,   0, 255,   0, 255,    1.0,    0   // Section #131
126, 127,   0, 255,   0, 255,    1.0,    0   // Section #132
127,  15,   0, 255,   0, 255,    1.0,    0   // Section #133
128, 133,   0, 255,   0, 255,    1.0,    0   // Section #134
128, 123,   0, 255,   0, 255,    1.0,    0   // Section #135
129, 130,   0, 255,   0, 255,    1.3,    0   // Section #136
130, 131,   0, 255,   0, 255,    1.3,    0   // Section #137
131, 132,   0, 255,   0, 255,    1.5,    0   // Section #138
133, 134,   0, 255,   0, 255,    1.0,    0   // Section #139
133, 129,   0, 255,   0, 255,    1.0,    0   // Section #140
134, 135,   0, 255,   0, 255,    1.3,    0   // Section #141
135, 136,   0, 255,   0, 255,    1.3,    0   // Section #142
136, 137,   0, 255,   0, 255,    1.5,    0   // Section #143
137, 138,   0, 255,   0, 255,    1.5,    0   // Section #144
139,   5,   0, 255,   0,  25,    1.0,    0   // Section #145
140, 107,   0, 255,   0, 255,    1.0,    1   // Section #146
141, 102,   0, 255,   0, 255,    1.0,    1   // Section #147
142,  88,   0, 255,   0, 255,    1.0,    1   // Section #148
0                                                             // Number of cop start points
END OF OPPONENT PATHS
7										// number of material modifiers
// default material
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
ROAD1.MAT							// skid mark material
//	material '0'
1										// car wall friction
1										// tyre road friction
0.90										// down force
6.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
0										// sparkiness
3										// room for expansion
MUD2.MAT										// room for expansion
//	material '1'
1.2										// car wall friction
1.2										// tyre road friction
1.0										// down force
10.0										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
2.0										// sparkiness
4										// room for expansion
SAND2.MAT										// room for expansion
//	material '2'
1.2										// car wall friction
1										// tyre road friction
1.0										// down force
5										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
0.0										// sparkiness
3										// room for expansion
MUD1.MAT										// room for expansion
//	material '3'
1.2										// car wall friction
1.00										// tyre road friction
1.0										// down force
8.0										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
0.0										// sparkiness
3										// room for expansion
MUD2.MAT										// room for expansion
//	material '4'
1										// car wall friction
1										// tyre road friction
2										// down force
1										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
20										// sparkiness
1										// room for expansion
1										// room for expansion
//	material '5'
1										// car wall friction
1										// tyre road friction
2.0										// down force
4.0										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
1										// sparkiness
4										// room for expansion
SAND2.MAT										// room for expansion
// Non CarObjects
5										// number of non car objects
GASPUMP.TXT
GREENCAR.TXT
WRECK.TXT
PALM2.TXT
PHONE.TXT
3										// number of dust shade tables
61, 84, 33								// r g b values
0.25, 0.5, 0.75							// quarter, half and three quarter "strength"
92, 51, 34							// r g b values
0.25, 0.5, 0.75							// quarter, half and three quarter "strength"
117, 94, 38							// r g b values
0.25, 0.5, 0.75							// quarter, half and three quarter "strength"
12										// Number of network start points
-248.296,-15.630,43.190							//1
100													
-253.514,-15.627,23.641							//2						
101									
-260.518,-15.656,20.924							//3						
189									
-274.246,-15.627,23.641							//4						
146									
-269.537,-15.627,23.339							//5						
256									
-282.704,-15.627,30.227							//6						
187									
-278.421,-15.624,49.670							//7						
280									
-271.077,-18.908,81.830							//8						
9									
-255.535,-15.627,43.903							//9						
11									
-248.102,-18.907,75.910							//10						
11									
-275.029,-15.251,13.741							//11						
198									
-281.298,-15.627,37.148							//12						
9									
1										// number of splash files
SPLSHBLU.PIX 								//  name of pixelmapfile for splashes
1
NETCOSTA.TXT
